충남음악창작소

장비 구축(구매 및 설치) 과업지시서

2017. 5.

충남음악창작소 장비 구축(구매 및 설치) 과업지시서

1. 일반사항

❍ 장비의 설치 시 사용자와의 협의에 따라 시스템 도입목적에 합당하도록 불편함이 없도록 시설규모와 장비성능, 운영의 효율성 등을 고려하여 설치되어야 한다.

❍ 납품되어지는 모든 장비, 시설은 제반 법규와 시설기준에 적합하게 구축한다.

❍ 구축에 대한 모든 부대비용은 사업자가 부담하며, 설치중의 제반 안전사고 및 구축과정에서 발생되는 일체의 행정적․기술적 문제의 처리는 사업자의 책임으로 한다.

❍ 사업자는 장비를 설치할 때 진흥원이 이미 설치한 부대장비, 네트워크 등에 전혀 지장이 없도록 완벽한 호환과 정상적인 운영이 이루어지도록 하여야 하고 손상 시에는 사업자의 비용으로 즉각 원상복구 하여야 한다.

❍ 기존 장비의 접속 및 상호 연동을 위하여 기존 장비들의 환경을 변경할 필요가 있을 시에는 진흥원의 승인을 득한 후 사업자의 책임 하에 조치하여야 한다.

❍ 물품의 확인은 본 과업안내서의 구매사양에 따르며 규격 확인이 어렵거나 미흡한 경우 사업자는 관련 증빙서류 제출 및 기타 확인과정을 통하여 이를 입증하여야 한다.

❍ 사업자는 검수 요청 전 진흥원의 입회하에 각종 현장시험을 실시하여 시스템의 정상 작동 여부를 입증하고, 그 결과 문제가 없을 경우 검수 요청을 하여야 하며 시험가동 시 발견되는 Error나 불합리한 문제점, 시스템 보완요구 등에 대해서는 즉시 조치한 후 그 결과를 서면으로 제출하여야 한다.

❍ 설치 시스템의 내용이 과업안내서에 요구되는 성능, 사양을 수용할 수 없다고 판단되면 진흥원은 설치 변경을 요구할 수 있으며, 사업자는 이에 응하여야 한다.

❍ 최종 검사 결과 구축 장비의 운영이 불가하다고 판단되거나 기기의 하자 발생으로 계약조건을 이행하지 못하는 것으로 판단될 시에는 진흥원의 요구에 의해 사업자는 납품․설치한 모든 장비를 철거 및 회수해야 하며 그 비용은 사업자의 부담으로 한다.

2. 주요내용

❍ 납품․설치 시 파손이나 시험운영 중 하자가 발생하였을 경우 A/S를 불허하며 동일 규격 이상의 신규제품으로 교체해야 하고, 설치 중 제반 안전사고 및 납품 과정에서 발생하는 행정적, 기술적 제반 비용과 그에 따른 문제 처리는 제안사가 부담한다.

❍ 설치 중에 발생되는 모든 사고는 수급자가 책임을 져야 하며, 이를 방지하기 위하여 수급자는 고용인에게 필요한 모든 교육 또는 지시를 작업 전에 시달하여 주의를 주어야 한다.

❍ 납품하는 모든 물품은 원제작자의 표준 포장규격에 맞도록 포장․운반하여야 하며, 반드시 감독관의 입회하에 포장을 해체하여야 한다.

❍ 설치와 관련하여 각종 환경 설정과 정상 가동에 따른 업무 협의 및 보완 사항은 발주기관의 사전 승인을 득한 후 제안사의 주관․책임 하에 제조사, 관련 기관과 협력하여 문제점을 보완하고 정상 가동하도록 조치해야 한다.

❍ 제안사는 시스템설치 완료시 각 설비의 기능과 이에 따른 검사 및 시험에 합격하여야 한다.

❍ [장비규격서]의 내역에 위배하여 납품하였을 경우 그 책임은 수급자에 있으면 발주기관은 계약을 파기할 수 있다.

❍ 검수는 발주기관 측이 입회하여 항목별로 시행하며, 제안사는 납품 설치되는 물품에 대하여 납품 완료계를 제출하여야 하고 검수자는 납품완료계 접수일로부터 14일 이내에 검사를 한다.

❍ 검수과정 중 발견된 오동작 및 미비점에 대해서는 제안사가 즉시 수리 및 보완해야 하며, 발주기관의 감독관 입회하에 재시험 결과가 확인되어야 한다.

❍ 검사 완료 후에라도 본 구매설치에 있어 사업자의 책임으로 발생되는 모든 사고와 그로 인한 진흥원의 손해에 대해서는 사업자가 변상 조치하여야 한다.

❍ 장비 운영인력에 대한 교육이 실시되어야 한다.

❍ 운영인력 교육에 필요한 일정과 장비 및 시스템에 대한 매뉴얼(한글)이 제공되어야 한다.

❍ 효율적인 유지 보수 및 관리계획에 대한 내용이 제안되어야 한다.

❍ 본 사업의 효과적인 시행을 위해 장비의 입고 시기 및 설치 시작단계에서 완성단계까지의 세부 상황이 보고되어야 한다.

❍ 본 사업과 관련하여 제안업체의 조직과 투입인력은 장비 및 시스템의 안정적 운영 및 고도화를 위한 전담 기술조직을 배정하여 운영해야 한다.

3. 유지보수

❍ 납품하는 장비 및 시스템에 대하여 무상하자보수기간(하자담보책임기간)은 납품일로부터 2년 이내로 하고 이 기간 중 발생하는 모든 하자에 대해 계약자 비용으로 최단 기간(문제발생으로 인하여 운영에 지장을 미치지 않는 기간) 안에 조치가 완료되어야 하며 수시점검 및 정기점검을 실시하며 긴급 A/S체계를 구축한다. 단, 제조사 또는 공급사가 보증하는 무상하자보수기간이 2년 이상일 경우, 제조사 또는 공급사가 보증하는 무상하자보수기간을 하자담보책임기간으로 한다.

- 제안사는 하자보수를 위하여 24시간(공휴일, 일요일 포함) 장애신고 접수 및 장애 처리체계를 제안서에 제시하여야 한다.

❍ 납품되어지는 장비의 유지보수는 장비 개별 유지보수가 아닌, 시스템 설치업체에서 전체적인 통합 유지보수 함을 원칙으로 한다.

4. 기타 사항

❍ 과업안내서의 내용 중 해석의 차이가 있을 시는 진흥원의 해석을 우선으로 한다.

❍ 본 과업 안내서에 포함되지 않은 사항에 대하여는 진흥원에게 별도의 사양서는 제출하여야 한다.

❍ 본 과업안내서의 내용을 수정할 필요가 있는 경우 별도의 합의서를 작성할 수 있다. 다만 진흥원의 추가비용이 없어야 하며 규격을 상향으로 하여야 한다.

❍ 사업자는 면허, 특허권, 의장권, 공업 소유권 및 지적 소유권의 침해로 인한 모든 문제와 소송에 대하여 사업자의 부담으로 하여야 하며 진흥원은 전적으로 면책권을 갖는다.

❍ 본 과업안내서 및 도입조건에 명시된 사항은 최소한의 사항, 내역만을 규정하였으므로 상세히 기술되지 않았거나 누락된 사항에 대하여 사업자는 시스템구축 운영상 하자가 발생되지 않도록 사전 조치하여야 하며, 본 과업안내서에 명시되지 않은 사항은 관계법령과 진흥원의 해석에 따른다.

❍ 본 과업안내서에서 정하는 것을 제외하고는 지방자치단체를 당사자로 하는 계약에 관한 법령, 조달관련규정에 의하여 당사자 협의하여 결정하며, 본 과업안내서에 관한 소송 관할 법원은 진흥원의 주소지를 관할하는 법원으로 한다.

5. 제출 서류

❍ 수급자는 계약 후 7일 이내에 진흥원 소정 양식의 착수계 서류 일체를 제출하여야 한다.

❍ 수급자는 검수 시 진흥원 소정 양식의 완료계 서류 일체를 제출하여야 한다.

장비 목록 및 규격서

1. 장비 목록

No.	Description	Q'ty	Unit	Remark
	개인연습실
1	Keyboard 1	1	ea
2	Keyboard 2	1	ea
3	Mixer	2	ea
4	Monitor Speaker	4	ea
	녹음실
	A. 조종실
1	Workstation	1	ea
	- 34“LED Monitor	1	ea	Thunderbolt
2	PCIe 2.0 Expansion System	1	set
	- Thunderbolt Cable	2	ea
	- Mobile Rack Device Mounting Kit	1	ea
	- SSD	4	ea
3	DAW System	1	set
	- DAW Software	1	copy
	- DSP	1	ea
	- IO	1	ea
4	Pre AMP. 1	1	ea
5	Pre AMP. 2	1	ea
6	Main Console	1	set
7	Mic Pre 1	1	ea
	Mic Pre 2	1	ea
	Mic Pre 3	2	ea
8	Compressor 1	1	ea
	Compressor 2	1	ea
9	Master Clock Generator	1	ea
10	Effecor	1	ea
11	Plug-In 1	1	ea
	Plug-In 2	1	ea
	Plug-In 3	1	copy
12	Monitor Controller	1	ea
13	Cue System 1	6	ea
	Cue System 2	2	ea
14	Headphone	8	ea
15	Pacth bay system	1	lot	케이블, 설계, 제작 설치 포함
16	Console Desk, Rack, Sub Desk	1	lot	Main Desk, Sub Desk
17	Speaker	2	ea
	- Stand or bracket	2	ea
18	Sub Woofer	1	ea
19	Sub Speaker	2	ea
	- Power Amp.	1	ea
20	자재 및 설치비	1	lot	Main booth Combination panel, 각 종 케이블, 월판넬
21	HDMI 1:2 분배기	1	ea
22	VIdeo I/O	1	ea
23	LED TV	2	ea	녹음실, 녹음부속실 모니터
	B. 녹음실, 녹음부속실
1	Mic POP Filter	2	ea
2	Drum Mic.	1	ea
3	Dynamic Mic. 1	1	ea
4	Dynamic Mic. 2	6	ea
5	Condenser Mic. 1	1	ea
6	Condenser Mic. 2	1	set	Matched Pair
7	Condenser Mic. 3	1	set	Matched Pair
8	Condenser Mic. 4	1	set	Stereo Set
9	Cardioid Mic.	1	ea
10	Dynamic Mic. 1	1	set	Matched Pair
11	Dynamic Mic. 2	4	ea
	Dynamic Mic. 3	4	ea
12	MIC Stand 'T'	10	ea
13	Drum	1	set
14	Cymbals	1	set
15	Guitar Amp. 1	1	ea
16	Guitar Amp. 2	1	ea
17	Bass Amp.	1	ea
18	Keyboard 1	1	ea
	Keyboard 2	1	ea
	편집 조정실
1	Workstation	1	set
2	MacBook Pro	1	set
3	34“LED Monitor	1	ea	Thunderbolt
4	Software	1	ea
5	Mixer	1	ea
6	Audio Interface	1	ea
7	Mointor Speaker	2	ea
8	Speaker Stand	2	ea
9	Master Keyboard	1	ea
10	Custom Desk	1	set
11	P.D.U	1	ea
12	Plugin	1	ea
13	가상악기(Vsti)	1	ea
14	Cue System 1	4	ea
	Cue System 2	2	ea
15	자재 및 설치비	1	lot	booth Combination panel, 각 종 케이블
	밴드 연습실
1	Drums	1	ea
2	Cymbals	1	set
3	Bass Amp.	1	ea
4	Guitar Amp. 1	1	ea
5	Guitar Amp. 2	1	ea
6	Keyboard 1	1	ea
7	Keyboard 2	1	ea
8	Mic. 1	4	ea
	Mic. 2	2	ea
9	MIC Stand 'T'	4	ea
10	Monitor Speaker	2	ea
11	Speaker Stand	2	ea
12	Mixer	1	ea
	융복합형 공연장
	A. Audio Part
1	Subwoofer Speaker	2	ea
2	Line Array Speaker (100°x 15°)	8	ea
3	Line Array Speaker Bumper	2	set
4	Line Array Speaker Pick up Bar	2	set
5	Stage Monitor Speaker	10	ea
6	C/R Moniter Speaker	2	ea
7	C/R Monitor Headphone	2	ea
8	Digital Audio Mixing Console	1	ea
9	Additional I/O BOox(Console)	1	ea
10	Digtal Audio Network Bridge	1	ea
	- Additional I/O Card	1	ea
11	Dual CD Player	1	ea
12	Wireless Mic Receiver	8	ea
13	W/L Hand Mic.	8	ea
14	W/L Belt Transmitter	4	ea
15	Pin Microphone	4	ea
16	W/L Headset	2	ea
17	Guitar Mic.	1	ea
18	악기용 Mic.	2	ea
19	W/L Antenna Splitter	2	ea
20	W/L Antenna	2	ea
21	Drum Mic. SET	1	set
22	Condenser Mic. 1	2	ea
23	Condenser Mic. 2	2	ea
24	Vocal Mic.	1	ea
25	Condenser Mic.	2	ea
26	Dynamic Mic. 1	4	ea
27	Dynamic Mic. 2	6	ea
28	Drums	1	ea
29	Cymbals	1	set
30	MIC Stand 'T' 1	6	ea
31	MIC Stand 'T' 2	12	ea
	B. Installstion & Materials
1	Switching HUB(PRI & SEC)	2	ea
2	Power Distibutor	2	ea
3	Multi Floor Box	4	ea
4	Multi Jack Panel	3	ea
5	DI Box - MONO	4	ea
6	DI Box - STEREO	4	ea
7	Condsole Desk	1	ea
8	Cable Duct	50	m
9	난연 CD관	100	m
10	난연 CD관	100	m
11	난연 CD관	100	m
12	Mic. Cable	5	ea
13	Mic. Multi Cable	100	m
14	Mic. Multi Cable	100	m
15	Video cable	200	m
16	Control Cable	1	ea
17	Power Cable	300	m
18	배관 부속재	1	lot
19	소모 잡자재	1	lot
20	설치 인건비	1	lot
21	설치 인건비	1	lot
	C. Video Part
1	PTZ Camera	3	set
2	Camera Controller	1	ea
3	Video Mixer	1	ea
4	자막기	1	ea
5	LED Monitor	2	ea
6	HD레코더	1	ea
7	메모리카드	2	ea
8	스트리밍 옵션	1	ea
9	Control Pannel	1	ea
10	Rackmount	1	ea
11	프로젝터	1	ea
12	DeskTop PC	1	ea
13	Monitor	2	ea
14	자재 및 설치비	1	lot
	D. Stage Lighting System
1	Suspension Batten	4	set
2	Ceiling Light Batten	1	set
3	Cable Reel	1	set
4	Fly Duct	5	ea
5	Power Cable	5	ea
6	Cable Basket	5	ea
7	Terminal Box	12	ea
8	Three Basic LED Multi Zoom Light	4	ea
9	Three Basic LED Multi Zoom Light	4	ea
10	Three Basic LED Multi Par Light	10	ea
11	Three Basic LED Multi Spot Light	2	ea
12	Three Basic LED Multi Spot Light	2	ea
13	Three Basic LED Elip Light	4	ea
14	Moving Spot Light	4	ea
15	Moving Wash Light	4	ea
16	DMX Splitter	1	ea
17	Safety Chain	34	ea
18	Light Hanger	34	ea
19	Plancard Batten	1	set
20	Roll Screen	1	set
21	Cover Curtain	1	set
22	Main & RD Unit Rack	1	set
23	Computer Console	1	set
24	MCC Control Console	1	ea
25	Local Control Board	1	ea
26	Grid Iron	1	lot
27	배관 및 배선	1	lot
28	경비및 잡자재비	1	lot
29	설치인건비	1	lot
30	무전기	6	ea

2. 장비 규격

※ 각 장비는 동등 규격 이상의 제품으로 제안, 납품해야 함

개인연습실 1, 2

❍ KEYBOARD 1

가. 기능

76-key nod to the classic Jupiter series, with a feature set and sound tailored for today's	performing keyboard player

나. 규격

• Keyboard	76 Keys (with velocity and channel aftertouch)

• Polyphony	256 Voices (varies according to the sound generator load)

• Multitimbral	4 parts (Upper, Lower, Solo, Percussion)

• Synthesis Method	Roland SuperNATURAL

• Presets	Registrations: 256 (including pre-loaded registrations)

Live Sets: 2,560 (including pre-loaded Live Sets)

• Effects	-Multi-Effects (MFX): 4 units (parallel connection only), 76 types per each                Upper/Lower (total: 8 units)

-Reverb: 1 unit, 5 types per each Upper/Lower (total: 2 units)

Solo part/Percussion part

-Compressor+Equalizer+Delay: 1 set per each Solo/Percussion (total: 2 sets)

-Reverb: 1 unit, 5 types

Master Effects

4-Band Equalizer: 1 unit

• Sequencer	Tracks: 1 Stereo Track

Playable File Format: Audio File: WAV, AIFF, MP3

Recording File Format: Audio File: WAV (44.1 kHz, 16-bit Linear, stereo)

Effects: 4-Band Equalizer: 1 unit

• Controllers	D Beam Controller

Pitch Bend/Modulation Lever

Assignable buttons (S1, S2)

Assignable knobs (E1--E4)

PART LEVEL sliders (PERC, LOWER, UPPER, SOLO)

• Internal Storage	USB Flash Memory (sold separately)

Use USB flash drive sold by Roland. Roland cannot guarantee operation if	other products are used.

❍ KEYBOARD 2

가. 기능

an 88-key performance controller that features a fully weighted hammer action, velocity and	aftertouch sensitive keyboard, loaded with a sound set that is both broad and deep. The	KORE 64 and the Artis German 9' Grand Piano expansion packs are built-in and together with	the KB3 ToneReal Organs and a variety of synthesis engines, they deliver over 1,300 factory	programs.

나. 규격

• Keyboard	88-key,fully weighted, hammer action, with velocity and aftertouch sensitivity	and a quick release spring

• Polyphony	128 voices, dynamically allocated

• Multitimbral	16 parts (one per MIDI channel)

• Presets	1,453

• User Memory	16,000 locations for user objects

• Expansion Slots	Includes KORE 64 and the German D Grand EXP Piano (built-in)

• Effects	16 insert effects distributed over 11 buses, 2 auxiliary sends and 2 master	effects (saved with each song and setup)

• Sequencer	Unlimited tracks (on import)

960 PPQ resolution

Song editing functions include both event and track-based tools like quantize,	swing, remap, controller scaling and more

Controller chasing and a global "set song length" functions

• Controllers	1 x Pitch wheel

1 x Modulation wheel

9 x Sliders/drawbar controllers

10 x Front panel switches (momentary or toggle, software selectable)

3 x Switch pedal inputs

2 x Continuous control pedal inputs

1 x Super Ribbon input

1 x Breath controller input

Mono pressure

• MIDI	216 factory programmed MIDI setups including up to 16 independent zones,	effects, independent controller assignments, triggerable pattern-based "Riffs"	and arpeggiator settings

Standard General MIDI

MIDI over USB

• Connections	4 x 1/4" TRS phone Out (24-bit DACs)

1 x 1/4" TRS Headphone

3 x 5-pin DIN MIDI In, Out, Thru

1 x RCA coaxial S/PDIF Out (24-bit stereo, 44.1, 48, 88.2, 96, 176.4, 192 kHz	modes and externally clockable)

• External Storage	Supports USB thumb-drives for loading/saving user data as well as	performing OS updates

USB computer port - load/save data directly to and from a Mac/PC as well	as perform OS updates

• Display	240 x 64 angled, back-lit CCFL with dedicated back panel brightness and	contrast controls

• Power Requirements	120~240 VAC, 50/60 Hz for internal AC power supply

❍ MIXER

가. 기능

a compact six-input mixer with built-in effects for small performances, lectures, recordings and similar applications. The mixer features two mic/line combo inputs with D-PRE mic preamps as well as four 1/4" line inputs with stereo level controls.

나. 규격

• Built-in Effects	SPX algorithm: 6 programs (3 reverb, 3 delay)

• Phantom Power	+48 V switchable, channels 1, 2

• Input Channels	2x mono [mic/line]

2x stereo [line]

• Output Channels	2x stereo out

1x headphone

• Bus	1x stereo

• Pad	26 dB (mono channels)

• HPF	80 Hz, 12 dB/oct (mono channels)

• Equalizer	EQ high (mono channels) gain: +15 dB/-15 dB, Frequency: 10 kHz shelving

EQ low (mono channels) gain: +15 dB/-15 dB, Frequency: 100 Hz shelving

• LED	Peak LED turns on when post EQ signal reaches 3 dB below clipping

• Level Metering	2 x 7-segment LED meter [PEAK, +6, +3, 0, -3, -10, -20 dB]

• Total Harmonic Distortion	0.01% @ +8 dBu (20 Hz to 20 kHz), GAIN knob: min, 0.003% @ +18	dBu (1 kHz), GAIN knob: min

❍ MONITOR SPEAKER

가. 기능

a high-quality nearfield studio monitor designed for use in smaller studio spaces. The bass-reflex cabinet houses a 5" woofer and a 1" dome tweeter to provide accurate sound with a frequency response of 50Hz to 40kHz. The cabinet is magnetically shielded for safe use near video monitors.

나. 규격

• Low Frequency Driver	5" (127mm) Cone Woofer

• High Frequency Driver	1" (25mm) Titanium Dome Tweeter

• LF Amplifier	40W

• HF Amplifier	27W

• Crossover	2.5kHz

LF: 24dB/Oct

HF: 24dB/Oct

• Frequency Range	50Hz - 40kHz (-10dB)

• Maximum Sound Pressure Level (SPL)	101dB

• Connectors	1 x XLR Input, Balanced

1 x 1/4" Phone Input, Unbalanced

1 x Power Input

• Input Impedance	10 kOhms

A. 조종실

❍ Workstation

가. 기능

DAW를 위한 고성능 워크스테이션

나. 규격

• Processor 3.0GHz 8코어 Intel Xeon E5 프로세서

• Memory	32GB of 1866 MHz DDR3 ECC RAM

• Graphics	2 x AMD FirePro D700 with 6GB of GDDR5 discrete memory

• Storage (SSD)	1TB PCIe-based flash storage

• Ports	6 x Thunderbolt 2

• 4 x USB 3.0

• 1 x HDMI 1.4 , 6 x mini DisplayPort (via Thunderbolt 2 ports)

Connect up to three 4K displays or six Thunderbolt displays

• 1 x Combined optical digital audio output/analog line out minijack

• 1 x Headphone minijack with headset output

• 1 x HDMI port supports multichannel audio output

• 1 x Built-in speaker

• Ethernet	2 x 10/100/1000 Mbps Gigabit Ethernet RJ-45

• Wi-Fi	802.11ac (802.11a/b/g/n compatible)

• Bluetooth 4.0

• Operating System	MacOS X

• Magic Mouse 2, 숫자 키패드를 부착한 Apple 키보드

❍ 34“LED Monitor

가. 기능

DAW 편집 창 및 DAW시스템 전반 모니터링

나. 규격

• 화면크기	34“/86.7cm

• 해상도	3,440 × 1,440

• 패널	LED/IPS

• 화면비율 21:9 Wide (곡면 울트라 와이드)

• 명암비 1000:1(DFC 무한 :1)

• 공장색교정, sRGB 100%, 10bits (8bit + FRC)

• DDC/CI, HDCP

•S/W : On Screen Controller, 화면분할프로그램, 듀얼PC컨트롤러

❍ PCIe 2.0 Expansion System

가. 기능

4U rackmount enclosure for the Mac Pro

나. 규격

• Rackmount Enclosure	4 U

• PCIe Expansion Slots	1 x8 mechanical (x8 electrical) PCIe 2.0

1 x16 mechanical (x8 electrical) PCIe 2.0

1 x8 mechanical (x4 electrical) PCIe 2.0

• PCIe Cards Supported	3 x Full-length PCIe cards, or

1 x Full-length, double-width PCIe card, plus 1 x single-width card

• External Connectors	2 x Thunderbolt (1 x open, 1 x used)

2 x RJ-45 Gigabit Ethernet port extensions

3 x USB 3.0 port extensions (1 x front mount and 2 x rear mount)

1 x HDMI port extension

• Internal Connectors	1 x 6-pin Mini-Fit Jr (same type as on legacy Mac Pro motherboard;	provides up to 75 W of power for PCIe cards that require supplemental power)

1 x C-8 power

• Compatibility	Mac Pro (late 2013)

• PCIe Card Compatibility	PCIe Card Thunderbolt Compatibility Chart

For maximum PCIe bandwidth, dedicate one Thunderbolt 2 bus to the PCIe expansion slots

• Power Supply	Universal 300 W, 115 to 230 VAC, 50 to 60 Hz

• Operating Temperature	32 to 95°F (0 to 35°C)

• RoHS Compliant	Yes

• 2 x TCB-TB-1M Thunderbolt Cable

• MR-STO-X8SSD Mobile Rack Device Mounting Kit

• 4 x 512GB SSD

❍ DAW System

가. 기능

Fully featured audio creation DAW System

나. 규격

1) Compose and Record

Record audio with up to 32-bit/192 kHz and experience exceptionally low latency when paired

with an Avid audio interface

Redesigned Avid Audio Engine and 64-bit performance delivers multiple times the processing

power of previous versions of Pro Tools on the same hardware configurations

Loop recording/track comping workflows

Use QuickPunch to quickly replace any questionable section with a better performance

Easily create parts for practically any musical instrument using virtual instruments, a MIDI

keyboard/controller or mouse, and the built-in MIDI editor

Includes virtual instruments and audio loops

2) Edit

Elastic Time and Elastic Pitch processing

Fine-tune music and audio with sample-accurate editing tools available in a single window

Speed up editing and mixing using the Clip Gain Smart Tool

Monitor the picture playback using optional video interfaces from Avid, AJA, and Blackmagic

Design

3) Mix

Polish mixes with over sixty included effects, sound-processing and utility plug-ins

Includes reverbs, EQs, and compressors, guitar amp emulators, surround sound fold-down,

channel strip dynamics, and more

Achieve phase-accurate mixes with Automatic Delay Compensation with four times the samples

(16,383) to handle the largest mixes, no matter how many plug-ins used

Bounce mixes to an iTunes library to share with others on a network

4) 구성

• Pro Tools | HD Software

• HDX Card

• HD I/O 16x16 Analog I/O

• iLok

• DigiLink Cable

❍ Pre AMp. 1 : Avid Pro Tools | HD PRE

❍ Pre AMp. 2 :  Avid Pro Tools | SYNC HD

❍ Main Console

가. 기능

• Traditional SSL preamps offer 75dB of gain and classic sound

• Phantom power, phase reverse, and -20dB pad onboard

• 3-way, mode-dependent insert points available per channel

• 4-band EQ with switchable E/G Series characteristics

• Two channel dynamics and a Master Bus compressor built in

나. 규격

• Type	Analog

• Channels	16

• Headphones	2 x 1/4"

• Phantom Power	16

• EQ Bands	4-band (E-Series, G-Series Switch)

• Aux Sends	4 x FX

• Busses/Groups	2 x Bus (Main Stereo)

• Faders	17 x 100mm

• Effects	Yes

• Talkback	Yes

• Computer Connectivity	6 x MIDI, 1 x Ethernet, 2 x Serial (9-pin)

❍ Mic Pre 1

가. 기능

a single-channel microphone preamp that utilizes vintage-style germanium transistors, which help it achieve a variety of sounds. Gain and Feedback knobs are provided for setting levels and achieving various tones, as is a Thick button and a -20dB pad button.

나. 규격

• Number of Channels	Single

• Inputs	1x XLR, transformer balanced, pin 2 hot

1x 1/4" (6.35 mm) instrument jack, unbalanced, 100k input impedance

• Output	1x XLR, transformer balanced, pin 2 hot

• Phantom Power	48V

• Gain Range	-5 to +65 dB

• Circuit	Discrete, transistor

• Cable Length	Included 4-pin cable: 6' (1.83 m)

• Power	+/- 28V

❍ Mic Pre 2

가. 기능

The API 3124MV adds transformer tap selection to the company's popular 3124MB+ 4-channel mic/instrument preamp. The 3124MV packs legendary API console sonics and performance into an easy-to-use, premium-quality rackmount unit — complete with a built-in stereo mixer.

나. 규격

• Preamp Type	Solid State

• Number of Channels	4

• Phantom Power	Yes

• Analog Inputs	4 x 1/4" (Hi-Z), 4 x XLR (mic), 1 x 1/4" (aux return)

• Analog Outputs	4 x XLR, 1 x 1/4" (aux send), 2 x 1/4" (stereo out)

• Channel Inserts	Yes

• Rack Spaces	1U

• Power Source	Standard IEC AC cable

❍ Mic Pre 3

가. 기능

an 8-channel microphone preamp that is based on the philosophy that "coloring" at source is not a good idea, and that maintaining the clarity and integrity of a signal through the recording and production process, is critical to communicating the artist's intention and individuality.

나. 규격

• Number of Channels	8

• Inputs	8 x XLR

• Output	8 x XLR

• Phantom Power	+48V, individually switchable

• Multi Function	No

• Gain Range	65dB

• Maximum Output Level	+32dBu

• Frequency Response	3Hz to 300kHz, +0/-3.0dB

• Noise	EIN: -133dB

• Power Requirements	100~120, 200~240 VAC, 50/60Hz (selectable)

❍ Compressor 1

가. 기능

a single-channel, vacuum tube Class-A processor that combines a tube microphone preamp,

instrument DI, opto-compressor, and a 4-band parametric EQ.

나. 규격

• Number of Channels	Single

• Inputs	1 x XLR Microphone (rear)

1 x XLR Balanced Line (rear)

1 x 1/4" TS Phone Instrument (front)

• Outputs	1 x XLR

• Frequency Response	10Hz to 200kHz, -3dB line in to line out

• Noise	EIN: -116dB, 22Hz to 22kHz unweighted

• Gain Range	Mic Pre: 0db to 58db

Instrument: 0dB to 30 dB

Line: -27dB to 28 dB

• Maximum Output	+30dB

• Phantom Power	+48V

Compressor

• Threshold Range	-30dB to +20dB

• Ratio	1:1 to 20:1

• Attack Time	2mSec to 200mSec

• Release Time	100mSec to 5Sec

• Sidechain	Internal with EQ

Equalizer

• Filter Type	Discrete Class A, variable active and switched passive design

• Frequency Bands	Treble: Switched, 10kHz, 15kHz, 20kHz, 32kHz

High-Mid: Variable 200Hz to 2.8kHz or 2kHz to 28kHz (10x switch)

Low-Mid: Variable 30Hz to 450Hz or 300Hz to 4k5Hz (10x switch)

Bass: Switched, 15Hz, 30Hz, 60Hz, 150Hz

❍ Compressor 2

가. 기능

single channel optical compressor with a push-pull tube amplifier. The unit contains a unique

low distortion gain-reduction element, and the input and output are balanced and are fully

floating.

나. 규격

• Function	Compressor

• Number of Channels	1

• Inputs	1 x XLR

• Output	1 x XLR

• Maximum Input Level	+21dBmdBu

• Compression Threshold	-40dBu to +20dBu

• Compression Ratio	Variable

• Maximum Output Level	+24dBm

• Make-up Gain	0dB to +30dB

• Frequency Response	5Hz to 25kHz

❍ Master clock Generator

가. 기능

• Vast choice of clocking options

• All that you love about Antelope's cult Trinity Master Clock now in just 1U

• Access all OCX HD features via Antelope Audio's flexible software control panel

나. 규격

• (2) x wordclock input - BNC

• (1) x composite video input - BNC

• (1) x atomic clock input - BNC

• (2) x SPDIF input - RCA

• (1) x AES / EBU input - XLR

• (10) x wordclock output - BNC

• (4) x AES / EBU output - XLR

• (2) x SPDIF output - RCA

• (1) x USB - 4 pin USB type A

❍ Effector

가. 기능

• World-class reverb performance for your studio

• Take complete control of your reverb

나. 규격

• Processor Type	Reverb

• Number of Channels	2

• Presets - Factory	100 Factory

• Presets - User	100 User

• Analog Inputs	2 x XLR

• Analog Outputs	2 x XLR

• Digital Inputs	AES/EBU

• Digital Outputs	AES/EBU

• MIDI I/O	In/Out

• Rack Spaces	1U

❍ Plug-In 1

• Flagship DSP-accelerator PCIe card for UAD Powered Plug-ins

• Loaded with 8x Analog Devices SHARC 21469 floating-point coprocessors

• Run complex mix processing without taxing your CPU in Pro Tools, Logic, Cubase, Nuendo, Digital Performer, and more

• AAX, VST, AU, RTAS support

• Mac compatibility: OS X 10.10 Yosemite and higher

• Windows compatibility: 64-bit editions of Windows 7, 8.1, or 10

• Linkable to existing UAD groups/systems — use up to 4 UAD-2s in one system

❍ Plug-In 2

• Over 150 stellar audio plugins

• One massive collection

• Upgrades available from all bundle

• AAX Native, RTAS, AudioSuite, TDM

• Audio Units, VST

• SoundGrid

• Mac OS X, Windows

❍ Plug-In 3

• Auto-Tune 8 Pitch Correction Plug-In

• Flex-Tune Natural Pitch Correction

• Ultra-Low Latency Mode

• Real-Time Pitch Correction

• For Native Based Applications

• Audio Units, RTAS, AAX, VST

• Mac and PC Compatible

• Requires iLok

❍ Monitor Controller

가. 기능

one-point analog, stereo and 5.1 volume control, and a switching matrix source and speaker management controller

나. 규격

• Inputs and Outputs	Inputs: Impedance, balanced: Sub-D: 50 kOhms;

Provides six surround and two stereo input channels

Unbalanced: 6 x RCA: 10 kOhms, for 5.1 Surround

Outputs: Impedance, balanced: 6 x 1/4" TRS: <600 Ohms

• THD & Noise	Input Level -10 dB: 0.04% Input Level 0 dB: 0.01%

Input Level +10 dB: 0.006%

• Noise	A-Weighted: - 98 dB

Maximum Input Level: + 22 dB

Dynamic Response: 120 dB

• Common Mode Rejection	@100 Hz: ›70 dBu

@1 kHz: ›70 dBu

• Frequency Response	10 Hz to 100 kHz (-3 dB)

• Phase	-36° (10 to 120 kHz, -3 dB center frequency)

Phase, linear 20 Hz to 100 kHz

❍ Cue System 1, 2

가. 기능

The system puts personal monitor mixing in the hands of musicians, singers, speakers and other talent, allowing them to set levels for up to 16 channels of audio, ultimately creating custom monitor mixes that favor their own signals.

나. 규격

• 16-channel digital stereo mixer to create your personal monitor mix

• Ultra-intuitive "analog" operation with total recall and 16 presets for custom mixes

• State-of-the-art 24-bit D/A converters for premium audio quality

• 16 Channel Select buttons with dual LEDs for perfect overview

• Level and Pan/Spread control per channel with LED meter

• 3-band EQ per channel with mid-band frequency control

• Solo and mute functions per channel

• Global Level and EQ controls plus Panic Mute function

• MIDI IN port for real-time remote control of all channels by external MIDI device such as BEHRINGER BCF2000, BCR2000, etc.

• with HA8000

❍ Headphone

가. 기능

• Circumaural closed-back stereo headphone ideal for use in professional applications

• 40mm diameter drive units deliver deeper bass, lower distortion and wider dynamic range

• OFC cable and gold plated Unimatch plug provides both 1/8" mini-jack and 1/4"TRS phono

connectivity

나. 규격

• Type	Circumaural, closed-back

• Frequency Range	10 Hz - 20 kHz

• Impedance	63 Ohms

• Sensitivity	104dB SPL/mW

• Maximum Input Power	1000 mW

• Connectors	1/8" stereo mini-jack, with 1/8" to 1/4" TRS phono adapter

• Cable Length	3 m

Focus Control Simple focus / Manual, Button control (Manual, Simple focus, Day & Night)

Lens Type Manual / DC auto iris / P-iris

Mount Type C / CS

❍ Pacth bay system

가. 기능

• 믹서, 패널, 프리앰프, 컴프레서 등 녹음장비의 입출력을 손쉽게 재구성할 수 있는 패치베이

나. 규격

• Patchbay 2x48 Jack Bantam

• 96 Hole

• MOGAMI 24"

❍ Console Desk, Rack

가. 기능

• 장비의 원활한 열 배출을 위한 벤틸레이션 설계

• 88Key 이상의 마스터 키보드 지원

• A;; Parts 최고급 Electric Powder Coating 마감

• 상 하단 각 16RU 랙 마운드 가능

• 각종 케이블 설치를 위한 9개의 홀 가공

• 편안한 고급 가죽 암레스트 패드

• 후면 디스플레이 암 장착가능

• 일체형 니어필드 스피커 스탠드

나. 규격

• Electric Powder Coating

• Durable Construction

• Ventilation

• Cable Accessibility

• Detail

• Display Arm

❍ Speaker

가. 기능

10" 2-Way Bi-Amplified Active Monitor (Single) Black Veneer is designed for high-power near-field monitoring such as in music studios, mobile vans, surround sound systems, multimedia installations, and TV broadcast facilities. The speaker consists of a 10" bass woofer, a 1" metal dome tweeter, a custom crossover network,

나. 규격

• Low Cut Filters	Lower cut-off frequency: -3 db ≤40 Hz

• High Cut Filter	Upper cut-off frequency: -3 dB: ≥22,000 Hz

• Frequency Response	42 to 21,000 Hz (±2.5 dB)

• Self Noise	Self-generated noise level in free field at 1 meter on axis: <10 dB	(A-weighted)

• Distortion	At 90 dB at 1 m on axis:	50 to 100 Hz: <1% >100 Hz: <0.5%

• Driver(s)	Bass: 10" (250 mm) cone

Treble: 1" (25 mm) metal dome

Both drivers are magnetically shielded

• Input Connector	XLR Female: pin 1 gnd, pin 2 +, pin 3 -

• Input Impedance	10 kΩ balanced

• Input Level	For 100 dB SPL output at 1 m: variable from +6 to -6 dBu

For maximum short-term sine wave output 113 db SPL at 1 m:	variable from +19 to +7 dBU

• Filter	Subsonic filter below 40 Hz: 18 dB/octave

Ultrasonic filter above 25,000 Hz: 12 dB/octave

• Crossover Frequency	Bass/Treble: 1,800 Hz

Slopes: 24 to 32 dB/octave

Amplifier

• Output Power	Bass amplifier short-term output power with a 4 Ω load: 180 W

Treble amplifier short-term output power with an 8 Ω load: 120 W

Long-term output power is limited by driver unit protection circuitry.

• Slew Rate	80 V/μs

• Distortion	THD: ≤0.05%

SMPTE-IM: ≤0.05%

CCIF-IM: ≤0.05%

DIM 100: ≤0.05%

• Signal to Noise Ratio	Referred to full output:

Bass: >100 dB

Treble: >100 dB

• with speak Stand or bracket

❍ Sub Wooper

가. 기능

• Smart Active Monitor (SAM™) Systems

• Bass Management System

• Active Crossovers

• Protection Circuitry

나. 규격

• Powered	Yes

• Speaker Size	10"

• Driver Type	Cone, magnetically shielded driver

• Total Power	300W Class D

• Frequency Range	19Hz-150Hz (-6 dB LFE), 19Hz-100Hz (-6 dB)

• Maximum Peak SPL	109 dB SPL @ 1m

• Input Types	7 x XLR, 1 x XLR (LFE), 1 x XLR (Link in), 1 x XLR (AES/EBU), 1

x 1/4" (bypass switch connector)

• Output Types	7 x XLR, 1 x XLR (LFE), 1 x XLR (Link in), 1 x XLR (AES/EBU), 2

x RJ45 (CAT5 GLM network)

❍ Speaker Stand

가. 기능

모니터 스피커를 받침

나. 기능

• Base: 21"x17"x2" (LxWxH)

• Stand Height: 56"

• Tweeter Height Adjustment: 13" to 54.5"

• Maximum clearance Under Speaker (vertical): 44.25"

• Maximum Clearance Under Speaker (horizontal): 49"

• Speaker Mount Tilt: 5 degrees up or down

❍ Sub Speaker

가. 기능

• 4.5" full-range driver

• 25W RMS/50W peak

• 8 ohms

나. 규격

• Frequency Response	75 Hz - 15 kHz

• Impedance	8 ohms

• Driver	4.5" full range

• SPL	90 dB @	1 W / 1 m

• Cabinet	Sealed 5/8" MDF

• Wattage	25 W RMS / 50 W peak

• with  Crown D75a Power AMP.

❍ Main Booth Combination panel

가. 기능

메인부스에 설치하여 오디오, 네트워크, 영상, 전원등을 접속하기 위한 패널

나. 규격

• 16CH MIC/LINE I/O + LK16CH

• ETHERNET 4CH

• COAXIAL 2CH

• POWER 16A 2CH

❍ Video I/O

가. 기능

• HD SDI, HDMI, Thunderbolt and 2 breakout cables

• Real-time, hardware-based up / down / cross conversion

• Connect to a quality HDMI monitor for precise color correction

• Captures in edit-friendly open standard DPX and QuickTime formats

나. 규격

• Outputs Video	SDI x1 10-bit SD/HD switchable, HDMI type A x1

• Sync Input	Blackburst in SD, 720p50, 720p59.94, 1080i50 and 1080i59.94 formats or Tri-Sync in any HD format

• Device Control	Sony compatible RS-422 deck control port

Serial ports TxRx direction-reversible under software control

• Computer Interface	Thunderbolt x1

• HDMI Resolution	Pixel for pixel HD resolution input to connected device

• with HDMI 1:2 Splitter

❍ LED TV

가. 기능

DWA에서 출력되는 영상을 모니터

나. 규격

• 화면크기	138 cm

• 해상도	1,920 × 1,080

• 패널	블랙 패널 +

• 사운드출력(RMS)	10W+10W

• 돌비 사운드, DTS Premium Sound / DTS Premium Sound 5.1

• 에너지효율 1 등급

• With TV Stand

B. 녹음실, 녹음부속실

❍ Mic POP Filter

가. 기능

보컬 녹음시 팝핑 현상 감소

나. 규격

• 필터 지름	35Cm

• 구즈넥 길이	30Cm

• 재질	나일론 필터 / 메탈 구즈넥 / 메탈 클램

❍ Drum Mic.

가. 기능

• Cardioid-pattern microphone

• Built-in swivel mount

• Built-in windscreen

나. 규격

• Transducer	Pressure Gradient Dynamic

• Polar Pattern	Cardioid

• Frequency Response	20 Hz to 17 kHz

• Power Requirements	None Dynamic, Requires No Phantom or Battery Power

• Output Impedance	210 ohms

• Output Connectors	XLR-3M Type

❍ Dynamic Mic. 1

가. 기능

a super-cardioid studio dynamic microphone

나. 규격

• Transducer	(Pressure Gradient) Dynamic

• Polar Pattern	Super-cardioid

• Frequency Response	40 Hz - 20 kHz

• Power Requirements	None Dynamic, Requires No Phantom or Battery Power

• Output Impedance	200 Ohms

• Output Connectors	XLR-3M Type

❍ Dynamic Mic. 2

가. 기능

a cardioid, dynamic microphone popularized by the recording and broadcast industry

나. 규격

• Transducer	(Pressure Gradient) Dynamic

• Polar Pattern	Cardioid

• Frequency Response	30 Hz - 17 kHz

• Power Requirements	None Dynamic, Requires No Phantom or Battery Power

• Output Impedance	200 Ohms

• Output Connectors	XLR-3M Type

❍ Condenser Mic. 1

가. 기능

designed for capturing vocals, close miking instruments, amplifier cabinets, and other sources in live sound reinforcement and crucial recording applications.

나. 규격

• Operating Principle	Pressure Gradient

• Transducer	Condenser

• Diaphragm	0.75" (19 mm)

• Polar Pattern	Cardioid

• Frequency Range	20 Hz to 20 kHz

• Signal to Noise Ratio	76 dB A-Weighted

• Equivalent Noise Level	18 dB A-Weighted

25 dB ITU-R 468

• Maximum SPL	159 dB SPL

• Impedance	200 ohms

• CMRR	60 dB

• Operating Relative Humidity	90%

• Operating Temperature	-40 to 113°F (-40.00 to 45.00°C)

• Operating Current Consumption	2.8mA

• Dynamic Range	121 dB

• THD	< 1.0% up to 139 dB SPL Peak

❍ Condenser Mic. 2

가. 기능

The cardioid in particular has become the classic high-quality miniature microphone. Now also available in attractive stereo sets, with cardioid, hypercardioid or omni directional characteristics.

나. 규격

• Acoustical operating principle	Pressure/Pressure gradient transducer

• Directional pattern	omnidirectional/cardioid/hypercardioid

• Frequency range	20 Hz ... 20 kHz

• Sensitivity at 1 kHz into 1 kohm	12/15/10 mV/Pa

• Rated impedance	50 ohms

• Rated load impedance	1 kohms

• Equivalent noise level, CCIR1)	24/22/24 dB

• Equivalent noise level, A-weighted1)	13/13/15 dB-A

• Signal-to-noise ratio, CCIR(rel. 94 dB SPL)	70/72/70 dB

• Signal-to-noise ratio, A-weighted1) (rel. 94 dB SPL)	81/81/79 dB

• Maximum SPL for THD 0.5%	140/138/142 dB

• Maximum output voltage	10 dBu

• Supply voltage (P48, IEC 61938)	48 V ± 4 V

• Current consumption (P48, IEC 61938)	3.2 mA

• Matching connectors	XLR 3F

❍ Condenser Mic. 3

가. 기능

a matched, stereo pair of omnidirectional, pressure condenser microphones with an AES/EBU digital output and built-in A/D converter

나. 규격

• Operating Principle	Pressure Gradient

• Polar Pattern	Omnidirectional

• Frequency Range	20 Hz to 20 kHz

• Signal to Noise Ratio	69 dB CCIR

81 dB A-Weighted

• Equivalent Noise Level	25 dB CCIR

13 dB A-Weighted

• Maximum SPL	135 dB SPL

153 dB SPL with 18 dB Pad Engaged

• Sensitivity	-41 mV/PA

• Power Requirements	48 V+/- 4 V

• Pad	Yes, 10 dB

• Output Connectors	3-pin XLR

• Operating Current Consumption	150 mA

❍ Condenser Mic. 4

가. 기능

The Neumann classic. Three directional characteristics and switchable pre-attenuation ensure suitability for a wide range of applications.

나. 규격

• Acoustical operating principle	Pressure gradient transducer

• Directional pattern	Omnidirectional, cardioid, figure-8

• Frequency range	20 Hz ... 20 kHz

• Sensitivity at 1 kHz into 1 kohm	20/28/22 mV/Pa1)

• Rated impedance	200 ohms

• Rated load impedance	1 kohms

• Equivalent noise level, CCIR2)	26/23/25 dB1)

• Equivalent noise level, A-weighted	15/12/14 dB-A1)

• Signal-to-noise ratio, CCIR (rel. 94 dB SPL)	68/71/69 dB1)

• Signal-to-noise ratio, A-weighted2) (rel. 94 dB SPL)	79/82/80 dB1)

• Maximum SPL for THD 0.5%	117 dB (cardioid)

• Maximum SPL for THD 0.5% with preattenuation3)	127 dB

• Maximum output voltage	390 mV

❍ Cardioid Mic.

가. 기능

a professional low-profile condenser microphone for capturing vocals, instruments and ambiance in recording and sound reinforcement applications.

나. 규격

• Polar Pattern	Cardioid

• Frequency Range	35 Hz to 50 kHz

• Equivalent Noise Level	13 dB A-Weighted, 22 dB CCIR

• Maximum SPL	142 dB SPL

• Impedance	25 ohms

• Load Impedance	1000 ohms

• Free-Field Sensitivity	20 mV/PA

• Power Requirements	48 V+/- 4 V

❍ Dynamic Mic. 1

가. 기능

• Dual-diaphragm 1” edge-terminated transducer

• 134 dB dynamic range (up to 158 dB SPL)

• Lock Mode for live operation – all controls can be conveniently disabled

나. 규격

• Polar Pattern	Cardioid, Figure-8, Hypercardioid, Omnidirectional, Wide-Angle Cardioid

• Frequency Range	20 Hz to 20 kHz

• Signal to Noise Ratio	88 dB A-Weighted

• Equivalent Noise Level	6 dB A-Weighted

• Maximum SPL	158 dB SPL with 18 dB Pad Engaged

• Impedance	200 ohms

• Load Impedance	2200 ohms

• Sensitivity	23 mV/PA

• Power Requirements	48 V

• Low-Cut Filter	Yes @ 160 Hz, Yes @ 80 Hz, Yes @ 40 Hz

• Pad	Yes, 6 dB, Yes, 12 dB, Yes, 18 dB

• Output Connectors	3-pin XLR

• Operating Temperature	14 to 140°F (-10.00 to 60.00°C)

• Operating Current Consumption	4.5 mA

• Operating Voltage	44 V - 52 V

❍ Dynamic Mic. 2

가. 기능

a unidirectional dynamic microphone and a true professional workhorse used in many applications including the USA's presidential podium for over 3 decades.

나. 규격

• Transducer	(Moving Coil) Dynamic

• Polar Pattern	Cardioid

• Frequency Response	40 Hz - 15 kHz

• Power Requirements	None Dynamic, Requires No Phantom or Battery Power

• Output Impedance	150 Ohms (300 Ohms Actual) for Connection to Low Impedance Microphone Inputs

• Output Connectors	XLR-3M Type

❍ Dynamic Mic. 3

가. 기능

• Frequency response tailored for vocals, with brightened midrange and bass roll-off

• Pneumatic shock-mount system cuts down handling noise

• Built-in spherical wind and pop filter

나. 규격

• Transducer	Dynamic

• Polar Pattern	Cardioid

• Frequency Range	50 Hz to 15 kHz

• Impedance	150 ohms

• Sensitivity	-54.5 dBV @ 1 kHz

• Output Connectors	3-Pin XLR

❍ MIC Stand 'T'

가. 기능

T Type Mic. Stand

나. 규격

• 890mm부터 1,600mm 까지 높이 조절이 가능한 2단 폴딩 마이크 스탠드

❍ Drum

가. 기능

Maple Custom 최고급 드럼세트

나. 규격

• 스네어:14x.5.5, 탐탐(2):12x10, 13x11, 플로어탐:16x16, 베이스드럼 : 22x17

• 하드웨어 : 1자 심벌스탠드, T자 심벌스탠드, Hi-Hat 스탠드, 스네어스탠드, 베이스 페달

❍ Cymbals

가. 기능

강렬한 보컬에 적합한 밝고 선명한 사운드의 심벌

나. 규격

• 14" A Custom Mastersound 하이햇

• 17" A Custom Fast 크래쉬

• 21" A Custom Anniversary 라이드

• 18" A Custom EFX 심벌

❍ Guitar Amp. 1

가. 기능

• Three channels give you plenty of sonic possibilities

• Graphic EQ provides you with a wide range of sound-shaping options

나. 규격

• Type	Tube

• Number of Channels	3

• Total Power	90W

• Speaker Size	1 x 12"

• Reverb	Yes

• EQ	3-band, 5-band (Graphic)

• Preamp Tubes	7 x 12AX7

• Power Tubes	4 x 6L6, 1 x 5U4 (Rectifier)

• Inputs	1 x Instrument

• Outputs	4 x Speaker, 1 x Slave, 1 x Tuner

• Footswitch I/O	Yes

• Effects Loop	Yes

❍ Guitar Amp. 2

가. 기능

has proven that there is an all-round, small, powerful and yet simple to use complete solution for stage, studio and home use that works up to the highest demands and standards of acoustic players.

나. 규격

• 60 watts, dynamic control

• 8” (200 mm) twin cone speaker

• Twin channel, 3 and 2 band EQ

• Digital effect processor with 4 presets    (2 x reverb/delay/chorus)

• 6,5 kg (14.30 lbs)

❍ Bass Amp.

가. 기능

• Dual power amplifiers operate in true stereo or mono bridged mode

• Adjustable crossover points and low-to-high balance controls for bi-amp capabilities

• Ampeg's proprietary Ultra Hi/Lo Options

• -15 dB pad and "Bright" pad available on input

• Nine-band graphic EQ with independent level control

나. 규격

• Amplifier Type	Hybrid

• Output Power	1600 W RMS

• Channels	1

• Tube Types	3 x Preamp 12AX7/ECC83

• Output Impedance	4/8 ohms Mono

• Effects Loop	Yes, Series

• Master Volume	Yes

• Inputs	1 x 1/4" Mono Instrument

2 x 1/4" Mono Power Amp

1 x 1/4" Mono Footswitch

1 x 1/4" Stereo Footswitch

2 x 1/4" Mono Effects Return

• Outputs	4 x 1/4" Mono Speaker

3 x speakON Mono Speaker

1 x 1/4" Mono Effects Send

2 x XLR Mono Line Level

2 x 1/4" Mono Line Level

2 x 1/4" Mono Tuner

• Tone Section	Channel 1: Bass, Gain, Mid, Treble

• EQ	9-Band Graphic

❍ Keyboard 1

가. 기능

• Fast and smooth feel from the 88-key fully-weighted Hammer Action keybed

•1GB of memory to add your favorite instrument sounds from the Nord Piano Library

•Synth sections has 380MB of memory for the Nord Sample Library

•Expanded instrument selection includes electric pianos, strings, voices, folk instruments and more

•Vital functions have dedicated controls so you can access them quickly

나. 규격

• Number of Keys	88

• Type of Keys	Hammer Action

• Other Controllers	1 x Pitch Stick, 1 x Mod Wheel

• Presets	400

• Polyphony	40-60 Notes

• Effects	Yes

• Audio Outputs	4 x 1/4", 1 x 1/4" (Headphones)

• Pedal Inputs	1 x Sustain, 1 x Control, 1 x Organ Swell, 1 x Rotor

• MIDI I/O	1 x In, 1 x Out, 1 x USB

❍ Keyboard 2

가. 기능

• SCM (Spectral Component Modeling) tone generation system

• 17 selected acoustic and vintage electric piano sounds

• NW-STAGE wooden weighted keyboard

• VCM emulations of historical pedals including phasers, flangers, wahs and choruses

나. 규격

• Number of Keys	88

• Type of Keys	Weighted

• Other Controllers	Pitch Bend

• Presets	17

• Polyphony	128 Notes

• Effects	Yes

• Audio Outputs	2 x TS, 2 x XLR, 1 x TRS (Headphones)

• Pedal Inputs	3

• MIDI I/O	In/Out/Thru/USB

편집 조정실

❍ Workstation

가. 기능

DAW를 위한 고성능 워크스테이션

나. 규격

• Processor	3.5GHz 6코어 Intel Xeon E5 프로세서

• Memory	32GB of 1866 MHz DDR3 ECC RAM

• Graphics	2 x AMD FirePro D500 with 6GB of GDDR5 discrete memory

• Storage (SSD)	1TB PCIe-based flash storage

• Ports	6 x Thunderbolt 2

• 4 x USB 3.0

• 1 x HDMI 1.4 , 6 x mini DisplayPort (via Thunderbolt 2 ports)

Connect up to three 4K displays or six Thunderbolt displays

• 1 x Combined optical digital audio output/analog line out minijack

• 1 x Headphone minijack with headset output

• 1 x HDMI port supports multichannel audio output

• 1 x Built-in speaker

• Ethernet	2 x 10/100/1000 Mbps Gigabit Ethernet RJ-45

• Wi-Fi	802.11ac (802.11a/b/g/n compatible)

• Bluetooth 4.0

• Operating System	MacOS X

• Magic Mouse 2, 숫자 키패드를 부착한 Apple 키보드

❍ NoteBook

가. 규격

• Processor	2.9GHz 쿼드 코어 Intel Core i7 프로세서(최대 3.8GHz Turbo Boost)

• Memory	16GB 2133MHz 메모리

• Graphics	Radeon Pro 455(2GB 메모리)

• Storage (SSD)	1TB PCIe 기반 SSD

• Ports	Thunderbolt 3(USB-C) 포트 4개

• Touch Bar 및 Touch ID

• 백라이트 키보드 및 사용 설명서

• 1 x Built-in speaker

• Wi-Fi	802.11ac (802.11a/b/g/n compatible)

• Bluetooth 4.2

• Operating System	MacOS X

❍ 34“LED Monitor

가. 기능

DAW 편집 창 및 DAW시스템 전반 모니터링

나. 규격

• 화면크기	34“/86.7cm

• 해상도	3,440 × 1,440

• 패널	LED/IPS

• 화면비율 21:9 Wide (곡면 울트라 와이드)

• 명암비 1000:1(DFC 무한 :1)

• 공장색교정, sRGB 100%, 10bits (8bit + FRC)

• DDC/CI, HDCP

•S/W : On Screen Controller, 화면분할프로그램, 듀얼PC컨트롤러

❍ Software

가. 기능

Fully featured audio creation DAW System

나. 규격

1) Compose and Record

Record audio with up to 32-bit/192 kHz and experience exceptionally low latency when paired with an Avid audio interface

Use QuickPunch to quickly replace any questionable section with a better performance

Includes virtual instruments and audio loops

Compose music using notation tools in the built-in Sibelius Score Editor

Export sessions as Sibelius (.sib) files for further work in Sibelius.

2) Edit

Elastic Time and Elastic Pitch processing

Fine-tune music and audio with sample-accurate editing tools available in a single window

Speed up editing and mixing using the Clip Gain Smart Tool

Share audio mixes with Media Composer editors through AAF

Play HD video with the Avid Video Engine in a variety of HD video formats and Avid DNxHD sequences directly in the Pro Tools timeline without transcoding

3) Mix

Polish mixes with over sixty included effects, sound-processing and utility plug-ins

Includes reverbs, EQs, and compressors, guitar amp emulators, surround sound fold-down, channel strip dynamics, and more

Achieve phase-accurate mixes with Automatic Delay Compensation with four times the samples (16,383) to handle the largest mixes, no matter how many plug-ins used

Automate the settings of every element in the Pro Tools environment to add life to tracks and achieve the best mix possible

Bounce mixes to an iTunes library to share with others on a network

4) 구성

• Pro Tools Software

• iLok

❍ Mixer

가. 기능

• Impressive flexibility for its size

• Great-sounding Midas-designed mic preamps

• Eight true-stereo multi-effects processors

나. 규격

• Type	Digital

• Channels	32

• Inputs - Mic Preamps	16 x XLR

• Phantom Power	32 x Channels

• Inputs - Line	16 x XLR (Mic/Line)

• Inputs - Other	2 x RCA (Aux), 6 x TRS (Aux)

• Inputs - Digital	2 x AES50 (32 via Optional Digital Snake)

• Outputs - Digital	1 x AES/EBU (XLR), 32 x USB, 2 x AES50 (32 via Optional Digital Snake)

• Outputs - Main	8 x XLR

• Computer Connectivity	1 x USB

• I/O Expansion Slots	1 x Slot (Includes 32x32 USB Interface)

• Headphones	2

• Faders	17 x 100mm (Motorized)

• EQ Bands	4-band Parametric (6-band on Mix Bus)

• Effects	Yes

• Talkback	Yes

• Transport Controls	via Assign Section

• DAW Control	Yes

❍ Audio Interface

가. 기능

• Apogee's next-gen multichannel audio interface

• Class-leading AD/DA conversion

• Connects directly to Pro Tools HD Native, HDX, or Core/Accel systems

• Ultra-low 1.35mS latency

• Flexible modular I/O

나. 규격

• Computer Connectivity	Mini-DigiLink Port, USB

• Form Factor	Rackmount

• Simultaneous I/O	8 x 8

• A/D Resolution	44.1kHz-192kHz

• Analog Inputs	1 x DB-25 (8 channel)

• Analog Outputs	1 x DB-25 (8 channel), 1 x 1/4" (headphones)

• Digital Inputs	1 x DB-25 (AES), 1 x Toslink (S/PDIF, ADAT, SMUX), 1 x Coax (S/PDIF)

• Digital Outputs	1 x DB-25 (AES), 1 x Toslink (S/PDIF, ADAT, SMUX), 1 x Coax (S/PDIF)

• Clock I/O	2 x In, 2 x Out

• Data I/O	HD Mini-DigiLink, USB Type B

❍ Mointor Speaker

가. 기능

• MEME™ Technology Voice Emulation

• Dual Ring Radiator Tweeter

• 650 Watts of Power

나. 규격

• Description:	3-way active monitor with MEME™ voice emulation

• Controls:	Input level stepped attenuator, MEME voice select

• Input Impedance:	Balanced XLR, 50k Ohm Impedance

• Sensitivity:	90dB @ 1 meter with -15dBV input signal (Level control set to 0dB)

• Frequency Response:	36Hz – 45kHz (±3dB), 45Hz – 40kHz (±1dB)

• Bass Response:	-3 dB @ 36Hz, Q = 0.707, Slope = 18 dB/octave

• Crossover Frequencies: 250 / 3600 Hz (Passive crossover between Midrange and Tweeter)

• Tweeter:	1″ ring radiator, Low distortion motor, Rear waveguide chamber

• Midrange:	4.0″ aluminum cone, Aluminum phase plug, Low distortion motor, +/- 3.5 mm linear excursion

• Woofers:	8″ paper cone, +/- 9.5 mm linear excursion

• High Frequency Amplifier:	150W

• Low Frequency Amplifier:	500W

• with Speaker Stand

❍ Master keyboard

가. 기능

• Aftertouch-enabled, 76-note FSX semi-weighted keybed

• Stereo 128-note polyphony, for full stereo sound without note stealing

• Almost 10 times the waveform capacity of Yamaha's MotifXF

나. 규격

• Number of Keys	76

• Type of Keys	FSX semi-weighted with aftertouch

• Polyphony	128-note stereo polyphony

• Wave Memory	1.75GB internal flash user memory

• Number of Presets	128 factory, 2048 user

• Effects Types	DSP effects engine

• Arpeggiator	Yes

• Audio Playback	USB flash

• Sequencer	16-track, 64 songs

• Audio Inputs	2 x 1/4" (left, right)

• Audio Outputs	2 x 1/4" (left, right), 2 x 1/4" (assignable left, right), 1 x 1/4" (headphones)

• USB	1 x USB Type A, 1 x USB Type B

• MIDI I/O	In/Out/Thru/USB

• Pedal Inputs	2 x foot controller, 1 x assignable, 1 x sustain

❍ Custom Desk

가. 기능

• 장비의 원활한 열 배출을 위한 벤틸레이션 설계

• 88Key 이상의 마스터 키보드 지원

• A Parts 최고급 Electric Powder Coating 마감

• 후면 디스플레이 암 장착가능

나. 규격

• Electric Powder Coating

• Durable Construction

• Ventilation

• Cable Accessibility

• Detail

❍ P.D.U.

가. 기능

1 번 채널은 항상 전원이 공급되고 2 번 ~8 번 채널은 순차적으로 전원이 공급되며 역순으로 8 번부터 2 번까지 전원이 차단되는 제품

나. 규격

• AC Voltage meter	Line input / output (use of the voltage)

• Channel	8Ch (CH No.1 always power on)

• Ch load	220V/10A, 2200W

• Total max load	220V/45A, 9900W

• Channel interval	2 sec

• Link	Enable

• Link cable	4P DIN CABLE

• Control	Channel on / off switch, Lamp switch, Bypass switch

❍ Plug-In

• Flagship DSP-accelerator PCIe card for UAD Powered Plug-ins

• Loaded with 8x Analog Devices SHARC 21469 floating-point coprocessors

• Run complex mix processing without taxing your CPU in Pro Tools, Logic, Cubase, Nuendo, Digital Performer, and more

• AAX, VST, AU, RTAS support

• Mac compatibility: OS X 10.10 Yosemite and higher

• Windows compatibility: 64-bit editions of Windows 7, 8.1, or 10

• Linkable to existing UAD groups/systems — use up to 4 UAD-2s in one system

❍ 가상악기(Vsti)

가. 기능

•  Comprehensive collection of industry-standard virtual instruments and processors

•  500GB of content includes 87 products, 18,000 sounds - all loaded on a convenient install	hard drive

•  Includes 7 new additions to the Komplete lineup (see full list of included Komplete	products below)

•  Hard-hitting samplers, powerful synthesizers, and other virtual instruments provide tons of	songwriting power

• Virtually all products are fully compatible with AAX, VST, and AU plug-in hosts on Mac or	Windows PCs

나. 규격

• Includes:

1. Kontakt 5

2. Reaktor 6 (NEW!)

• Synthesizers

• Creative Samplers

• Drums and Percussion

• World Instruments

• Acoustic Pianos

• Electric Pianos and Organs

• Acoustic-electric Guitars

42. Scarbee Funk Guitarist

43. Strummed Acoustic (NEW!)

• Electric Bass

• Classical Instruments

• Cinematic

• Studio Effects

• Creative Effects

❍ Cue System

가. 기능

The system puts personal monitor mixing in the hands of musicians, singers, speakers and other talent, allowing them to set levels for up to 16 channels of audio, ultimately creating custom monitor mixes that favor their own signals.

나. 규격

• 16-channel digital stereo mixer to create your personal monitor mix

• Ultra-intuitive "analog" operation with total recall and 16 presets for custom mixes

• State-of-the-art 24-bit D/A converters for premium audio quality

• 16 Channel Select buttons with dual LEDs for perfect overview

• Level and Pan/Spread control per channel with LED meter

• 3-band EQ per channel with mid-band frequency control

• Standard CAT5e connection delivers power and 16 signals to each Personal Mixers

• Mounts easily on a mic stand with the P16-MB mic stand mount (not included)

• Extremely rugged construction ensures long life even under the most demanding conditions

• with HA8000

❍ Booth Combination panel (패치 판넬 공사)

가. 기능

메인부스에 설치하여 오디오, 네트워크, 영상, 전원등을 접속하기 위한 패널

나. 규격

• 16CH MIC/LINE I/O + LK16CH

• ETHERNET 4CH

• COAXIAL 2CH

• POWER 16A 2CH

밴드 연습실

❍ Drum

가. 기능

Maple Custom 최고급 드럼세트

나. 규격

• 스네어:14x.5.5, 탐탐(2):12x10, 13x11, 플로어탐:16x16, 베이스드럼 : 22x17

• 하드웨어 : 1자 심벌스탠드, T자 심벌스탠드, Hi-Hat 스탠드, 스네어스탠드, 베이스 페달

❍ Cymbals

가. 기능

강렬한 보컬에 적합한 밝고 선명한 사운드의 심벌

나. 규격

• 14" A Custom Mastersound 하이햇

• 17" A Custom Fast 크래쉬

• 21" A Custom Anniversary 라이드

• 18" A Custom EFX 심벌

❍ Bass Amp.

가. 기능

• Dual power amplifiers operate in true stereo or mono bridged mode

• Adjustable crossover points and low-to-high balance controls for bi-amp capabilities

• Five-position midrange selector for greater mid manipulation

• 2x Power amp in and preamp out

• Footswitch control for effects loop, graphic EQ, and mute feature (Footswitch not included)

나. 규격

• Amplifier Type	Hybrid

• Output Power	1600 W RMS

• Channels	1

• Tube Types	3 x Preamp 12AX7/ECC83

• Output Impedance	4/8 ohms Mono

• Effects Loop	Yes, Series

• Master Volume	Yes

• Inputs	1 x 1/4" Mono Instrument

2 x 1/4" Mono Power Amp

1 x 1/4" Mono Footswitch

1 x 1/4" Stereo Footswitch

2 x 1/4" Mono Effects Return

• Tone Section	Channel 1: Bass, Gain, Mid, Treble

• EQ	9-Band Graphic

• SVT-410HE

❍ Guitar Amp. 1

가. 기능

British-built, the 100 Watt 2 x 12â€³ all-valve JVM410C combo redefines versatility thanks to four tonally-independent channels: Clean, Crunch, OD1 and OD2, each with three switchable modes.

나. 규격

• CHANNELS	4

• WATTAGE	100W

• INPUTS	1 (+MIDI)

• CONTROLS	VOLUME/GAIN/BASS/MIDDLE/TREBLE x 4, REVERB x 4, CHANNEL SELECT x 4, PRESENCE, RESONANCE, FX LOOP, FOOTSWITCH/PROGRAMME

• SPEAKER SIZE	2 x12"

• OUTPUT POWER	70W EACH

• NAME	1 x CELESTION VINTAGE, 1 x CELESTION HERITAGE

• IMPEDANCE	16 Ohm

• PRE AMP VALVES	4 x ECC83

• POWER AMP VALVES 1 x ECC83 , 4 x EL34

• FOOTSWITCH	PEDL-91005 INCLUDED (6 WAY FOOTCONTROLLER)

• CABLES	POWER

❍ Guitar Amp. 2

가. 기능

• 85 watts

• 2 Jensen 12" speakers

• 2 channels

• Tube spring reverb

나. 규격

• Vintage Reissue '65 Twin Reverb 85W 2x12 Guitar Combo Amp

• 26-1/2"W x 20"H x 10-1/2"D

• 64 lbs.

❍ Keyboard 1

가. 기능

• Comprehensive high sound quality, including an enormous 741MB of waveforms

• An additional 128 Voices and 8 drum kits, for a total of 1,353 high-quality Voices

• Up to 2GB of additional content available through separately sold flash memory

• Enhanced sampling through 128MB of onboard SD-RAM

• The popular FSX (MOTIF XF6/7) and BH (MOTIF XF8) keyboards

나. 규격

• Tone Generator	AWM2, with Expanded Articulation

• Polyphony	128 notes

• Multi Timbral Capacity 16 Parts (internal), Audio Input Parts (A/D, FW*) *1 stereo Part

• Wave : 741 MB (when converted to 16-bit linear format), 3,977 waveforms

• Voice : Preset: 1,024 Normal Voices + 64 Drum Kits GM: 128 Normal Voices + 1 Drum Kit User: 128 x 4 (Bank 1: original, Bank 2 – 4: selected and copied from Preset bank) + 32 Drum Kits (No. 1 – 8: original, No. 9 – 32: selected and copied from Preset bank)

• Performance	User: 128 x 4 (up to 4 Parts)

• Filter	18 types

• Samples	Up to 128 Waveforms (Multi Samples) Up to 256 Key Banks per Waveform Up to 512 Key Banks

• Sampling Sources	Analog input L/R, Stereo output (Re sampling) FW (available when the FW16E has been installed)

• A/D Conversion	24-bit, 64x over sampling

• D/A Conversion	24-bit,128x over sampling

• Tempo (BPM)	5 – 300

• Recording type	Real time replace Real time overdub (with the exception of the Pattern Chain) Real time punch in/out (Song only)

• Tracks	Pattern: 16 Phrase tracks Pattern Chain: Pattern track, Tempo track, Scene track Song: 16 sequence tracks (Loop on/off can be set for each track), Tempo track, Scene track

❍ Keyboard 2

가. 기능

• Players, take note. You want the ultimate keyboard instrument for performing and creating? We've put it all together for you. Exceptional quality instrument sounds. A piano sound to die for. A truly realistic, naturally expressive keyboard. Convenient, comprehensive control.

• Real-time controls for tweaking of the sound as you play. Audio recording to USB memory. Extensive computer music features. Ease of use, plus compact size and portability. Introducing the S90 XS and S70 XS Music Synthesizer.

나. 규격

• Keyboard	88-key, fully weighted, hammer action, with velocity and aftertouch

• Number of Keys	88

• Type	Balanced Hammer Effect Keyboard

• Initial Touch	Yes

• Aftertouch	Yes

• Pitch Bend	Yes

• Modulation	Yes

• Tone Generating Technology	AWM2 with Expanded Articulation

• Multi Timbral Capacity	16 Internal Parts + Mic Input Part

• Ware ROM Capacity	456 MB (when converted to 16-bit linear format), 2,772 waveforms

• Number of Polyphony (Max.)	128

• Number of Voices	Preset: 1,024 normal voices + 64 drum kits, GM: 128 normal voices + 1 drum kits, User: 128 x 4 (Bank 1 - 3: selected and copied from Preset bank) Normal Voice + 32 drum kits

❍ Mic. 1

가. 기능

• Uniform cardioid pickup pattern isolates the main sound source and minimizes background noise

• Legendary Shure quality, ruggedness and reliability

• Cardioid (unidirectional) dynamic

• Frequency response: 50 to 15,000 Hz

나. 규격

• Type	Dynamic

• Frequency Response	50 to 15,000 Hz

• Polar Pattern	Cardioid

• Sensitivity(at 1,000 Hz Open Circuit Voltage)	–54.5 dBV/Pa (1.85 mV)

1 Pa = 94 dB SPL

• Connector	Three-pin professional audio connector (male XLR type)

• Net Weight	298 grams (10.5 oz)

• Dimensions	162 mm (6-3/8 in.) L x 51 mm (2 in.) W

❍ Mic. 2

가. 기능

a unidirectional dynamic microphone and a true professional workhorse used in many applications including the USA's presidential podium for over 3 decades. It has an extremely effective cardioid pickup pattern which isolates the main sound source while minimizing background noise.

나. 규격

• Transducer	(Moving Coil) Dynamic

• Polar Pattern	Cardioid

• Frequency Response	40 Hz - 15 kHz

• Power Requirements	None Dynamic, Requires No Phantom or Battery Power

• Output Impedance	150 Ohms (300 Ohms Actual) for Connection to Low Impedance Microphone Inputs

• Output Connectors	XLR-3M Type

❍ MIC Stand 'T'

가. 기능

The tripod microphone stand and boom offers sturdy support for live sound and recording applications. The stand features a fixed length boom measuring at 31.69" and the stands height is adjustable between 39.76 – 67.72".

나. 규격

• Construction	Zinc Diecast Base

• Stand Height	Adjustable: 39.76 - 67.72" (100.99-172cm)

• Boom Length	Adjustable: 31.69" (78.74cm)

• Base Type	Tripod

• Weight	5.51 lbs (2.49 kg)

❍ Monitor Speaker

가. 기능

• 1000W system power with 12" high-output LF driver and 1.4" titanium dome compression driver

• High-Definition Audio Processing for professional sound with unmatched clarity

• Precision 2-way crossover, driver time alignment, and phase correction for easy set up no matter the venue

• One-button speaker mode selection for application-specific voicing, get the sound you need

나. 규격

• Powered	Yes

• Power Configuration	Bi-amped

• LF Driver Size	1 x 12"

• HF Driver Size	1.4"

• LF Driver Power Amp	400W (RMS, Class D)

• HF Driver Power Amp	100W (RMS, Class AB)

• Crossover Frequency	3kHz

• Maximum Peak SPL	128dB

• Horizontal Coverage Angle	90 Degrees

• Vertical Coverage Angle	45 Degrees

• Enclosure Material	Polypropylene

• Mounting Options	Floor, Pole, Fly

❍ Speaker Stand

가. 기능

• Rugged yet lightweight aluminum and fiberglass PA speaker stands

• Clamping-lever choke secures height adjustments and prevents slipping

• Tripod also supported by a clamping-lever mechanism for added stability

나. 규격

• Load Capacity	110 lbs.

• Color	Black

• Stand Material	Aluminum

• Height	50"-75.9"

• Weight	5.1 lbs.

• Base Diameter	1.378" tube diameter

❍ Mixer

가. 기능

• Four TRS auxiliary outputs with dedicated send level controls on each channel for routing aux mixes to external devices such as reverb units, monitor mixers and more

• 3-band EQ on channels 1-8 and 2-band EQ on channels 9-16

• Pan/balance control on each channel

나. 규격

• Phantom Power	+48 V switchable, channels 1 - 12

• Input Channels	8x mono [mic/line]

2x mono/stereo [mic/line]

2x stereo [line]

• Pad	26 dB (mono)

• HPF	80 Hz, 12 dB/oct (mono/stereo: MIC only)

• Compressor	Threshold: +22 dBu to -8 dBu

Ratio: 1:1 to 4:1

Output level: 0 dB to 7 dB

Attack time: approx. 25 msec

Release time: approx. 300 msec

• Equalizer	EQ high gain: +15 dB/-15 dB, frequency: 10 kHz shelving

EQ mid gain: +15 dB/-15 dB, frequency: mono 250 Hz - 5 kHz peaking

EQ low gain: +15 dB/-15 dB, frequency: 100 Hz shelving

• LED	Peak LED turns on when post EQ signal reaches 3 dB below clipping

• Total Harmonic Distortion	0.03% @ +14 dBu (20 Hz to 20 kHz), GAIN knob: Min, 0.005% @ +24 dBu (1 kHz), GAIN knob: Min

• Frequency Response	+0.5 dB/-1.5 dB (20 Hz to 48 kHz), refer to the nominal output level @ 1 kHz, GAIN knob: Min

• Equivalent Input Noise	-128 dBu (mono input channel, Rs: 150 Ω, GAIN knob: max)

• Residual Output Noise	-102 dBu (STEREO OUT, STEREO master fader: min)

융복합형 공연장

A. Audio Part

❍ SUBWOOFER SPEAKER

가. 기능

본 기기는 전기신호를 저음의 음파로 변환시키는 장치이다.

나. 규격

• ACOUSTICAL SPECIFICATIONS

- Frequency response : 30 ~ 140Hz

- Max SPL: 135dB

- Woofer: 18”, 4.0” v.c.

• PROCESSOR SECTION

- Protections: Themel, RMS

- Sensitivity control: yes

- Limiter: soft limiter

- High pass: yes

- Controls: Volume, EQ shape, X-over

• AMPLIFIER

- Power supply: 1000 Watt

- Low frequencies: switching / 1000 Watt

- Cooling: convection / forced

- Connection: VDE connector IN

❍ LINE ARRAY SPEAKER (100°x 15°)

가. 기능

본 기기는 전기신호를 음파로 변환시키는 장치이다.

나. 규격

• ACOUSTICAL SPECIFICATIONS

- Frequency response: 55 ~ 20,000 Hz

- Max SPL: 135 dB

- Coverage angle(HxV): 100 ° x 15° max.

- Compression driver: 2” Driver, 3.0” Voice coil

- Woofer: 2 x 10” Driver, 2.5” Voice coil

• PROCESSOR SECTION

- Crossover frequencies: 1000Hz

- Protections: Themel, RMS

- Limiter: soft limiter

- Controls: Cluster, HF, High curving, Indoor

• AMPLIFIER

- Power supply: switching 700 Watt

- High frequencies: D/200w

- Low frequencies: Low D/500w

- Cooling: convection

- Connection: VDE connector IN

❍ LINE ARRAY SPEAKER BUMPER

가. 기능

본 기기는 Line Array Speaker를 천장에 거치하기 위하여 사용되는 Bar이다.

나. 규격

• Suspending bar for HDL20-A line array system. Stack bar included.

- FLY BAR PICKUP HDL 20 included.

- 3 pins included

- 1 stack bar included

- Strong steel construction

❍ LINE ARRAY SPEAKER LINK BAR

가. 기능

본 기기는 Line Array Speaker와 Subwoofer를 연결하기위한 Link Bar이다.

나. 규격

• Link bar for HDL 20-A and HDL 18-AS

- To link HDL 20-A to HDL 18-AS

- Strong steel construction

❍ LINE ARRAY SPEAKER PICKUP BAR

가. 기능

본 기기는 Line Array Speaker의 FLY BAR와 천장설치용 체인블럭을 연결하기 위한 PICKUP             ACCESSORY이다.

나. 규격

• 재질 : STEEL

❍ STAGE MONITOR SPEAKER

가. 기능

본 기기는 전기신호를 음파로 변환시키는 장치로 스테이지 모니터용이나 필드 모니터 등 다양          한 용도로 사용 할 수 있는 스피커이다.

나. 규격

• ACOUSTICAL SPECIFICATIONS

- Frequency Response: 60 ~ 20,000Hz

- Max SPL: 127dB

- Coverage angle(HxV): 60°x 60°

- Compression Driver: 1" neo, 1.7 voice coil

- Woofer: 12" neo, 2.5" voice coil

• INPUT SECTION

- Input Signal : bal/unbal

- Input/Output Connectors : XLR JACK/ XLR

- Input Sensitivity : +4dBu

• PROCESSOR SECTION

- Crossover frequencies: 1700Hz

- Protections: RMS limiter, HF

- Limiter: Soft Limiter

- Controls: Freefield, floor

• AMPLIFIER

- Power supply: switching 400W

- High frequencies: D/100W

- Low frequencies: D/300W

- 보호회로: 배기

- Connection: powercon input / powercon output

• PHYSICAL

- Dimension(WxHxD) : 450x324x417 mm

- Net Weight : 14.5 kg

- Cabinet : 발트해산 자작나무

- 색상 : 검정

❍ C/R MONITOR SPEAKER

가. 기능

본 기기는 2-way 양방향 레퍼런드 스튜디오 모니터이다.

나. 규격

• ACOUSTICAL SPECIFICATIONS

- 주파수 응답특성: 50 ~ 20,000Hz

- Max SP: 108dB

- Coverage angle(HxV): 110° x 110°

- Compression driver: 1" neo, 1“ voice coil

- Woofer: 6"

• PROCESSOR SECTION

- Crossover 주파수: 1900Hz

- Protections: Themel, RMS

- Sensitivity control: yes

- Limiter: Soft limiter

- Controls: HF adjust

• AMPLIFIER

- Power supply: 75 Watt

- High frequencies: 25 Watt

- Low frequencies: 50 Watt

- Cooling: convection

- Connection: XLR, Jack, RCA

❍ C/R MONITOR HEADPHONE

가. 기능

본 기기는 머리에 걸치고 귀에 압착하는 방식의 음을 듣는 수화기이다.

나. 규격

• Transmission type : Wired

• Headphone design (operating principle) : Closed

• Headphone impedance : 250 ohms

• Headphone frequency response : 5 - 35.000 Hz

• Nominal sound pressure level : 96 dB

• Construction : Circumaural (around the ear)

• Cable & plug : Coiled connecting cable with mini-jack plug (3.5 mm) & ¼“ adapter (6.35 mm)

❍ DIGITAL AUDIO MIXING CONSOLE

가. 기능

본 기기는 여러 가지로 출력되는 오디오를 하나로 혼합하여 소리의 균형을 잡아주는 장치이다.

나. 규격

• Connections

- 8 x (XLR) inputs / 8 x (XLR) outputs

- 4 x (XLR) monitor outputs

- 2 x (XLR) master outputs

- 2 x (XLR) AES3 stereo inputs / 2 x (XLR) AES3 stereo outputs

- 1 x (XLR) AES3 sync input / 1 x (XLR) AES3 sync output

- 1 x (XLR) talk input / 1 x (XLR) talk output

• Resilience N+1 cable redundancy and dual redundant PSUs

• Sampling frequency: 96kHz

• Latency delay: <2ms input to master (no compensation)

• Dynamic range: 106dB, 22Hz to 22kHz (no pre-emphasis)

• Crosstalk at 10kHz: -90dB physically adjacent input channels

• Fader/pan cut off at 1kHz: -100dB

• Fader/pan cut off at 10kHz: -100dB

• Display screens: 1 x 15” daylight-viewable colour screen

• LCD switch: 25 x RGB colour

• Motorised faders: 20 x touch-sensitive

• Fader resolution: 1024 steps

• Encoders: 31 x touch-sensitive

• Encoder resolution: 512 steps

❍ ADDITIONAL I/O BOX (CONSOLE)

가. 기능

본 기기는 Main Digital Mixer와 연동하여 채널 확장이 가능한 Stage Box이다.

나. 규격

• 5U rack I/O box houses

- 16 x (Male XLR) line outputs

- 48 x (Female XLR) mic/line inputs

- 1 x (EtherCon®) Ethernet control

- 3 x (EtherCon®) AES50 audio

- MIDI in / MIDI out / MIDI thru

- 1 x boot mode switch

- 1 x MUTE Button

- 5 x (9-way D-type) diagnostics

- N+1 cable redundancy and dual redundant PSUs

• Sampling Frequency: 48kHz (snake), 96kHz (with MIDAS console)

• Dynamic Range: 107dB 22Hz – 22kHz (no pre emphasis)

• Crosstalk @ 10kHz: -90dB physically adjacent input channels

❍ ADDITIONAL I/O CARD

가. 기능

본 기기는 본 기기는 네트워크  모듈이다.

나. 규격

• Module format: Cirrus CM-1 compatible

• Sample rates	: 44.1/48/88.2/96 kHz

• Audio channels (44.1/48kHz): Up to 64 bidirectional channels

• Audio channels (88.2/96kHz): Up to 32 bidirectional channels

• Sample Bit Depth: 16, 24 or 32 bits per sample

• Audio Buffering: Up to 2000 samples per channel

• Clock Source	: Onboard word clock or external word clock

• Interfaces: Primary and Secondary Dante network	interfaces

❍ DUAL CD PLAYER

가. 기능

본 기기는 다양한 기능과 고성능 특성을 갖춘 듀얼 디지털 미디어 플레이어이다.

나. 규격

• USB 메모리로 오디오 파일 재생 (AAC, AIFF, MP3, WAV)

• MP3 CD 파일 검색 시스템 CD Text / ID3 Tag 지원

• 드라이브 당 CD-R/RW 디스크 재생 2 Hot Starts/Stutter

• 드라이브 당 2 Seamless Loops

• w/B Point Trim Power on Playback

• Pitch Control: ±4.0/10.0/16.0/24.0/50.0/100.0%

• (CD) : ±4.0/10.0/16.0%(MP3)

• 형식: CD 플레이어

• 디스크 종류: 표준CD(12cm 디스크), CD-TEXT, CD-R, CD-RW 디스크

• 구성 및 규격

- Plyer unit	: W 482 mm x H 88 mm x D 252 mm

- Remote control unit	: W 482 mm x H 88 mm x D 62 mm

• 소비 전력	: 25 W

❍ Wireless Mic Receiver

가. 기능

트루 다이버시티 수신기. 42 MHz 대역폭 및 1,680개의 조정 가능한 UHF 주파수. 20개의 주파수          뱅크(각 32개의 프리셋)와 사용자가 프로그래밍할 수 있는 6개 뱅크. "무선 시스템 관리자              (Wireless Systems Manager)"를 통한 원격 제어 가능.

나. 규격

• 주파수 대역 : 516-865 MHz, 925-937.5 MHz

• 규격 : 212 x 202 x 43 mm

• 주파수 응답 (마이크로폰) : 25 - 18000 Hz

• 프리셋 : max. 32

• THD,:  총 왜곡율 < 0,9 %

• 무게 980 g

• 신호 대 잡음비 : > 115 dB(A)

• RF 주파수 대역 : 516...865 MHz

• 송신/수신 주파수 : 1680

• 스위칭 대역폭 : 42 MHz

• 피크 편차 : +/- 48 kHz

• 적합성 : ETS 300422 , ETS 300445 , CE , FCC

• 안테나 커넥터 : 2 BNC, 50 Ω

• 오디오 출력 레벨 (밸런스) XLR : +18 dBu max

• 오디오 출력 레벨 (언밸런스) Jack : +12 dBu max

❍ W/L Hand Mic.

가. 기능

고급 수퍼 카디오이드 마이크/전송기. 강력하고 선명한 사운드를 제공하는 Evolution 900 시리          즈 마이크 캡슐. 최고의 피드백 차단. 자동 잠금 기능으로 우발적인 설정 변경 방지.

나. 규격

• 주파수 대역 : 516-865 MHz, 925-937.5 MHz

• 규격 : Ø 50 x 265 mm

• 주파수 응답 (마이크로폰) : 80 - 18000 Hz

• 컴팬더 : HDX

• 프리셋 : max. 32

• 마이크로폰 : dynamic

• 음압레벨(SPL) : 154 dB(SPL) max.

• THD, 총 왜곡율 : < 0,9 %

• 무게 : 450 g

• AF 감도 : 2,5 mV/Pa

• RF 주파수 대역 : 516...865 MHz

• RF 출력 전압 : 10/30 mW

• 송신/수신 주파수 : 1680

• 스위칭 대역폭 : 42 MHz

• 피크 편차 : +/- 48 kHz

• 적합성 : ETS 300422, ETS 300445, CE, FCC

• 작동 시간 : > 8 h

❍ W/L Belt Transmitter

가. 기능

전환 가능한 HF 출력 전원을 갖춘 견고한 고품질 보디팩 전송기. 10 mW 출력으로 전환 시 더          많은 채널 선택 가능. 사용자 친화적인 메뉴와 백라이트 그래픽 디스플레이. 메탈 하우징.

나. 규격

• 주파수 대역 : 516-865 MHz, 925-937.5 MHz

• 주파수 응답 (마이크로폰) 80 - 18000 Hz

• 컴팬더 HDX

• LEMO Plug Male(Pin Michrophone 부착 커넥터와 호환)

• THD, 총 왜곡율 < 0,9 %

• 신호 대 잡음비 > 115 dB(A)

• RF 주파수 대역 516...865 MHz

• RF 출력 전압 10/30 mW

• 송신/수신 주파수 1680

• 스위칭 대역폭 42 MHz

• 피크 편차 +/- 48 kHz

• 적합성 ETS 300422, ETS 300445, CE, FCC

• 입력 전압 1,8 V line

• 송신기

- 무게 ~ 160 g

- 작동 시간 > 8 h

❍ Pin Microphone

가. 기능

스피치 및 보컬 애플리케이션을 위한 소형 무지향성 클립온 마이크. 높은 스피치 명료성. 의복          에 간단하게 부착 가능.

나. 규격

• 주파수 응답 (마이크로폰) : 20 - 20000Hz +-3db

• 연결 케이블 : LEMO Plug Female(Belt Pack Transmitter 부착 커넥터와 호환)

• 케이블 길이 : 1,6 m

• 픽업 패턴 : omni-directional

• 자유 음장내 감도, 무부하 : (1kHZ) 5 mV/Pa +-3db

• 상응하는 소음 수준 : 26 dB

• 최대 음압 레벨 (수동) : 142 dB

• 작동 전압 (단독 사용시) : 7,5 V

❍ W/L Headset

가. 기능

초소형 캡슐을 가진 초경량 헤드원 마이크.

무대, 방송, 전관 및 발표자 등을 필요로 하는 분야에 이상적으로 음질이 깨끗하고                     자연스럽습니다. 조절 가능한 이어 후크 는 마이크 붐이 어느쪽이던 쉽게 전송 가능하도록             평면 배치.

나. 규격

• Generation Element  : Electret Condenser

• Polar Pattern : Omni-Directional

• Frequency Range : 20-20'000 Hz

• Signal-to-noise ratio : 47 dB

• Equivalent SPL : 35dB

• Max. SPL : 127dB

• Nominal Impedance : 1 k0hm

• 연결 케이블 : LEMO Plug Female(Belt Pack Transmitter 부착 커넥터와 호환)

❍ Guitar Mic.

가. 기능

어답터가 장착되어 있는 기타용 클립 마이크로 라이브 사운드 및 라이브 녹음시 사용하는 원           핸드 마운팅 시스템이다.

나. 규격

• Transducer Type : Condenser

• Polar Pattern : Supercardioid

• Principle of Operation : Pressure Gradient

• Frequency Range :

- 20 Hz to 20 kHz

- 80 Hz to 15 kHz with 2 dB Soft Boost @ 10 to 12 kHz, Second Order Low-Cut Filter @ 80 Hz (>+/- 2 dB, 20 cm Distance)

• Sensitivity : 6 mV/Pa; -44.5 dB Reference: 1 V/Pa (Nominal, +/- 3 dB)

• Equivalent Noise Level : Typ. 23 dB(A) Reference: 20 µPa (Maximum 26 dB(A)) (A-Weighted)

• Signal to Noise Ratio :	71 dB (Reference: 1 kHz @ 1 Pa, 94 dB SPL)

• Total Harmonic Distortion (THD) :

- < 1 % up to 123 dB SPL peak

- < 1 % up to 120 dB SPL RMS sine

• Dynamic Range : 100 dB

• Maximum SPL : 142 dB (Peak Before Clipping)

• Output Impedance : MicroDot: 30 to 40 Ω, XLR: 100 Ω

• Cable Drive Capability : XLR: 984' (300 m)

• Output Balance Principle : Signal balanced with XLR adapter

• CMRR : XLR Adapter: > 60 dB at 50 Hz to 15 kHz

• Polarity : Positively increasing sound pressure produces positive going voltage at MicroDot pin (and pin 2 on DAD6001 XLR adapter)

• Operating Temperature : -40 to 113°F (-40 to 45°C)

• Relative Humidity : Up to 90%

• Cable Length : 6' (1.8 m)

❍ 악기용 Mic.

가. 기능

탁월한 선명함을 제공하는 전문가용 카디오이드 콘덴서 구즈넥. 유동적인 서스펜션을 갖춘 관          악기, 콩가, 드럼용 마이크. 손쉬운 장착/고정.

나. 규격

• Transducer : Condenser

• Polar Pattern : Unidirectional (Cardioid)

• Frequency Response : 20 Hz - 20 kHz

• Dynamic Range (Typical) : 132 dB (2.5 kΩ Load)

• Signal-to-Noise Ratio : 63 dB at 94 dB SPL (IEC 651)

• Maximum Input Sound Level : 143.5 dB

• Power Requirements : 11 to 52V DC Phantom Power, or

• (Use a Battery in the Optional MX1-BP Battery Powered Supply)

• Output Impedance : 150 Ohms

• Output Connectors : Tini Q-G Connector (from Microphone), XLR-3M Type (from Pre-Amp)

❍ W/L Antenna Splitter

가. 기능

안테나 분배기

나. 규격

• 감쇠 : 0 dB

• RF 주파수 대역 : 500 - 870 MHz

• 작동 전압 (단독 사용시) : 13,8 V DC

• Wireless Mic Receiver와 동일 제조사 제품에 한함.

❍ W/L Antenna

가. 기능

전방향성 수동형 안테나

나. 규격

• 임피던스 : 50 Ohm

• 어댑터 : BNC

• 주파수 응답 : 450 - 960 MHz

• 픽업 패턴 : Directional

• Wireless Mic Receiver와 동일 제조사 제품에 한함.

❍ Drum Mic. Set

가. 기능

베이스 드럼, 베이스 기타 캐비닛, 튜바에 특히 적합한 카디오이드 악기용 마이크. 견고하고 가          벼우며 쉽게 고정 가능. 스튜디오, 클럽, 리허설 룸, 소규모 콘서트 또는 홈 레코딩에 적합.

나. 규격

• 어댑터 : XLR-3 /, XLR-3M / XLR-3M

• 주파수 응답 : 20 - 16000 Hz / 40 - 16000 Hz / 40 - 20000 Hz

• 무게 : 318 g / 60 g / 93 g

• 공칭 임피던스 : 350 Ω / 350 Ω/ 50 Ω

• 최소 종료 임피던스 : 1000 Ω

❍ Condenser Mic. 1

가. 기능

스튜디오와 무대에서 보컬과 악기를 위한 멀티 패턴 콘덴서 마이크로폰. 모든 응용 분야에 완          벽한 음향 포착을 위해 9 개의 극 패턴을 선택할 수 있다.

나. 규격

• Audio frequency bandwidth : 20 to 20000 Hz

• Equivalent noise level : 6 dB-A

• Sensitivity : 23 mV/Pa

• Signal to Noise : 88 dB-A

• Bass cut filter : 160, 80, 40 Hz

• Electrical impedance : 200 Ohms

• Recommended load impedance : 2200 Ohms

❍ Condenser Mic. 2

가. 기능

다목적, 내구성 및 정밀한 단일 지향성 컨덴서 마이크로폰.  스튜디오 용도로 설계되었지만 라          이브 애플리케이션의 높은 음압 레벨 (SPL)을 견딜 수 있다.

나. 규격

• Transducer : Condenser

• Polar Pattern : Cardioid

• Frequency Range : 20 Hz to 20 kHz

• Signal to Noise Ratio : 80 dB

• Equivalent Noise Level : 14 dB A-Weighted

• Power Requirements : 48 V+/- 4 V

• Low-Cut Filter : 6 dB/Octave @ 115 Hz, 18 dB/Octave @ 80 Hz

• Output Connectors : 3-Pin XLR

• Operating Current Consumption : 4.65mA

• Dynamic Range : 131 dB

❍ Vocal Mic.

가. 기능

카디오이드 폴라 패턴의 듀얼 다이나믹 카트리지를 장착한 라이브 보컬 및 프리젠테이션을 위           한 휴대용 마이크로써 Dualdyne 기술이 적용된 제품이어야 한다

나. 규격

• Cartridge Type : Dual-Diaphragm dynamic (moving coil)

• Frequency Response : 40 Hz to 16 kHz

• Polar Pattern : Cardioid

• Output Impedance : 300 ohms

• Sensitivity : -51.5 dBV/Pa (1.85 mV) at 1 kHz, open circuit voltage

• Polarity : Positive pressure on diaphragm produces positive voltage on pin-2 with respect to pin-3

• Connector : 3-pin XLR male

• Housing : Die-cast aluminum with paint or brushed nickel finish

❍ Condenser Mic.

가. 기능

스튜디오 레코딩, 방송 및 사운드 강화 용으로 고안된 고품질의 단방향 콘덴서 마이크.

나. 규격

• Transducer : (Electret Bias) Condenser

• Polar Pattern : Cardioid

• Frequency Response : 20 Hz - 20 kHz

• Dynamic Range (Typical) : 120 dB

• Signal-to-Noise Ratio : 78 dB, (@ 94 dB SPL, IEC 651)

• Maximum Input Sound Level : 136 dB, (@ 250 Hz 0.5% THD), 146 dB, (with Pad)

• Power Requirements : Phantom 11 - 52v DC

• Output Impedance : 150 Ohms (85 Ohms Actual)

• Output Connectors : XLR-3M Type

• Pad : -10 dB Attenuation

• Low Frequency Roll-Off : -6 dB/Octave @ 100 Hz, -18 dB/Octave @ 80 Hz

❍ Dynamic Mic. 1

가. 기능

카디오이드 폴라 패턴의 다이내믹 카트리지를 장착한 라이브 보컬에 이상적인 휴대용 마이크.

나. 규격

• Transducer : Dynamic

• Polar Pattern : Cardioid

• Frequency Range : 50 Hz to 15 kHz

• Impedance : 150 ohms

• Sensitivity : -54.5 dBV @ 1 kHz

• Output Connectors : 3-Pin XLR

❍ Dynamic Mic. 2

가. 기능

전문 스피치용과 공연시 악기용으로 사용하는 단일지향성 다이내믹 마이크

나. 규격

• Transducer : (Moving Coil) Dynamic

• Polar Pattern : Cardioid

• Frequency Response : 40 Hz - 15 kHz

• Maximum Input Sound Level : Not Specified by Manufacturer

• Power Requirements : None Dynamic, Requires No Phantom or Battery Power

• Output Impedance : 150 Ohms (300 Ohms Actual) for Connection to Low Impedance Microphone                Inputs

• Output Connectors : XLR-3M Type

❍ Drums.

가. 기능

자작 나무로 제작된 스테이지 드럼으로 초보자 또는 전문가용으로 사용된다.

나. 규격

• Material :

- Birch; shell

- Steel; hoop

- Remo UT Clear; head (top and bottom)

- Remo UT Clear P3; head (batter)

- Remo UT Ebony P3; head (front)

• Dimensions :

- Bass Drum: 22 x 17" (55.9 x 43.2 cm)

- Floor Tom: 16 x 15" (40.6 x 38.1 cm)

- Tom Tom: 12 x 8" (30.5 x 20.3 cm) and 10 x 7" (25.4 x 17.8 cm)

- Snare Drum: 14.0 x 5.5" (35.6 x 14.0 cm)

❍ Cymbals

가. 기능

밝고 깨끗하고 선명한 사운드를 구현하는 심벌즈 세트.

나. 규격

• 14"  New Beat Hi-Hats (Pair)

• 16"  Medium Thin Crash

• 18"  Medium Thin Crash

• 21"  Sweet Ride

❍ MIC Stand 'T' 형 1

가. 기능

마이크 스탠드와 붐 암(Arm)으로 이루어진 업계 표준 마이크 스탠드.

나. 규격

• Boom arm:2-piece telescopic design

• Boom arm clamping:T-bar locking screw

• Boom arm length:from 470 to 775 mm

• Height:from 425 to 645 mm

• Height adjustment:clutch

• Leg construction:socket with foldable legs

• Material:steel

• Rod combination:2-piece folding design

• Special features:low-level microphone stand; zinc die-cast base

• Threaded connector:3/8"

❍ MIC Stand 'T' 형 2

가. 기능

마이크 스탠드와 붐 암(Arm)으로 이루어진 업계 표준 마이크 스탠드.

나. 규격

• Boom arm clamping: T-bar locking screw

• Boom arm length: 805 mm

• Height: from 900 to 1,600 mm

• Height adjustment: clutch

• Leg construction: socket with foldable legs

• Material: steel

• Product Category: Topline

• Rod combination: 2-piece folding design

• Threaded connector: 3/8"

B. Installation & Materials

❍ SWITCHING HUB

가. 기능

본 기기는근거리 통신망(LAN) 구축에 사용되는 장치로, 여러 대의 PC와 연결할 수 있으며 빠르          고 안전하게 데이터를 전송하는 장치이다.

나. 규격

• PAC Voltage meter : Line input / output (use of the voltage)

• Channel : 8Ch (ch.1 always power on)

• Ch load/ Total max : 220V/10A, 2200W , 220V/45A, 9900W

• Main voltage : 220V / 50Hz-60Hz, standard 3-wire, GND wire

❍ POWER DISTRIBUTOR

가. 기능

기기에 전원을 순차적으로 공급하는 기능으로 전원을 켜면 2번 채널부터 (1번채널은 상시전원)          8번 채널 순으로 전원을 공급하고, 끌 때에는 그 역순으로 8번 채널부터 차단하여, 한꺼번에 전          원을 공급 할 때 생기는 전원 과부하 현상을 줄인다.

나. 규격

• Fixed Port : 24P 10/100M + 10/100/1000M 25SFP/2TP

• LED Indicator : PWR, PoE, LinK/Act LED.

• Input Voltage : 100V~240V AC, 50/60Hz

• PoE Port : 24 /10/100Base-TX Port

• Powr Consumption : 0'C~70'C

• Switching Capacity : 52G

❍ MULTI FLOOR BOX

가. 기능

부대 바닥에 설치되는 마이크 및 스피커 박스이다.

나. 규격

• Fixed size : 210 x 160 x 108 (W x H x D)

• Cutting Size : 164 x 102 (W x D)

• Panel Size : 155 x 98 (W x D)

❍ MULTI JACK PANEL

가. 기능

각종 영상 음향 소스의 연장 및 확장단을 판넬에 부속 하여 벽부에 고정하는 판넬이다.

나. 규격

• Connector : Mic, Speaker, HDMI, Power

• Fixed size : 210 x 160 (W x H)

• Cutting Size : 190 x 140 (W x D)

❍ DIRECT BOX (Mono)

가. 기능

본 기기는 외부잡음을 방지하고 악기의 음색에 변화를 주지 않도록 하기 위해서 악기의 출력과  믹서의 입력사이에 설치하는 Active Direct Injection Box로써, Merge기능을 통해 스테레오 시그널을 모노로 출력 가능한 기기이여야 한다.

나. 규격

• Input Connections : 2 x 1/4" TS Phone In, Thru

• Output Connectors : 1 x 3-pin XLR Male

• Impedance : Input: 220 kOhms, Output: 600 Ohms

• Distortion : <0.5% (at 20 Hz)

• Frequency Response : 10Hz to 40kHz

• Signal-to-Noise Ratio : 119dB @ 100Hz

• Power : 48V Phantom, 2 x 9V Battery

❍ DIRECT BOX (Stereo)

가. 기능

본 기기는 외부잡음을 방지하고 악기의 음색에 변화를 주지 않도록 하기 위해서 악기의 출력과 믹서의 입력사이에 설치하는 Stereo Direct Injection Box이다.

나. 규격

• Harmonic Distortion : 0.01%(20Hz ~ 20kHz)

• Phase Distortion : 1 degreea at 1kHz / 8 degrees at 20kHz

• Harmonic Distortion : 0.01%(20Hz ~ 20kHz)

• Phase Distortion : 1 degreea at 1kHz / 8 degrees at 20kHz

• Output Connectors : 2 x XLR

• Input Impedance : 100 kOhms

• Output Impedance : 600 Ohms

• 2 x 1/4" TS phone Thru

• Controls : -15dB pad, Ground lift switch

• Frequency Response : 20Hz to 20kHz, +/-2.5dB

• Noise : Not specified by manufacturer

• Power : Passive

• Dimension(W x H x D) : 83 x 127 x 48 mm

❍ MIC CABLE

가. 기능

24AWG 굵기를 가지고 있는 2심의 오디오 케이블이며, 표준타입으로 마이크에 연결되어 사용한          다.

나. 규격

• 케이블 외경: 6.0 mm

• 케이블 중량: 17.2 (Kg/1,000ft)

• 케이블 재질: Flexible Matte PVC

• 케이블 색상: 검

• 도체굵기: 24 AWG (41x40)

• 도체재질: 구리

• 95% 순동 편조차폐

• 도체저항 (1,000ft): 25.4Ω

• 차폐/실드저항 (1,000ft): 6.0Ω

• 정전용량: 20 pF/ft 도체와 도체, 36 pF/ft 차폐와 도체

• 작동온도 : -40˚C to 80˚C

❍ MIC MULTI CABLE

가. 기능

24AWG 굵기를 가지고 있는 4채널 아날로그 오디오 멀티케이블이며, 배관/배선 및 실외 현장용          등 다목적으로 사용된다.

나. 규격

• 케이블 채널 수: 4채널

• 전체 케이블 외경: 11.04 mm

• 전체 케이블 중량: 45.3 (Kg/300m)

• 전체 케이블 재질: 열가소성 탄성체(TPE)

• 개별 케이블 실드: 알루미늄섬유 100% 포일 차폐

• 도체저항 (300m): 23.5Ω

• 그라운드 저항 (300m): 23.5Ω

• 정전용량: 24.0 pF/ft 도체와 도체, 43.0 pF/ft 도체와 쉴드

• 작동온도 : -30˚C to 75˚C

• UL타입: CMR

❍ MIC MULTI CABLE

가. 기능

24AWG 굵기를 가지고 있는 8채널 아날로그 오디오 멀티케이블이며, 배관/배선 및 실외 현장용          등 다목적으로 사용된다.

나. 규격

• 케이블 채널 수: 8채널

• 전체 케이블 외경: 14.22 mm

• 전체 케이블 중량: 79.3 (Kg/300m)

• 전체 케이블 재질: 열가소성 탄성체(TPE)

• 전체 케이블 색상: 검정

• 개별 케이블 색상: 갈, 적, 주, 노, 녹, 파, 보, 회

• 도체저항 (300m): 23.5Ω

• 그라운드 저항 (300m): 23.5Ω

• 정전용량: 24.0 pF/ft 도체와 도체, 43.0 pF/ft 도체와 쉴드

• 작동온도 : -30˚C to 75˚C

• UL타입: CMR

❍ VIDEO CABLE

가. 기능

신호 전송 대역폭 4.5Ghz 까지 지원되는 coaxial 케이블로써, 영상신호를 전송하거나 언발란스          타입의 디지털 오디오 신호를 전송할 때 사용된다.

나. 규격

• 대역폭: 4.5Ghz

• 임피던스: 75 Ω

• 도 체: 18AWG

• 도체재질: 순동 (단심)

• 절연체: 가스 고발포 폴리에틸렌

• 정전용량 : 16.3 pF/ft

• 작동온도 : -30˚C ~ 75˚C

• UL타입: CMR

❍ CONTROL CABLE

가. 기능

데이터를 보호하기 위해 2중 쉴드 처리가 되어진 케이블로 각 2쌍의 케이블에 쉴드처리 뿐아니          라 전체적으로 한번 더 쉴드처리가 되어 노이즈 방지 효과가 우수한 케이블입니다.

나. 규격

• 도체 : AWG26

• Connector : NEUTRIK etherCON Carrier

• 차폐 : Solid Copper

• 쉬스 : PVC

• 완성외경:(mm) : 6.4

• 중량 kg/300m : 39 g/ m

• 길이 : 100m

C. Video Part

❍ PTZ Camera

가. 기능

• Highly-accurate pan-tilt head offers precise, fast, fluid movement in all directions, enabling the capture of both slow- and fast-moving objects without excessive vibration and bounce

• Freeze During Preset function may be enabled to freeze the video during preset playback. The immediately preceding still image is output during preset movements so that the swiveling movement is not displayed.

나. 규격

• Image Sensor	1/2.3" Type MOS

• Lens	Motorized 30x zoom, f/1.6 to 4.7(F=4.3 to 129mm, 35mm equivalent: 31.6 to 962mm)

• Focus Distance	Entire zooming range: 3.9' / 120 cm, Wide end: 4" / 10 cm

• Compression	JPEG (M-JPEG)/H.264

• Image Resolution	VGA (640 x 480) (16:9 Letterbox: 640 x 320), QVGA: (320 x 240) (16:9 Letterbox: 320 x 180)

• Output Format	1080p: 29.97/25, 1080i: 59.94/50, 1080PsF: 29.97/25, 720p: 59.94/50

• Synchronization System	Internal

• Pan/Tilt Speed	Maximum 90°/sec

• Pan Range	± 175°

• Tilt Range	-30 to 90°

• Sound Level	NC35 (at normal speed), NC40 (when preset)

• Input/Output Connectors	LAN: 1 x RJ-45

Hd-SDI: 1 x BNC 75 Ω Compliant with the SMPTE292M standards	RS232C: 1 x Mini DIN 8-pin (in)/1 x Mini DIN 8-pin (out)

RS422: 1 x RJ-45 (control in RS422A)

USB: 1 x Mini B-port (for maintenance)

SD Card: ` x microSD card slot (for maintenance)

❍ Camera Controller

가. 기능

The Remote Camera Controller uses serial and IP control to support Panasonic pan/tilt heads,

integrated, and box cameras. Simple to set up and operate, the controller offers automatic IP          setup and can be configured via your PC

나. 규격

• Remote Control	Protocol - IPv4, RS-422 (Panasonic AW series protocol)

• Adjustment functions - Pan/Tilt, Zoom, Focus, Iris, Gain, Pedestal, Shutter, Detail,White Balance (Auto, R/B Gain), Black Balance (Auto, R/B Pedestal),

• Switch scene files : Preset memory - Up to 100

• Switcher Control	Connection - IP: 1selection (AUX/PVW/PinP/KEY-F), Parameter changes (Pan/Tilt lever, Zoom button)

• Interface	TALLY/GPI - TALLY input x 5 channels, GPI INPUT x 4 channels, GPI OUTPUT x 4 channels, D-sub 15 pin (female x 1)

• Power Requirements	DC 12V ±10 % (AC adapter provided)

❍ Video Mixer

가. 기능

HD와 SD 멀티 포맷을 지원하며 HD, SD모드 동일하게 총 7채널의 입력을 받을 수 있고 출력은

HD/SD SDI 4개(PGM, PVW, AUX, 멀티뷰어), DVI-D 2개(PGM, 멀티뷰어)가 장착되어 있다. 기존          의 HD, SD 방송용 비디오 스위쳐와는 달리 3D 믹싱 기능을 가지고 있다.

나. 규격

• Power Source	AC 100 V-240 V, 50/60 Hz

• Video Format	HD: 1080/59.94i, 1080/50i, 720/59.94p, 720/50p

SD: 480/59.94i, 576/50i

• Signal Processing	4: 2: 2: 4 12 bit (internal process)

• Video In	Analog Composite x 2, SDI x 4, HDMI x 2, DVI-I x 1

• Video Out	PGM: SDI x 1, DVI-D x 1

PVW: SDI x 1

AUX: SDI x 1

MULTIVIEW: SDI x 1, DVI-D x 1

• Audio In	XLR x 4 (L/R), SDI (Embedded Audio) x 4

HDMI (Embedded Audio) x 2

AUX: Pin Jack x 1(L/R)

Microphone: M6 x 1

Headphone: M6 x 1

❍ 자막기

가. 기능

PC가 필요없이 TV처럼 전원만 켜면 간편하게 영상에 문자 자막을 표시할 수 있는 제품으로,	사용법이 쉬운 Full HD의 고화질 문자 믹스 장비이다.

나. 규격

HD 본체

•  신호형식	SD, HD

•  입력신호	1x HDMI, 1x SDI (HD/SD), 1x Component (RGB/YPbPr)

2x Composite, 75 Ohm BNC Jack

•  출력신호	1x SDI (HD/SD), Loop Out, 1x HDMI, 1x Composite

•  편집화면 디스플레이	1x HDMI (최대 1920x1080)

•  I/O Interface	2x USB 2.0 (Front), 4x USB 2.0 (Rear), x LAN(RJ-45)

모니터

•  디스플레이	사이즈 : 23", 비율 : 16:9, 해상도 : 1920 x 1080

•  입출력 및 연결성	D-sub : 1, HDMI : 2, RF 입력(지상파/케이블) : 1

USB : 1, 컴포넌트 입력(Y/Pb/Pr) : 1, 컴포지트 입력 : 1

MHL : 1

•  기능	TV 수신(디지털 TV),   PiP(Picture in Picture)

•  제품 구성 리스트	1. Aurora 3K HD 본체, 2. 모니터, 3. 파워코드, 4. Manual CD

5. 키보드, 6. 마우스

❍ LED TV

가. 규격

• 화면크기	138 cm

• 해상도	1,920 × 1,080

• 패널	블랙 패널 +

• 화질엔진	HyperReal

• MR	60

• 와이드 컬러 컨트롤

• 스피커 시스템	2CH (Full Range SPK+Tweeter)

• 사운드출력(RMS)	10W+10W

• 돌비 사운드, DTS Premium Sound / DTS Premium Sound 5.1

• 크기 스탠드 제외 (가로x높이x깊이)    1232.6 x 752.5 x 98.0 mm

• 중량 스탠드 제외     15.6 kg

• 에너지효율 1 등급

• With TV Stand or Bracket

❍ HD레코더

가. 기능

portable broadcast quality record/playback deck that can also be rackmounted. It features a	6G-SDI input that allows capturing video up to 2160p30, and it incorporates one HDMI and	two 6G-SDI outputs. It records to two SD card slots, which enable virtually endless recordings.

나. 규격

• Video Input	6G-SDI: 1 x BNC

• Video Output	6G-SDI: 2 x BNC , HDMI: 1 x HDMI (type A)

• Audio Input	None (embedded audio only 16 channel)

• Audio Output	None (embedded audio only 16 channels SDI, 8 channels HDMI)

• Reference	In: Tri-Sync or Black Burst, Out: Tri-Sync or Black Burst

Input Connector: 1 x BNC, Output Connector: 1 x BNC

• Media Interface	2 x SD slots for SD, HD and UHD recording

Media Type: UHS II and able to support ProRes 4444 playback and 422 recording

• Supported Resolutions	4K : 3840 x 2160p: 30/29.97/25/24/23.98

HD : 1920 x 1080p: 60/59.94/50/30/29.97/25/24/23.98

1920 x 1080i: 60/59.94/50, 1280 x 720p: 60/59.94/50

SD : NTSC, PAL

• SDI Compliance	SMPTE 259M/292M/296M/425M

• SDI Metadata Support	HD RP188 and closed captioning

• Video Sampling	4:4:4:4

• Color Depth	10-bit

• Color Space	REC 601, REC 709

• Audio Sampling	Television standard 48 kHz, 24-bit

❍ 스트리밍 옵션

가. 기능

Web Presentermakes any SDI or HDMI video source appear as a USB webcam for higher	quality web streaming using software such as Skype or streaming platforms such as YouTube	Live, Facebook Live, Twitch.tv, Periscope and more.

나. 규격

• SDI Video Inputs	1

• SDI Video Outputs	1x program out, 1x loop out.

• SDI Rates	270Mb, 1.5G, 3G, 6G, 12G

• HDMI Video Inputs	1

• HDMI Video Outputs	1x loop out

• Analog Audio Inputs	1x XLR.2 x RCA HiFi.

• RCA	2 X HiFi Analog audio input

• XLR	1 X input supporting both microphone and line levels

• USB Webcam	1

• HDMI 2.0	1 X Input, 1 X loop out, (2 channel embedded audio)

• USB 2.0	1 X Type B

• Mini USB	1 X for software updates

• with Teranex Mini Smart Panel

• with Teranex Mini Rack Shelf

❍ 프로젝터

가. 기능

10,000-Lumen WUXGA DLP Projector features a solid-state laser light source	and full-spectrum color wheel that boosts color without sacrificing brightness

나. 규격

• Display System	1-Chip 0.67" / 1.70 cm DLP

• Native Resolution	WUXGA - 1920 x 1200 Progressive

• Format	NTSC 4.43, PAL M, SECAM N

• Brightness	10000 Lumens

• Uniformity	90%

• Aspect Ratio	16:10

• Dynamic Contrast Ratio	10000:1

• Color Range	R, G, B

• Lens Focus	Manual

• Projection Size	50 - 600" / 127.00 - 1524.00 cm

• Keystone Correction	Vertical: ± 40°, Horizontal: ± 15°

• Picture-in-Picture	Yes

• Ceiling Mountable	Yes

• Rear Screen Projection	Yes

• Light Source	Laser-phosphor

• Watts	Normal Mode: 742 W, Eco Mode: 617 W

• Life	Normal Mode: 20000 Hours, Eco Mode: 24000 Hours

• Fan Noise	Normal Mode: 41 dB

• Maximum Pixel Clock	162 MHz

• Remote Control	Yes

❍ DeskTop PC

가. 기능

조종실 장비 제어

나. 규격

• CPU	코어i7-6세대 / i7-6700 (3.4GHz)

• 운영체제	WINDOWS10 Pro

• VGA	(인텔) HD 그래픽스 530

• 메모리	8GB

• 저장장치	256GB SSD

• 메인보드	인텔 H110 CHIPSET

• CASE	슬림 케이스(083 블랙)

• 파워	300W

• 포트	PS2x2, DVI-Dx1, D-subx1, HDMIx1, USB3.0x2, USB2.0 x4, COMx1, RJ45 x1, Audio x3

• 네트워크	Gigabit(10/100/1000MBITS/S)ETHERNET

• 사운드	5.1 CHANNEL HIGHDEFINITION AUDIO

• 입력장치	한글106키보드&마우스

• 제조국가	한국

• KC인증	MSIP-REM-JYT-JT83AM18

• 규격	181x423x435

❍ Monitor

가. 기능

The 24" 16:9 LCD Monitor features a 16:9 aspect ratio allowing you to divide the display into          four separate sections, eliminating the need to flip between documents. Its dimming technology          is applied to minimize the flicker level that may cause eye fatigue. With almost-zero flicker           technology, looking at your computer screen for longer periods of time is more comfortable.

나. 규격

• Panel Type	TN

• Resolution	Maximum: 1920 x 1080 at 60 Hz

VESA: 1920 x 1080 at 60 Hz

• Aspect Ratio	16:9

• Brightness	250 cd/m2

• Color Gamut	sRGB 72%

• Response Time	2 ms GtG

• Refresh Rate	60 Hz

• Contrast Ratio	5M:1 (DFC)

• Interfaces	1 x HDMI

1 x 15-pin D-Sub connector

• Input Form	RGB analog (0.7 Vp-p / 75 ohms)

Digital

• Special Features	Color wizard

Reader mode

• LED Indicators	On Mode: White (for 15 seconds)

Sleep Mode: Blinking white

Off Mode: Off

• Plug and Play	DDC 2B (analog)

DDC 2B (HDMI)

DDC 2B (digital)

D. 조명시스템

❍ SUSPENSION / CEILING LIGHT BATTEN

가. 기능

공연 시 필요한 조명기구 및 기타 시설물을 손쉽게 취부 할 수 있도록 상 하 전동으로 동작하	는 기기로 FLOOR에서 1M 높이까지 하강 되어 손쉽게 부착할 수 있어야한다.

나. 규격

1) Device

• 크  기  : L=10,000 (도면 참조)

• 동  력  : 2.2KW x 4P

• 속  도  : 8-20 M/MIN

• 조  점  : 제작사양

❍ CABLE REEL

가. 기능

SPRING TYPE CABLE REEL은 반력을 이용한 것으로서 무대상부 GRID에 설치되어 바텐이 MOTOR에 의해서 움직이면 CABLE이 인출되면서 CABLE DRUM이 회전하고 이때, 반대방향으로 축적된 SPRING의 반력에 의해 바텐이 되돌아 올 때 CABLE DRUM이 회전하면서 CABLE을 자동으로 감기게 하는 구조를 이용 하여야한다.

나. 규격

• 외함은 STEEL PLATE 의 재질을 사용하여 견고하고 미려하게 제작 되어야 한다.

• SPRING은 장시간 동작에도 강도가 변화하지 않은 상급 재질을 사용해야 한다.

(강종 SK5 및 유사 재질)

• 절연이 좋아야 하고 마모 시 쉽게 교체할 수 있는 구조로 제작하여야 한다.

• 인입되는 전원 전단에 TERMINAL 형식으로 간편하게 연결될 수 있도록 한다.

• 설치가 용이하도록 BASE에 의한 BOLT조임 형식으로 제작하여야 한다.

• CABLE : 제작사양

❍ FLY DUCT

가. 기능

조명기구의 전원공급 장치로서 조명기구 PLUG의 사양에 맞게 내부배선 및 CONSENT가 전기적, 기계적으로 견고 하고 안전하게 부착되어야 하며, 수리 및 점검이 용이하게 부착하여 FLY DUCT에 연결이 쉽게 되도록 한다.

나. 규격

• BODY	: ALUMINIUM or STEEL

• CONSENT	: A TYPE 매입형

• 내부배선	: HIV 4.0SQ 이상 회로용량에 맞게 배선하며 회로는 COLOR로 구분한다.

• DIMENSION	: 제작사양

❍ TERMINAL BOX

가. 기능

전원 연결용 단자박스로서 무대 상부의 WIRE DUCT또는 FLY DUCT의 CABLE 접속용으로 사용되며 보수 및 점검 유지를 위해 뚜껑을 개폐구조로 하되, 외부의 이물질 유입 을 방지하여야 한다.

나. 규격

• BODY    :  STEEL PLATE 제작사양

• 단  자   :  조립식 16A 이상

❍ THREE BASIC LED MULTI ZOOM LIGHT

가. 기능

본 기기는 공연 연출용 조명기기로서 원격조정이 가능한 전동 줌 기능을 갖추고 있으며 다채로우면서 화려한 연출이 가능 하여야한다.

나. 규격

• LEDs: 14(4 in1) RGBW*10W TIANXIN LEDs     (A+UV Optional)

• 8° to 35° motorized zoom

• 4 digital LED display-flip option

• Master/Slave mode

• Built-in 8 chases-w,speed,strobe

• Control: USITT DMX 512

• DMX Channels: 11CH

• Strobe: Strobe effect(1-18 flashes per second)

• Power Supply: 120-240V,50/60Hz

• Power Consumption: 120W

• Cooling: Fan Cooled( High-Auto setting)

• IP Rating: IP44

• Lamp Life: 50,000hrs

❍ THREE BASIC LED MULTI ZOOM LIGHT

가. 기능

본 기기는 공연 연출용 조명기기로서 원격조정이 가능한 전동 줌 기능을 갖추고 있으며 다채로우면서 화려한 연출이 가능 하여야한다.

나. 규격

• LEDs: 14(6 in1) RGBWA+UV*18W TIANXIN LEDs

• 8° to 40° motorized zoom

• 4 digital LED display-flip option

• Master/Slave mode

• Built-in 8 chases-w,speed,strobe

• Control: USITT DMX 512

• DMX Channels: 13CH

• Strobe: Strobe effect(1-18 flashes per second)

• Power Supply: 120-240V,50/60Hz

• Power Consumption: 280W

• Cooling: Natural Cooling

• IP Rating: IP65

• Lamp Life: 50,000hrs

• Weight: 7KG

❍ THREE BASIC LED MULTI PAR LIGHT

가. 기능

본 기기는 공연 연출용 조명기기로서 다채로우면서 화려한 연출이 가능 하여야한다.

나. 규격

• LEDs: 9(4 in1) RGBW*10W TIANXIN LEDs

• BEAM ANGLE 15°(OPTIONAL　25°35°4５°）

• 4 digital LED display-flip option

• Display panel: LED digital display DMX address code, test or play auto-programs.

• Auto-mode:8 program parameters changeable by DMX console

•　Strobe: Speed adjustable between 0~32.5Hz

• DMX Channels: 13CH

• Power Supply: 120-240V,50/60Hz

• Power Consumption: ９0W

• Cooling: Natural Cooling

• IP Rating: IP65

• Lamp Life: 50,000hrs

❍ THREE BASIC LED SPOT LIGHT (400W)

가. 특징 및 기능

Three Basic LED Spot Light는 연색지수 (CRI) 97 이상의 PHLIPS LED (COB)의소자로 구성되어 강한 밝기와 자연 색 그대로의 뛰어난 색 재현력을 나타내야 합니다.(±1%)

LED 소자로 구성된 SPOT LIGHT 로서 피사체를 중심으로 KEY Light 역활을 하는 광원이다.

스튜디오 상부에 설치하여 인물의 중심 방향으로 투사하는 조명으로 인물의 윤곽을 선명하게

하고 입체감을 살려줄 수 있는 조명기구이다.

조명 소자는 최신 반도체소자를 사용하여야 하며, 개별적인 방열관 구조로 방열판과 일체형으로	개별 조립식 방식으로 제작되어 있으며, 촬영에 방해가 되지 않도록 FAN 혹은 기타 방열장치를	장착하지 않고 자연순환 방식의 Heat Pipe Technology 방식으로 제작되어야 한다.                         파워서플라이가 조명기구에 내장되어 있지 않고 분리 되어있어 조명기구의 고장에 따른	조치에 신속히 대응할 수 있다. 투사 각도를 조절하는 방법이 Knop 방식이 아닌 렌즈 스크류	방식이어서 조명기구의 불필요한 체적을 최소화 하였다.

전용 어플리케이션으로 REMOTE Control에 의한 Wifi DIGITAL SETTING 이 가능 하여야 한다.

렌즈 구면부와 조명기구 몸체의 분리가 원터치로 가능하다.

렌즈를 분리하여 보웬스 마운트 어댑터 악세사리를 장착할 수 있어야 한다.

별도의 Option으로 Diffusing Hood를 장착할 수 있어야 한다.

나. 규격

• Power : AC 100 ~ 240V 50~60Hz 0r DC 54V , 5A

• Power Consumption : 400 W cnds

• Light Source : COB 1PCS　PHLIPS LED

• CRI : >95

• Lumen Out put : >27,500Lumen

• Color Temperature : 5600K

• Lens Degree : 15o  ~ 45o

• Control Protocol : DMX512 /Master/slave / Wireless Remote Control APP Wifi 2.4G

• Refresh Frequency : 40,000 Hz

• Cooling Method : Efficient heat pipe technology, natural cooling, No Fan , No Noise

• Size : 565 x 390 x 450 이하

• Weight : 18.01Kg 이하(contains adapter)

• Material  : Aluminum & Steel

• Built-In 2.4G remote control receiver,Working with Wifi-2.4G control box, Can both control by the APP of mobile phone and 2.4G remote controller.

❍ THREE BASIC LED SPOT LIGHT (200W)

가. 특징 및 기능

Three Basic LED Spot Light는 연색지수 (CRI) 97 이상의 PHLIPS LED (COB)의소자로 구성되어 강한 밝기와 자연 색 그대로의 뛰어난 색 재현력을 나타내야 합니다.(±1%) LED 소자로 구성된 SPOT LIGHT 로서 피사체를 중심으로 KEY Light 역활을 하는 광원이다.

스튜디오 상부에 설치하여 인물의 중심 방향으로 투사하는 조명으로 인물의 윤곽을 선명하게	하고 입체감을 살려줄 수 있는 조명기구이다.

조명 소자는 최신 반도체소자를 사용하여야 하며, 개별적인 방열관 구조로 방열판과 일체형으로	개별 조립식 방식으로 제작되어 있으며, 촬영에 방해가 되지 않도록 FAN 혹은 기타 방열장치를	장착하지 않고 자연순환 방식의 Heat Pipe Technology 방식으로 제작되어야 한다.	파워서플라이가 조명기구에 내장되어 있지 않고 분리 되어 있어 조명기구의 고장에 따른

조치에 신속히 대응할 수 있다. 투사 각도를 조절하는 방법이 Knop 방식이 아닌 렌즈 스크류

방식이어서 조명기구의 불필요한 체적을 최소화 하였다.

전용 어플리케이션으로 REMOTE Control에 의한 Wifi DIGITAL SETTING 이 가능 하여야 한다.

렌즈 구면부와 조명기구 몸체의 분리가 원터치로 가능하다.

렌즈를 분리하여 보웬스 마운트 어댑터 악세사리를 장착 할수 있어야 한다.

별도의 Option으로 Diffusing Hood를 장착할 수 있어야 한다.

나. 규격

• Power : AC 100 ~ 240V 50~60Hz 0r DC 54V , 5A

• Power Consumption : 200 W

• Light Source : COB 1PCS　PHLIPS LED

• CRI : >97

• Lumen Out put : >13,900Lumen

• Color Temperature : 5600K

• Lens Degree : 10o  ~ 65o

• Control Protocol : DMX512 /Master/slave / Wireless Remote Control APP Wifi 2.4G

• Refresh Frequency : 40,000 Hz

• Cooling Method : Efficient heat pipe technology, natural cooling, No Fan , No Noise

• Size : 520 x 370 x 290 이하

• Weight : 7.05Kg 이하(contains adapter)

• Material  : Aluminum & Steel

• Built-In 2.4G remote control receiver,Working with Wifi-2.4G control box, Can both control by the APP of mobile phone and 2.4G remote controller.

❍ THREE BASIC LED ELIPSOID SPOT LIGHT

가. 기능

램프에서 나오는 빛이 구형 반사경에 의해 퍼넬 렌즈를 통과할 때 나타나는 확산 현상을 이용하여 밝기가 고르고 테두리가 부드럽운 빛을 얻을 수 있는 조명기. 램프, 반사경 몸체와 렌즈 사이의 거리를 조절하여 빛의 각도를 조정 할 수 있다.

또한 사용 용도에 따른 렌즈의 교환이 쉬워야 한다.

나. 규격

• Power : AC 190 ~ 240V 50~60Hz(AUTO RANGING)

• Power Consumption : 100 W

• Light Source : COB 1PCS　CITIZEN LED

• CRI : >85

• The spot pixels distributed evenly (the deviation between the spot center and the edge is small), no halo edge. The image edge has no obvious color difference (eliminate the blue rim), and the imaging resolution reach micron grade (1/1000 mm of the object can be clearly imaged).

• Color Temperature : 3200K or 5600K

• Beam angle available of 19°/26°

• Control Protocol : DMX512 /Master/slave

• 16 Bit dimming, LCD display

• 19°5M distance：4339LUX.(Traditional 750w profile light 19°5M distance：4500LUX.) For the applications of surface light, box boom, side light,

❍ LED MOVING SPOT　LIGHT

가. 기능

극장 및 공연장의 컬러 페인팅용 무빙 라이트로서, DMX 512 신호 방식에 의해 라이트의 헤드가 상.하.좌.우로 자유 자재로 움직이며 조명을 할 수 있어야 하며,LED 램프 소자 를 사용하는 등기구로 칼라믹싱이 가능하여야 한다.

나. 규격

• Voltage：Auto 100-240V, 50/60Hz

• Power consumptions：240w

• Profile LED Source: Ultra bright TIANXIN LED

• Product size: 359×407×440mm

• Weight : N.W:16Kg; G.W: 17.5 Kg

• International universal control signal: DMX512

• DMX Channels: 18 DMX channels

• DMX, Sound, Auto, Slave/Master

• 2 Gobos wheels: Fixed gobo wheel & Rotating gobo   wheel (7 inter changeable quick clip gobos+open)

• Color wheel: 7 main colors+open with the rainbow     effect ,Iris effect, Frost effect, Focus: Electronic       Focus, Prism: 3 Face Rotating Prism

• DMX Connectors: 3 pin XLR connector in and out

• Center Beam Angle: 15°

• LED Beam Angle: 45°（optional 25°）

• Super low noise fans

• Program inside ,Adjustable flash frequency

❍ LED MOVING WASH　LIGHT

가. 기능

극장 및 공연장의 컬러 페인팅용 무빙 라이트로서, DMX 512 신호 방식에 의해 라이트의 헤드가 상.하.좌.우로 자유 자재로 움직이며 조명을 할 수 있어야 하며,LED 램프 소자를 사용하는 등기구로 칼라믹싱이 가능하여야 한다.

나. 규격

• Voltage: 100V-250V/50-60Hz

• Power consumptions : 420W

• Light Source: LED10W * 36pcs (Quad LED)

• Channel: 15CH

• Zoom Angle: 25°

• Control Mode: DMX512 Control, Sound Active, Master/Slave, Auto-run, Stand Alone.

• Color Mixing: RGBW

• Lumen: 10000lux, 5m

• Casing: Black, White

• Display Screen: Control panel with LCD display.

• Cooling: Forced air convection

• Pan & Tilt Function : Pan: 450°(8/16bit) Tilt: 270°(8/16bit)

• Strobe: 1-10/s strobe, very glare strobe

• Dimmer: Variable electronic dimmer (0-100%)

• Working Temperature: -20 - 40degree

• IP Grade:IP20

❍ DMX SPLITTER

가. 기능

조명 콘솔의 디지털 신호인 DMX신호를 분배하고 증폭하여 먼 거리까지 신호를 전달하여주는 장치 이다.

나. 규격

• Voltage：AC190V~230V 50/60Hz±10％

• 1 IN　8 OUT , THRUH Socket.

• Independent transformer for each input and output channel

• Eight optical isolation signal amplification to expand DMX signal output

• Amplification function can make connection extended over the standard Technical parameter

• Output signal interface use three-pin XLR female socket.

❍ SAFETY CHAIN

가. 기능

LIGHT를 BATTEN에 설치한 후 라이트의 추락을 방지하기 위하여 라이트와 바텐을 연결하여주는 안전고리이며 견고 하게 제작 하여야 한다.

나. 규격

• 재   질  :  STEEL WIRE ∅ 2  L=700

❍ LIGHT HANGER

가. 기능

LIGHT를 BATTEN에 설치할 수 있도록 하는 부속 이며, 장착 및 취급이 간편하고 기계적, 물리적으로 견고하도록 재료를 선정 하여야 하며 특히, 기구의 흔들림에 의하여 BATTEN으로부터 이탈되지 않는 구조이어야 한다.

나. 규격

• BODY	:  프레스 및 압출가공  TYPE

• 재   질  :  AL 및 스틸(제작사양에 따라 상이)

• 도   장  :  흑색 및 기타 색상

❍ PLACARD BATTEN

가. 기능

공연 시 필요한 현수막 및 기타 시설물을 손쉽게 취부할 수 있도록 상 하 전동으로 동작하는 기기로 FLOOR에서1M 높이까지 하강 되어 손쉽게 부착할 수 있어야한다.

나. 규격

• 크  기  : L=10,000 (도면 참조)

• 동  력  : 1.5KW x 4P

• 속  도  : 8-20 M/MIN

• 조  점  : 제작사양

❍ ROLL SCREEN

가. 기능

상,하로 이동되는 영사막으로 불필요시 상부의 박스로 감아 두어 공간을 극대화 시키고 작동시 소음이나 잡음을 최소화 하여야 한다.재 질은 매트화이트를 기본으로 한다.

나. 규격

• 크  기  : 300인치

• 동  력  : DC 270W ~ 370W

• 속  도  : 제작사양

• 조  점  : 제작사양

❍ COVER　CURTAIN

가. 기능

무대부에 설치되는 막으로서 좌우로 계폐되어 공연 행사의 장면 전환 및 무대를 가려주는 역할을 한다.

케리어 레일은 알루미늄으로 제작된 제품을 사용 하여야 하며 시각적인 효과를 위한 커튼에 입체율(주름)를 적용하여야 한다. 또한 CURTAIN은 지정색상으로 제작하며 지정색상이 없을 경우 진자주 색으로 하며 재질은 벨벳을 사용한다.

나. 규격

• 크  기  : L=10,000 x 6,000 (도면 참조)

• 동  력  : 0.4KW x 4P

• 속  도  : 제작사양

• 조  점  : 제작사양

❍ MAIN & R/D UNIT RACK

가. 기능

주간선 M.C.C.B MAGNET S/W 및 기타 전기장치 등으로 구성된다.

제작사양에 따라 전기적으로 안전하게 제작되어야 하며 시설 관리자가 동작 상태를 쉽게 볼 수 있는 곳에 설치한 CONTROL 부분과 연결하여 사용한다.

나. 규격

• 외함은 옥내 자립형으로 제작되며, 각부의 주요 취부틀에 대해서는 STEEL PLATE 1.2T이상을 사용하고 측면 및 문은 1.2T이상의 강판을 사용한다.

• PANEL 전면에 DOOR를 설치하여, 설치 후 점검 및 보수가 용이 하도록 개폐할 수 있도록 제작한다.

• PANEL의 모든 입, 출입 배선은 현장여건에 따라 상부 및 하부로 통하여 결선 되도록 제작한다.

• 외 함  : 지정색상이 없을 경우 베이지 혹은 회색

• DIMENSION  : 도면참조(제작사양)

❍ COMPUTER CONSOLE

가. 기능

DMX-512 시그날로 조명기구를 콘트롤하는 제어용 저장 장치이며 간편한 메모리 방식을 채택하여 초보자도 쉽고 편 하게 운용할 수 있다. 인텔리전트 조명기구 40CH 조명기 를 240대 개별로 컨트롤 가능하며, 디밍 채널을 240 회로 까지 운용가능하다.DMX OUT 포트가 4개 구성되어있다.

나. 규격

• Voltage：AC110V~240V 50/60Hz±10％

• Voltage: AC 100-240V,50/60Hz.

• Performance characterisitic: 2048 dmx channels,4 optical isolative DMX output ports.

• Control 240 computer lamp or light path.

• LCD English display

• 15 repeat putting * 60 pages,900 show program,a two data control wheel.

• 200 sets of storage.

• 210 preset date storage,30 storage key * 7 pages,quick change computer light color,pattern,location data.

• Built-in a variety of fraphics operation effect,change size,speed,expansion parameter can create infinite change.

• Over 4000 built-in computer lamp data,the user can create new database computer lamp.

• The site provides the lamp base and software upgrade.

• Available USB disk storage of multiple users show file and backup system,new light library file or control a new software download form U disk loading to the console.

• The Lights go program music trigger function.

• Acceptance criteria MIDI Master device control,or to main-from the way to achieve Phantom2024 and machine work.

• The data auto-saves;

• Matching 12V gooseneck lamp.

• Size: 73*49*12cm 이하

• Weight: 14kg 이하

❍ MCC CONTROL CONSOLE & LOCAL CONTROL BOARD

가. 기능

자동제어에 의한 누름 버튼 스위치 방식으로 무대막의 조작 및 각 바텐을 CONTROL ROOM에서 구동시킬 수 있어야 한다.

나. 규격

• BUTTON SWITCH TYPE  : 조광형 사각 및 원형

• 접점전류	: 사용치의 배수

• 조광램프	: LED

• CONTROL SIGNAL	: DC 전원

❍ GRID IRON

가. 기능

모든 무대 조물기구의 구동부등을 설치하기 위하여 무대 상부의 가장 높은 곳에 지붕 슬라브 또는 트러스와 라운드 바 혹은 평철 등의 철재로 결합하여 보를 걸치고 형강과 상부의 공간이 여유가 있을 시에는 엑스펜디드 메탈로 발판을 설치하여 활차의 점검, 보수나 수리 작업을 실시 할 수 있도록 하여야한다.

작업에 용이하도록 제작설치하고 건축 및 기타 공종과 협의하여 다른 작업에 지장이 없도록 설치 하여야한다

나. 규격

• 재   질  :  ㄷ – 찬넬,라운드 바,평철,턴버클(필요시)

샤클(필요시),스틸플레이트, 앙카 및 빔 브라켓(필요시)

* 향후 추가적인 구동부(바턴)를 설치하기 위한 기본 인프라를 구축하여야 한다.

❍ PIPING & WIRING

설계도서 및 시방서에 준하여 시설하며, 모든 사항은 감독 관의 지시에 필히 따라야 한다.

시공 전 건축 구조 및 설비 도면과 충분히 비교 검토하여 공정상 차질이 없도록 하여야 한다.

일반 전기용품은 K․S 제품 사용을 원칙으로 하고,  K․S 제품이 없는 것은 정부기타 공인기관의 형식승인 제품을 사용하되 감독관의 사전 승인을 받아 시공하여야 한다.

사용하는 모든 전기 재료 중 규격화된 제품을 사용 하여야 한다. 현장에 반입되는 모든 기자재중 파손이 있을 시에는 즉시 신품으로 교체하여야 한다.

전기설비 시설에 변경이 필요할 때는 감독관의 지시에 따라야 한다.