과업설명서(사양서)

계 약 명	천안시영상미디어센터 장비 구매(교체․설치 포함)
주관기관	(재)충남문화산업진흥원

2015. 12.

www.ctia.kr

Ⅰ	과업개요

□ 사업개요

○ 발 주 처 : (재)충남문화산업진흥원 천안시영상미디어센터

○ 과 업 명 : 천안시영상미디어센터 장비 구매(교체․설치 포함)

○ 계약기간 : 계약일로부터 15일 이내

○ 기초금액 : 금49,995,000원(금사천구백구십구만오천원), 부가세 포함

○ 납품장소 : 천안시영상미디어센터 내 발주처 지정장소

○ 납품방법 : 현장설치도

□ 목     적

○ 트랜드에 부합하는 장비교체를 통해 비채 프로그램을 확장‧강화하여 이용자 만족도 제고 및 활성화 도모

○ 건전한 여가문화를 조성하고 가족이 함께 할 수 있는 미디어 프로그램 운영

○ 양질의 영상제작 환경 구축을 통한 지역기반 영상제작 활동가 발굴 및 양성

□ 기대 효과

○ 매력도 있는 장비구축을 통한 취약이용계층(청소년) 해소

○ 영상제작 선도적 진흥기관으로서의 정체성 확립

□ 주요 과업 내용

○ 천안시영상미디어센터 사업별(교육, 상영, 제작지원) 장비구축

- 소프트웨어 및 하드웨어 등 총21종 구축

- 구축장소 : 오디오스튜디오, 상영관, 일반편집교육실, 고급편집실, 장비대여실 등

○ 기존 장비에 대한 부분 변경지원 및 해당 장비 활용교육 포함

○ 기타 구축에 수반되는 모든 제반사항

Ⅱ	과업내용

1. 구성

□ 장비구축은 각 사업별, 구축장소별 이용목적에 맞게 설치 또는 납품하고 해당 장비의 원활한 활용을 위한 기본운영교육 및 향후 최소 1년간 무상 A/S를 실시해야 한다. 모든 기능이 원활하게 작동 될 수 있도록 책임시공을 준수해야 한다.

□ 모든 장치는 그 용도에 적합한 부속물을 사용하며, 향후 소모성 부품의 원활한 교체가 가능하고 그 교체금액이 합리적인 제품이어야 한다.

□ 소프트웨어의 경우 천안시영상미디어센터가 안내한 해당 PC에 설치해야 한다.

□ SSD 구매의 경우 천안시영상미디어센터가 안내한 해당 PC에 설치 및 기존 소프트웨어 재설치까지 포함한다.

□ 오디오스튜디오 PC의 경우 하드웨어 업그레이드를 위한 재조립 및 설치를 해야 한다.

□ 모든 제품은 정품(신품)이어야 하며, 내수 등 A/S 불가 제품은 사용 금지한다.

□ 모든 제품은 구축 전 천안시영상미디어센터에게 구축내용을 보고해야하며 최종 확정 시 반드시 기일 내 구축해야 한다.

2. 오디오스튜디오 내 구축

□ 구축장비는 초기세팅 시 기존장비와의 호환성을 반드시 고려해야하고 누구나 쉽게 사용 및 운용할 수 있도록 기초운용교육을 해야 한다. 또한, 구축 후 일년 내 재교육을 요청할 수 있으며 이 경우 무상으로 방문교육을 진행해야 한다.

□ DAW / 1copy

가. 기능 및 요건

- Compose, Record, Edit, Mix

- Up to 128 Audio Tracks

- Offline Bounce

- Over 75 VIs, Effects, Utility Plug-Ins

- Work Directly with HD Video

- AAX Native, AAX, AudioSuite

- include Activation Card & iLok2 Usb Key

* 아래 사양과 동급 혹은 상위 사양이어야 한다.

나. 사양

구 분	내 용
Record and Compose	- Record audio with up to 32-bit/192 kHz and experience exceptionally low latency when paired with an Avid audio interface - Redesigned Avid Audio Engine and 64-bit performance delivers multiple times the processing power of previous versions of Pro Tools on the same hardware configurations - Loop recording/track comping workflows - Use QuickPunch to quickly replace any questionable section with a better performance - Easily create parts for practically any musical instrument using virtual instruments, a MIDI keyboard/controller or mouse, and the built-in MIDI editor - Includes virtual instruments and audio loops - Compose music using notation tools in the built-in Sibelius Score Editor - Export sessions as Sibelius (.sib) files for further work in Sibelius. - Exchange sessions with any Pro Tools user or studio, or work on projects created in other audio and video software, including Media Composer, Logic, Cubase, and other third-party apps directly in Pro Tools
Edit	- Elastic Time and Elastic Pitch processing - Fine-tune music and audio with sample-accurate editing tools available in a single window - Speed up editing and mixing using the Clip Gain Smart Tool - With the Beat Detective tool, quickly fix timing issues across multiple tracks, change the feel of a beat to get a different groove, or keep the rhythm section "in the pocket" by extracting the groove from a drumbeat and applying it to the bass part - Create and cut sound to picture using the built-in Timecode Ruler and video track - Record and edit voiceovers, Foley, and ADR with frame accuracy - Share audio mixes with Media Composer editors through AAF - Play HD video with the Avid Video Engine in a variety of HD video formats (such as QuickTime, XDCAM, and more) and Avid DNxHD sequences directly in the Pro Tools timeline without transcoding - Monitor the picture playback using optional video interfaces from Avid, AJA, and Blackmagic Design
Mix	- Polish mixes with over sixty included effects, sound-processing and utility plug-ins Includes reverbs, EQs, and compressors, guitar amp emulators, surround sound fold-down, channel strip dynamics, and more - Avid Channel Strip plug-in delivers exact replications of the renowned EQ and compression algorithms of the Avid System 5 - Achieve phase-accurate mixes with Automatic Delay Compensation with four times the samples (16,383) to handle the largest mixes, no matter how many plug-ins used Automate the settings of every element in the Pro Tools environment to add life to tracks and achieve the best mix possible - Speed up mix delivery with faster-than-real-time off-line bouncing with time-stamped automation - Get hands-on Pro Tools control with a choice of optional Avid Pro Mixing control surfaces and consoles, plus third-party boards - With direct SoundCloud support, share files privately with other collaborators, or share finished projects with the world - Bounce mixes to an iTunes library to share with others on a network
Virtual Instruments	- AIR Boom drum machine and sequencer - AIR DB-33 tonewheel organ emulator with rotating speaker simulation - AIR Mini Grand acoustic grand piano - AIR Structure Free sample player (based on AIR Structure) - AIR Vacuum monophonic vacuum tube synthesizer - AIR Xpand!2 multitimbral synth and sample workstation
Effects, Sound-Processing, Utility Plug-Ins	- 1-Band EQ III, 7-Band EQ III, AIR Chorus, AIR Distortion, AIR Dynamic Delay - AIR Enhancer, AIR Ensemble, AIR Filter Gate, AIR Flanger, AIR Frequency Shifter - AIR FuzzWah, AIR KillEQ, AIR Lo-Fi, AIR MultiChorus, AIR Multi-Delay - AIR Nonlinear Reverb, AIR Phaser, AIR Reverb, AIR Spring Reverb, AIR StereoWidth - AIR Talkbox, AIR Vintage Filter, AutoPan panning effects - BF76 Compressor 1176 emulator, Channel Strip (based on the System 5 console) - Click II, Compressor/Limiter, D-Verb reverb and ambience, DC Offset Removal - De-Esser, DigiReWire, Dither, Down Mixer (5.1 to stereo fold down), Duplicate - Eleven Free(guitar amp emulator based on Eleven), Expander/Gate, Gain - InTune digital tuner, Invert, Lo-Fi retro processing, MasterMeter oversampling meter - Maxim sound maximizer, Mod Delay III, Normalize, Pitch II, POWr Dither - Recti-Fi harmonic synthesis, Reverse, SansAmp PSA-1 tube amp simulator - Sci-Fi ring modulator, Signal Generator, Time Adjuster, Time Compressor Expansion - Time Shift time/pitch stretching, Trim, Vari-Fi speed shifter

□ Music S/W / 1copy

가. 기능 및 요건

- Powerful beat creation

- Alchemy. A synth powerhouse

- Build your own wall of sound

- The power of Patches

- Smart Controls. The fastest way to shape your sound

- The ultimate way to record

- Build, organize, and manage tracks

- Music and sound for picture

- Edit in perfect rhythm

- Get the most out of MIDI

- Music notation the way it should be

* 아래 사양과 동급 혹은 상위 사양이어야 한다.

나. 사양

구 분	내 용
Minimum System Requirements	- 4GB of RAM - Display with 1280-by-768 resolution or higher - OS X v10.9.5 or later - Requires 64-bit Audio Units plug-ins - Minimum 6GB of disk space. 49GB of optional content available via in-app download.
General	- 1220 definable key and MIDI commands - 90 recallable screen configurations - 200-step undo history - Full plug-in latency compensation, also for external audio and MIDI gear - 1/3840 note resolution for MIDI events
Audio	- Audio file and I/O resolution up to 24 bit/192kHz - Maximum project length greater than 6 hours at 96kHz; 13 hours at 44.1kHz - High-end dithering algorithms (POW-r, Apogee UV22HR) Score Editor - Up to 16 independent voices per part - Over 4000 predefined chord grids - Tablature supports up to 16 string instruments with any tuning
Mixer	- Up to 255 audio channel strips - Up to 255 software instrument channel strips - Up to 255 auxiliary channel strips - Up to 64 busses - Up to 99 external MIDI tracks - 15 inserts for internal or Audio Units effect plug-ins - 8 inserts for internal or Audio Units MIDI plug-ins - 8 sends per channel strip, pre- or post-fader, or post-pan - 32 groups for audio, software instrument, or MIDI channel strips

□ I/O / 1ea

가. 기능 및 요건

- 8-Lane PCIe Gen2 I/O Card

- Multi-Rate 12G-SDI and HDMI Connections

- Supports UHD 4K and DCI 4K Up to 60 fps

- Single & Dual Link 4:4:4:4/4:2:2 Signals

- 3D Stereoscopic SDI Output at 4:4:4:4

- Up/Down/Cross Conversion

- Optional Optical Fiber I/O Modules

- Breakout Cable for Analog / RS-422

- Genlock & Deck Control

- Support Pro Tools Software

* 아래 사양과 동급 혹은 상위 사양이어야 한다.

나. 사양

구 분	내 용
SDI Video Input	- 2 SDI
SDI Video Output	- 2 SDI
Analog Video Input	- 1 x Component or S-Video or Composite
Analog Video Output	- 1 x Component or S-Video or Composite
HDMI Video Input	- 1 x HDMI type A connector (supports Ultra HD 4K 60p in 4:2:0)
HDMI Video Output	- 1 x HDMI type A connector (supports Ultra HD 4K 60p in 4:2:0)
Analog Audio Input	- 2 channels of professional balanced analog audio
Analog Audio Output	- 2 channels of professional balanced analog audio
AES/EBU Audio Input	- 2 channels unbalanced with sample rate converter
AES/EBU Audio Output	- 2 channels unbalanced
SDI Audio Input	- 16 channels embedded in HD/2K/4K - 8 channels embedded in SD
SDI Audio Output	- 16 channels embedded in HD/2K/4K - 8 channels embedded in SD
HDMI Audio Input	- 8 channels embedded in SD, HD, and Ultra HD
HDMI Audio Output	- 8 channels embedded in SD, HD, Ultra HD
Sync Input	- Blackburst in SD, 720p50, 720p59.94, 1080i50 and 1080i59.94 formats or Tri-Sync in any HD format
Device Control	- Sony compatible RS-422 deck control ports - Serial ports TxRx direction reversible under software control
Computer Interface	- PCI Express 8-lane generation 2, compatible with 8- and 16-lane PCIe with HDMI mezzanine card

□ HDMI Splitter / 1ea

가. 기능 및 요건

- The 1 to 2 HDMI Splitter allows transmission from a single HDMI audio or video device to be duplicated and simultaneously distributed to up to two connected HDMI devices such as TV, AVR, digital signage panel, HDTV, or digital projector. It is EDID and HDCP compliant and supports HD audio and all video formats up to 1080p / 24 Hz with full 3D support

* 아래 사양과 동급 혹은 상위 사양이어야 한다.

나. 사양

구 분	내 용
Video Amplifier Bandwidth	- 6.75 Gb/s
Input Video Signal	- 0.5 to 1 Vpp
Input DDC Signal	- 5 Vpp (TTL)
Maximum Single Link Range	- 1080p, 24-bit color depth
Transmission Distance	- HDMI Transmission: Up to 15m
Video Formats	- VESA : 640 x 480, 800 x 600, 1024 x 768, 1280 x 1024, 1600 x 1200, 1920 x 1200 - DTV/HDTV: 480i, 576i, 480p, 576p, 720p, 1080i, 1080p
Output Video	- HDMI 1.3b
Audio Formats Supported	- DTS-HD, Dolby HD
Power Consumption	- 4W maximum
Operating Temperature Range	- -41 to 95°F (-5 to 35°C)
Operating Humidity Range	- 5 to 90% RH (non-condensing)

□ TV / 2ea

가. 기능 및 요건

- 32inch LCD TV

- LED Back Light

- include Stand

- 녹음실 & 녹음조종실 설치

- 이동형 스탠드 포함

* 아래 사양과 동급 혹은 상위 사양이어야 한다.

나. 사양

구 분	내 용
TV	- 화면크기 : 80 cm - 패널 : 블랙패널+ - CMR (Clear Motion Rate) : 120 Hz - 스피커 종류 : Down Firing + Full Range - 음성출력(RMS) : 10W (L:5W x R:5W) - DTS Studio Sound / DNSe+ - DTS Premium Sound / DTS Premium Sound 5.1 - CPU : 싱글코어 - ConnectShare™ (USB 2.0) - 자막기능 - Component In (Y/Pb/Pr) - Composite In (AV) - HDMI : 2 port - USB - 색상 : Black - 에너지효율 등급 : 1등급 - 정격 전압 : AC220-240V 60Hz - 평균소비전력 : 28 W - 중량 스탠드 제외 (kg) 5.4 kg - 리모컨 종류 : TM1240
Stand	- 32~60인치 이동형 거치대 - 멀티코드 장착 - 셋업박스 및 컨트롤박스등 기기 전용 수납공간 - 이동 손잡이 및 바퀴 장착으로 이동이 용이 - 700 x 1980 x 750 mm - 재질 : 스틸 - 마감 : 분체도장

□ 마이크 / 2set

가. 기능 및 요건

-  대형 1” HF1 금도금 캡슐

-  몸체에 극성 선택, HPF 및 PAD 조절 기능 장착

-  3개의 선택 가능한 다양한 극성 – 무지향, 카디오이드, Figure 8

-  3단계 선택이 가능한 하이패스 필터 – 무적용(Flat), 40Hz 또는 80Hz

-  3단계 PAD 기능: 0dB, –5dB 또는 –10dB

-  초저잡음

-  내장 캡슐 쇼크마운트

-  SM6 쇼크마운트, 팝필터, 먼지 커버, T-Type 마이크 스탠드 포함

-  10년 보증

* 아래 사양과 동급 혹은 상위 사양이어야 한다.

나. 사양

구 분	내 용
Acoustic Principle	- Pressure Gradient
Active Electronics	- JFET impedance converter with bipolar output buffer
Capsule	- 1.00"
Polar Pattern	-
Address Type	- Side
Frequency Range	- 20Hz - 20kHz
Output Impedance	- 200Ω
Maximum SPL	- 147dB SPL (@ 1kHz, 1% THD into 1KΩ load)
Maximum Output Level	- 16.0mV
Sensitivity	- -36.0dB re 1 Volt/Pascal (16.00mV @ 94 dB SPL) +/- 2 dB @ 1kHz
Equivalent Noise Level (A-weighted)	- 7dB-A
Power Options	- 24V or 48V
Weight	- 860.00gm
Dimensions	- 209.00mmH x 55.00mmW x 55.00mmD
Output	- XLR

□ Hard Disk Drive / 1ea

가. 기능 및 요건

- 1TB Storage Capacity

- SATA 6 Gb/s Interface

- 3.5" Form Factor

- 64MB Cache

- 7200rpm Spindle Speed

- 녹음실 워크스테이션의 부트 드라이브로 장착 OS, 드라이버, 응용프로그램 최신버전으로 재설치 및 녹음실 하드웨어 연동설치

* 아래 사양과 동급 혹은 상위 사양이어야 한다.

나. 사양

구 분	내 용
Capacity	- 1TB
Cache	- 64MB
Interface	- SATA 6Gb/s
Rotational Speed	- 7200rpm
Formatted Capacity	- 1,000,204MB
User Sectors per Drive	- 1,953,525,168
System Compatibility	- Windows/Mac
Dimensions (WxHxD)	- 101.6 x 26.1 x 147 mm
Weight	- 0.69 kg

3. 상영관 및 이동상영장비 구축

□ 구축장비는 초기세팅 시 기존장비와의 호환성을 반드시 고려해야하고 누구나 쉽게 사용 및 운용할 수 있도록 기초운용교육을 해야 한다. 또한, 구축 후 일년 내 재교육을 요청할 수 있으며 이 경우 무상으로 방문교육을 진행해야 한다.

□ 2ch 무선마이크 / 1set

가. 기능 및 요건

- 프로페셔널 사운드 음질과 간편한 셋업 그리고 직관적인 인터페이스의 2ch 핸드헬드 무선마이크 시스템

- 기존상영관의 음향시스템에 연결 설치

* 아래 사양과 동급 혹은 상위 사양이어야 한다.

나. 사양

구 분	내 용
Output Impedance	- XLR connector : 200 Ω 6.35 mm (1/4”) connector: 50 Ω
Audio Output Level Ref.	- ±33 kHz deviation with 1 kHz tone
XLR connector	- –27dBV(into 100 kΩ load) 6.35mm(1/4”)
connector	- –13dBV (into 100 kΩ load)JFET impedance converter with bipolar output buffer
RF Sensitivity	- -105 dBm for 12 dB SINAD, typical
Image Rejection	- >50 dB, typical
Dimensions	- 40mm X 388mm X 116mm (H x W x D)
Power Requirements	- 12–15 V DC @ 160 mA (BLX88, 320 mA) supplied by external power supply
무선 핸드헬드 송신기	- 전원과 배터리 표시 LED - 조정 가능한 게인 컨트롤 - 주파수 매칭 기능 - AA 배터리로 최대 14시간 연속 사용 가능 - 최대 91m (300 feet)의 사용 가능 범위 - 주파수 사용 범위 925 - 937.5MHz - 오디오 범위 50-15,000Hz (마이크 종류에 따라 다름) - 송신기 RF 출력 전원 10mW, typical (지역에 따라 다름) - 오디오 출력 커넥터 XLR과 1/4” (6.3mm) 언발란스 - 최대 출력 레벨 -27 dBV (XLR, mic level), -13 dBV (1/4”) - 다이나믹 레인지 -27 dBV (XLR, mic level), -13 dBV (1/4”) - 시스템 디스토션 0.5% THD typical (ref. +/- 38 kHz deviation, 1 kHz tone) - 운용 온도 범위 -18°C (0°F) - +50°C (122°F)
기타	- Housing Molded ABS

□ 200인치 조립식 스크린 / 1set

가. 기능 및 요건

- Supplied standard as a kit

▸ front projection surface, folding frame and a heavy duty road case.

- Rear projection surfaces available as an optional extra.

- Main frame is a single piece of hinged aluminium that folds out.

- Legs are then attached, and are one metre wide along the base for stability.

- Projection Surface attaches with press studs.

- Drape Kits are available.

- Maximum size available 5,000mm wide.

- 16:10 Aspect Ratio available by order.

- Includes road case, front projection surface and frame with roll wheel

* 아래 사양과 동급 혹은 상위 사양이어야 한다.

나. 사양

- Diagonal : 200”

- Aspect Ratio : 16:9

- Image Size w x h (mm) : 4,430 x 2,490

- Total Width (mm) : 4,625

- Total Max Height (mm) : 3,910

- Total Min Height (mm) : 3,185

- Shipping Size l x h x d (mm) : 1,390 x 510 x 410

- Weight(Inc. Fabric) (kg) : 34

4. 교육용 영상장비 구축

□ 고프로 실버 어드벤처 액세서리 / 2set

가. 기능 및 요건

- 실버 어드벤처 모델에 적합한 정품 액세서리

* 아래 사양과 동급 혹은 상위 사양이어야 한다.

나. 사양

- 스포츠 핸들 마운트 홀더 어댑터 BMGP02, 삼각대 마운트 BMGP05 x 2ea

- 퀵 릴리즈 버클 마운트 BMGP07 x 2ea, 2 x flat, 2 x curved mounts BMGP11

- J-Hook 버클마운트키트 BMGP21 , 헤드스트랩 마운트 BMGP29

- 체스트 벨트 마운트 BMGP33, 수중 분실방지 플로티 스폰지 BMGP57

- 흡착젤 석션컵 마운트(7cm) BMGP65, 바이크 마운트 트라이포트 어뎁터 BMGP72

- 헬멧 셀프 촬영 연장 마운트 BMGP78, 수중 부양 부력 핸들 BMGP80

- 안개 김서림 방지 패드(12매) BMGP86, 실리콘케이스 BMGP92

- 미니어뎁터 BMGP93 x 2ea, 전용케이스 BMGP106

- 어댑터 + 37 UV Lens Cap BMGP110, 360도 회전손목 마운트 BMGP130

- 인조토끼털 윈드스크린 BMGP133, 회전식 클립 마운트 BMGP136

- 모노포트 경량 삼각대 BMGP184, 밴티드 헬멧 스트랩 마운트 BMGP26

- SELF Pro , 악세사리 파우치 BMGP102, 스켈레톤 하우징 케이스 BMGP83

- 듀얼배터리 충전기 + 배터리 2ea

- 600X 32GB micro SDHC 메모리카드

□ HDR-PJ670용 액세서리

가. 기능 및 요건

- PJ670과 유선마이크 간 결합 가능한 핫슈어뎁터 6ea

- 정품 충전기 및 충전지 6ea

- 3.5ⵁ 유선마이크 8ea

* 아래 사양과 동급 혹은 상위 사양이어야 한다.

나. 사양

- 핫슈어댑터 MSA MIS  6ea

- 충전지 ACC-FV100 / 충전기 ACC-TCV5 각6ea

- 유선마이크 RODE VIDEOMIC PRO 8ea

5. 일반편집교육실 내 구축

□ 구축장비는 초기세팅 시 기존장비와의 호환성을 반드시 고려해야하고 누구나 쉽게 사용 및 운용할 수 있도록 기초운용교육을 해야 한다. 또한, 구축 후 일년 내 재교육을 요청할 수 있으며 이 경우 무상으로 방문교육을 진행해야 한다.

□ SSD 구축 / 18ea

가. 기능 및 요건

-  240GB Storage Capacity

-  2.5" Form Factor

-  SATA Rev 3.0 6 Gb/s Interface

-  Phison PS3110-S10 Controller

-  Operating Vibration 2.17G

-  Non-Operating Vibration 20G

-  1,000,000 Hours MTBF

-  3.5인치 가이드 포함

-  기존 교육용 PC의 부트디스크로 장착하여 OS와 어플리케이션 재설치

* 아래 사양과 동급 혹은 상위 사양이어야 한다.

나. 사양

-  Capacity : 240 GB

-  Form Factor : 2.5"

-  Interface : SATA Rev 3.0 (6 Gb/s) with backward compatibility to SATA Rev 2.0 (3 Gb/s)

-  Controller : Phison PS3110-S10

-  Compressible Data Transfer (ATTO) : Read: 560 MB/s , Write : 360 MB/s

-  Incompressible Data Transfer : Read: 520 MB/s ,  Write: 350 MB/s

-  IOMETER Random 4k Read/Write  Read (maximum): Up to 100,000 IOPS

-  Write (maximum): Up to 84,000 IOPS

-  Random 4k Read/Write  Read: Up to 93,000 IOPS , Write: Up to 83,000 IOPS

-  PCMARK Vantage HDD Suite Score : 800

-  PCMARK 8 Storage Bandwidth : 223 MB/s

-  PCMARK 8 Storage Score : 4,940

-  Anvil Total Score : 4,700

-  Power Consumption  Idle: 0.39 W ,  Average: 0.5 W ,  Read: 1.4 W (maximum)

-  Write: 4.35 W (maximum)

-  Storage Temperature : -40 to +185°F (-40 to +85°C)

-  Operating Temperature : +32 to +158°F (0 to +70°C)

-  Vibration (Operating) : 2.17G Peak (7 to 800 Hz)

-  Vibration (Non-Operating) : 20G Peak (10 to 2000 Hz)

-  Life Expectancy : MTBF: 1,000,000 hours

-  Total Bytes Written (TBW) : 113TB 0.89 DWPD*

5. 제작지원용 장비구축

□ DSLR 사운드어뎁터 / 1ea

가. 기능 및 요건

- Two Neutrik Combo XLR / ¼" Inputs

- Loop Back for Playback Monitoring

- 3.5mm Jack for Connecting to Camera

- Headphone Amp with Volume Control

- 3.5mm Headphone Jack

- Phantom Power

- Switchable 12V/OFF/48V Phantom Power

- VU Meter

- Fast Acting Limiters

- Gain Switch for Each Channel

* 아래 사양과 동급 혹은 상위 사양이어야 한다.

나. 사양

구 분	내 용
Maximum Input Level	MIC level (LO gain), +10 dBu MIC level (HI gain), -20 dBu LINE level, +14 dBu
Output Level	-26 dBu at 0 dB on the VU meter
Frequency Response	20 Hz to 20 kHz (+/- 0.5 dB)
THD	Less than 0.01% @ 1 kHz, -30 dBu input
S/N Ratio	85 dB @ 1 kHz, -30 dBu input
Gain	LO, 0 dB HI, +30 dB
Phantom Power	Dual regulated 12- or 48-volt power supplies Current to 14 mA (direct short)
VU Meter	-18 to +3 dB in 3 dB increments
Battery Type	One 9-volt alkaline or lithium battery
Battery Duration	3 hours typical with alkaline battery (no phantom) 8 hours typical with lithium battery (no phantom)

□ 메모리카드 / 2ea

가. 기능 및 요건

- 64GB Storage Capacity

- Optimized for 4K Video Recording

- Up to 160MB/s Read Speed

- Up to 150MB/s Write Speed

- Compatible with RAW & JPEG Formats

- Includes RTV Silicone Coating

* 아래 사양과 동급 혹은 상위 사양이어야 한다.

나. 사양

- Card Type : CompactFlash Type I

- Storage Capacity : 64 GB

- Speed (X-rating) : 1067x

- Ultra Direct Memory Access (UDMA):  UDMA 7 Compliant

- Data Transfer : Read Speed 160 MB/s Maximum, Write Speed 150 MB/s Maximum

- Video Performance Guarantee : VPG- 65

□ 5인치 모니터 레코더 / 1ea

가. 기능 및 요건

-  1920 x 1080 Touchscreen LCD

-  Records 1080p up to 60 fps / ProRes 10-Bit, 4:2:2 Encoding

-  HDMI and 6G-SDI Video Inputs / Loop-Through Video Outputs

-  Stores to Single SDHC/SDXC Memory Card

-  On-Screen Histogram and Audio Levels

-  Can control settings on Blackmagic Micro Cinema Camera

-  Machined aluminum housing / Built-in kickstand

-  Six 1/4"-20 threaded mounting holes (three on top, three on bottom)

-  Dual Canon LP-E6 Type Battery Slots / AC Adapter Included

-  아래 추가 악세서리 포함

▸ LP-E6 배터리 4ea & 호환 충전키트

▸ 492LCD Micro ball head with Hot Shoe mount

▸ 주요장비 및 악세서리를 모두 수납 가능한 케이스(충격방지, 수심5M방수 완전 밀폐, 특수 Fiber플라스틱, 성형폼)

▸ FullHD녹화가 가능한 초고속 32GB SDHC 메모리 카드

* 아래 사양과 동급 혹은 상위 사양이어야 한다.

나. 사양

구 분	내 용
Display
Type	LCD touchscreen
Size	5" (12.7 cm)
Resolution	1920 x 1080
Viewing Angle	135°
Connections
SDI Video Input	1 x SD/HD/3G/6G-SDI (DIN 1.0/2.3 connector)
SDI Video Output	1 x SD/HD/3G-SDI (DIN 1.0/2.3 connector)
HDMI Video Input	1 x HDMI Type A
HDMI Video Output	1 x HDMI Type A
SDI Audio Input	16 channels embedded in SD and HD in QuickTime files
SDI Audio Output	16 channels embedded in SD and HD in QuickTime files
HDMI Audio Input	2 channels embedded
HDMI Audio Output	2 channels embedded
Audio Output	1 x 3.5 mm stereo analog audio output jack
USB Interface	1 x USB 2.0 (Mini-B connector)
General
OS Compatibility	Mac OS X 10.9 Mavericks, Mac OS X 10.10 Yosemite or later, Windows 7, Windows 8
Power Requirements	12 VDC
Batteries	2 x Rechargeable LP-E6 lithium-ion batteries
AC Adapter	110 to 240 VAC
Operating Temperature	41 to 104°F (5 to 40°C)
Storage Temperature	-6 to 113°F (-21 to 45°C)
Relative Humidity	0 to 90% non-condensing
Dimensions	5.63 x 1.20 x 3.54" (14.30 x 3.05 x 8.99 cm)
Weight	12.77 oz (362.02 g)
Recording
Recording Media	UHS-1 SDHC/SDXC cards
Codecs Supported	Apple ProRes 422 HQ / ProRes 422 / ProRes LT / ProRes Proxy
Supported Video Formats	SDI: 1920 x 1080p 23.98/24/25/29.97/30/50/59.94/60 1920 x 1080PsF 23.98/24 1920 x 1080i 50/59.94/60 1280 x 720p 50/59.94/60 625/50i PAL 525/59.94i NTSC HDMI: 1920 x 1080p 23.98/24/25/29.97/30/50/59.94/60 1920 x 1080i 50/59.94/60 1280 x 720p 50/59.94/60 480p60 576p50 625/25 PAL 525/29.97 NTSC
Recording Time	With 128GB SD card: Apple ProRes 422 HQ: 1.61 hours ProRes 422: 2.43 hours ProRes LT: 3.47 hours ProRes Proxy: 7.9 hours
SDI Video Sampling	4:2:2 YUV
SDI Audio Sampling	48 kHz, 24-bit
SDI Color Precision	10-bit
SDI Compliance	SMPTE 259M, SMPTE 292M, SMPTE 296M, SMPTE 425M
SDI Metadata Support	HD RP188 and closed captioning
SDI Color Space	REC 601, REC 709
HDMI Color Precision	10-bit
HDCP Compatible	No

□ 동시녹음기 / 2ea

가. 기능 및 요건

- 4x Balanced Mic/Line Inputs

- 6x Unbalanced Outputs

- Records to SD/SDHC/SDXC Cards

- HDDA Microphone Preamplifiers

- WAV, BWF, and MP3 File Format Support

- COAXIAL Digital Input and Output

- Cascade Multiple Recorders Together

- GANG Multiple Tracks Together

- Supports Lithium Batteries

- Includes Shoulder Strap

- CS-DR680전용 케이스 & 32GB SDHC 메모리카드 포함

* 아래 사양과 동급 혹은 상위 사양이어야 한다.

나. 사양

구 분	내 용
Recording
Recording Media	SD card (64 MB to 2 GB) SDHC card (4 to 32 GB) SDXC card (64 to 128 GB)
File System	FAT16 / FAT32
Recording Format	WAV: 44.1/48/96/192 kHz at 16/24-bit (192 kHz limited to 2-channel recording/playback) BWF: 44.1/48/96/192 kHz, 16/24-bit (192 kHz limited to 2-channel recording/playback) MP3: 44.1 kHz, 16-bit, 96 to 320 kbps
Analog Audio Inputs
Connector	Channel 1 to 4: 4x XLR/TRS 1/4" (6.3 mm) combo jack Channel 5 to 6: 2x 1/4" (6.3 mm) TRS
Input Impedance	2.4 kOhm
Phantom Power	+48V (+5%, -10%), +10 mA/ch
Standard Input Level	Low: -51.5 dBu High: -75.5 dBu
Maximum Input Level	Low: +3 dBu High: -21 dBu
Input Gain	63 dB
Line Input
Input Impedance	10 kOhm
Maximum Line Input Gain	63 dB
Analog Audio Outputs
Connector	RCA pin jacks
Output Impedance	200 ohm
Standard Output Level	-10 dBV
Maximum Output Level	+6 dBV
Speaker
Diameter	35 mm
Impedance	8 ohm
Maximum Output Level	500 mW
USB
Connector	Mini-B type
Format	USB 2.0 High Speed (480 Mbps)
Power	8x AA batteries(LR6) AC100 to 240V, 50-60Hz
Power Consumption	8 W (Phantom power on)
Continuous Battery Life	Alkaline Batteries (EVOLTA): About 6:00 (Rec:2-channel, Phantom power OFF) About 4:30 (Rec:2-channel, Phantom power ON) About 3:30 (Rec:6-channel, Phantom power ON) NI-MH Batteries: About 5:30 (Rec: 2-channel, Phantom power OFF) About 4:30 (Rec: 2-channel, Phantom power ON) About 4:00 (Rec: 6-channel, Phantom power ON) Lithium Batteries: About 11:00 (Rec: 2-channel, Phantom power OFF) About 9:30 (Rec: 2-channel, Phantom power ON) About 7:30 (Rec: 6-channel, Phantom power ON)
Operating Temperature	32 to 104°F (0 to 40°C)
Headphones
Connector	1x 1.4" (6.3 mm) stereo phone jack
Maximum Output Level	50 mW + 50 mW (32 ohm loaded)
Speaker
Diameter	35 mm
Impedance	8 ohm
Maximum Output Level	500 mW
Digital Interface
Connector	RCA pin jack
Format	IEC60958-3(S/PDIF) AES3-2003(AES/EBU) Single: 44.1/ 48 kHz Double: 96 kHz Quad: 192 kHz
Level	0.5 Vp-p typical
Output Impedance	75 ohm ±20% unbalanced
Sync
Connector	RCA pin jack
Audio Performance
Frequency Response	20 to 20,000 Hz +0.5/-1.5dB (Fs 44.1 kHz, LINE IN to LINE OUT, Input Level=FS-1dB) 20 to 20,0000 Hz +0.5/-0.5dB (Fs 48 kHz, LINE IN to LINE OUT, Input Level=FS-1dB) 20 to 40,000 Hz +0.5/-1.0dB (Fs 96 kHz, LINE IN to LINE OUT, Input Level=FS-1dB) 20 to 80,000 Hz +0.5/-5.0dB (Fs 192 kHz, LINE IN to LINE OUT, Input Level=FS-1dB)
Distortion	0.007% (1 kHz, LINE IN to LINE OUT)
S/N Ratio	100 dB (A-Weight, MIC IN to DIGITAL OUT) 100 dB (A-Weight, LINE IN to LINE OUT)
EIN	-124 dBu or less

□ 마이크 / 1ea

가. 기능 및 요건

- Superior broadcast sound quality

- High Sensitivity

- Super-cardioid polar pattern

- Designed to withstand adverse environmental conditions

- 50% less self-noise than the majority of shotgun microphones

- Extremely low handling noise

- High level of immunity to radio frequency interference

- True Condenser (external RF biased)

- Includes durable aluminium storage cylinder for transport, pop filter, mic clip and large zip pouch

- Designed for professional use on film, television, ENG & wherever high resolution broadcast audio is required

- 10 year extended warranty

- Greatly reduces handling and wind noise

- Accommodates most shotgun microphones 325mm in length and 19-22mm diameter

- Rycote Lyre suspension system onboard with internal spacing guide

- Lightweight skeleton handle with 3/8” thread mount

- Mogami cable with Neutrik and Switchcraft XLR connectors

- Dead Wombat windshield included

- Lightweight aluminium construction

- New ultra smooth extension and retraction system

- Easy to use locking mechanism

- Precision balanced

- 5m XLR Cable 포함

* 아래 사양과 동급 혹은 상위 사양이어야 한다.

나. 사양

구 분	내 용
마이크
Acoustic Principle	Line Gradient
Active Electronics	RF Bias
Capsule	0.50"
Polar Pattern
Address Type	End
Frequency Range	40Hz - 20kHz
Output Impedance	25Ω
Maximum SPL	130dB SPL (@ 1kHz, 1% THD into 1KΩ load)
Maximum Output Level	8.2mV
Sensitivity	-30.0dB re 1 Volt/Pascal (31.60mV @ 94 dB SPL) +/- 2 dB @ 1kHz
Equivalent Noise Level (A-weighted)	13dB-A
Power Options	+P48V
Weight	163.00gm
Dimensions	255.00mmH x 19.00mmW x 19.00mmD
블림프
Weight	550gm
Dimensions	285.00mmH x 490.00mmW x 125.00mmD
Warranty	10 year warranty
붐폴
Weight	940.00gm
Dimensions	3300.00mmH x 40.00mmW x 40.00mmD
Warranty	1 year

□ Jib / 1ea

가. 기능 및 요건

- Lets you capture shots from high angles and scale across scenes with cinematic movements

- Pulley wire system tilts your camera up and down in accordance with your movement of the jib

- Supports loads up to 6.6 lb

- Weighs only 11 lb

- Lets You Capture Shots from High Angles

- Lets You Fluidly Scale Through a Scene

- Pulley Wire Tilt Adjustment

- Supports Loads Up to 6.6 lb

- Weighs Only 11 lb

- Multi-Slot/Thread Camera & Tripod Plates

- Durable H-Beam Design

- Supports Standard Size Weight Plates

- Box Shaped Carry Case

- Bubble Level

- 집 운영을 위한 삼각대 509HD, 545BK 세트 포함

* 아래 사양과 동급 혹은 상위 사양이어야 한다.

나. 사양

구 분	내 용
Load Capacity	6.6 lb (3 kg); Optimal Load: 2.2 - 4.4 lb (1 - 2 kg)
Mount Types	Multi-slotted camera mount plate; multi-threads tripod mount plate
Dimensions	114 x 0.6 x 2" (290 x 1.5 x 5 cm) Pulley Wire Length: 138" (352 cm) Balance Wire Length: 60" (152 cm)
Total Weight	11 lb (5 kg)

□ LED 조명 / 4set

가. 기능 및 요건

- 고발광 LED 로우릴레이 전구를 적용하여 LED의 수명을 길게하고 안정성을 높임

- 전문적인 스튜디오 및 영화 촬영등에 적합한 모델로 고발광, 낮은 온도, 저 소비전력

- 2중 색온도(5600K, 3200K)조절가능

- 10%~100%의 미세한 밝기 조절 가능

- LCD터치 패널로 구성되어 LCD화면을 직접 보면서 터치를 이용한 미세한 색온도 및 광량 조절

- 전용 2구 수납 가방 x 2ea

- 전용 중형 스탠드 x 4ea

- 13.2Ah, 190Wh V마운트 배터리 x 8ea

- 2구 V마운트 배터리 배터리 충전기 x 4ea

* 아래 사양과 동급 혹은 상위 사양이어야 한다.

나. 사양

LED조명

- 색온도 : 3200K ~ 5600K / 밝기 조절 : 10% ~ 100% / 색 연속성 : CRI > 85

- 조도 : 7000 Lux / m / LED 수 : 1024 PCs / 출력 전압 : 61.5W

- 사이즈 : 40.3 x 45 x 9.5 Cm / 무게 : 2.7Kg

- 재질 : ABS Housing & Metal Barndoor and stand Bracket

V-마운트 배터리

- 14.8V, 13.2Ah, 190Wh

- With a built-in 4-level LED power status display

- Standard Power Tap connector: power camera light directly

- Operating temperature: -20℃~+55℃

- Dimensions: 98(W)×147(L)×71(D)mm / Weight: 1160g

충전기

- Input AC: 90~242VAC, 47~63Hz

- Output Charging Terminals 1 and 2: 16.8V 3.0A

- Output DC Power: 15V 4.0A

- Dimensions: 140(L) X 116(W) X 225(H)mm / Weight: 990g

- Operational Temperature: -10℃~35℃

- Portable two simultaneous charger. CE approved.

- Designed to recharge V type Li-ion battery

- Standard Mount: Install with“V”type mount.

- Provide DC power supply: As an adapter, can offer DC15V power supply for Camera. Adapter output: DC15V,4.0A.

□ Sony FDR-AX1 액세서리

가. 기능 및 요건

- 정품 대용량 배터리 및 충전기, 전용 메모리카드 32gb 각 2개

- 메모리카드 리더기 / 줌 서보

- 소프트 케이스 / UV Filter / 전용 또는 카메라와 적합한 삼각대 세트

- 콘덴서 마이크

- 무선 마이크 세트 x 2set

* 아래 사양과 동급 혹은 상위 사양이어야 한다.

나. 사양

- 대용량 배터리 NP-F970 x 2ea / 충전기 AC-VQ1050 x 2ea / 전용 메모리 XQD 32GB x 2ea

- 메모리카드 리더기 MRW-E80 / RM-1BP 줌 서보

- CC-195PL 소프트 케이스 / UV Filter / 504HD, 546BK 삼각대 세트

- NTG3 콘덴서 마이크

- UWP-D11 무선 마이크 세트 x 2set

□ 스테디캠(짐벌) / 1set

가. 기능 및 요건

- 3축 핸드헬드 짐벌시스템

- 손쉬운 세팅 및 효과적 스테디 기능탑재

- 단독, 2인 혹은 3인 촬영 시스템(별도 리모컨 활용) 기능

- 업라이트, 언더슬링, 브리프케이스 모드

- 모바일과 기기 간 블루투스 연동지원

- 엄지컨트롤러, 엄지컨트롤러 수신기, 베터리 각 1개(기본 패키지 보유 시 각 1개씩 추가, 정품)

* 아래 사양과 동급 혹은 상위 사양이어야 한다.

나. 사양

- 전원 연결 액세서리 : 12V 조절된 P-Tap x 2, USB 500mW x 1, DJI 라이트브릿지x 1

- GCU 입력 전원 : 4S 로닌 배터리

- 연결 : 2.4GHz 조종기,블루투스, USB

- PC 지원 소프트웨어 요건 : Windows XP SP3; Windows 7; Windows 8 (32 or 64 bit)

- 모바일 지원 소프트웨어 요건 : iOS 버전 6.1 또는 그 이후 버전 (예: iPhone 4s, iPhone 5, iPhone 5s, iPod touch 5 , iPad 3, iPad 4, iPad mini)

- 부하 질량 (참고 값) : 7.25kg (16lbs)

- 각도 진동 범위 : ± 0.02°

- 최대 제어 회전 속도 : 팬 축: 90°/초 | 틸트 축 : 100°/초 | 롤 축: 30° /초

- 기계 엔드 포인트 범위 : 팬 축 컨트롤: 360° | 틸트 축 컨트롤: 위 45° 에서 아래 120° | 롤 축 컨트롤: ± 25°

- 작동 전류 : 정적 전류: 300mA (@16V) | 동적 전류: 600mA (@16V) | 잠금 로터 전류: 최대 10A (@16V)

- 작동 온도 : -15°C ~ 50°C (5°F ~ 120°F)

- 무게 : 4.20kg (9.26lbs) 핸들바 포함 완전 장착시

- 짐벌 치수 : 620mm(가로) x 280-380mm(세로) x 500mm(높이)

- 지원 카메라 치수 : 카메라베이스 플레이트에 질량 중심에서 최대 깊이 : 140mm | 카메라베이스 플레이트의 상단에서 측정된 최대 높이 : 225mm | 최대 길이: 195mm

□ 스테디캠(액션캠) / 1set

가. 기능 및 요건

- 360도 파노라마 영상촬영

- 손쉬운 세팅 및 효과적 스테디 기능탑재

- 모바일과 기기 간 연동지원, 모바일기기에서 원격 세팅 등

- 4k 화질 지원

- 추가 정품 베터리 1개

* 아래 사양과 동급 혹은 상위 사양이어야 한다.

나. 사양

- Dji 오즈모 (OSMO)

- 카메라 : 1/2.3인치 1200만 화소, 35mm 환산 20mm F2.8 조리개 단초점 렌즈마이크로 SD 메모리 슬롯, USB 단자

- 무게 : 핸들 201g, 짐벌 221g

- 기타 : 화각 - 94도, ISO - 100~3200(비디오), 100~1600(사진), 셔터스피트 - 8s~1/8000s(M 모드시 30s가지 지원), 스로우 모션 모드와 셀카 촬영 모드, 타임 랩스 기능 지원

- 전용 앱을 통한 원거리 조정

□ 기타 악세사리

가. 기능 및 요건

- UV 차단용 필터 / 1ea

- dslr 상시 유지보수용 청소도구 / 10ea

- 삼각대 다리가 변형가능 한 스파이더 포드 / 4ea

* 아래 사양과 동급 혹은 상위 사양이어야 한다.

나. 사양

- 겐코 52mm Air MC UV 필터

- 3M 참올 소형 극세사 클리너 16x18Cm, 안티포그 스프레이, 에어블로워, 브러시, 면봉 등

- 호루스벤누 SM-836

6. 납품 및 설치

□ 장비의 납품·설치 결과가 요구서에서 요구되는 성능·규격을 수용할 수 없다고 판단될 때 시공자 및 납품자에게 설치 변경을 요구할 수 있으며 규격의 누락 또는 기준 미달의 경우 계약해지를 할 수 있음

□ 장비의 설치 중 기기의 손상될 우려가 있을 때 필요한 방지책을 강구하여야 하며 피해 발생 시 제작자의 부담으로 조치 및 복구 하여야 함

□ 시공자 및 납품자는 납품장비 설치 전 계약발주자의 승인을 받아야 하며 납품장비는 명시된 규격을 준수하여야 하고 파손이나 시험운영 중 장애가 발생하였을 경우 동일규격 이상의 제품으로 교체 함

□ 설치과정 중 발생하는 모든 결함은 전적으로 시공자 및 납품자의 책임이며 최단시간내에 복구 조치하고 제품의 불량으로 설치가 불가능할 경우 빠른 시간 내에 신제품으로 교체하여야 함

7. 하자보증

□ 시공자 및 납품자는 천재지변이나 자연 사고를 제외한 시공 및 납품과정의 하자나 부품결함에 의한 하자에 대해서는 납품일로부터 2년간 무상 보증하여야 함

□ 무상하자 보증기간 중 장비에 하자가 발견될 경우 제작자는 해당 장비를 무상으로 수리하거나 동일 이상의 제품으로 교환해야 함

8. 교육 및 기술지원 사항

□ 시공자 및 납품자는 장비의 운용방법에 대한 기초교육실시 및 설명서를 함께 납품하여야 함

□ 시공자 및 납품자는 사업 수행 중이나, 완료 이후에도 관련분야 지식정보 등 지속적인 정보제공 여부에 관한 내용을 제시하여야 함

9. 기타사항

□ 시공 및 납품과정에서 사양변경 사항발생 시 상호 협의 후 조정해야 함

□ 본 과업지시서에 명시되지 않은 사항이라도 장비 시공‧납품과정 및 완료 후 기존 설비의 기능과 성능이 지장이 없도록 하여야 함

□ 시공 및 납품완료 후 장비 테스트 및 안전성에 이상이 없는지 검수

□ 납품 장소는 수요자가 지정한 장소로 해야 함

Ⅲ	과업진행 준수사항

□ 수행기업은 노후장비교체지원사업 운영 시 시공‧납품자 및 유‧무형의 자산에 대한 안전사고가 발생하지 않도록 안전관리에 만전을 기하여야 함

- 시공 및 납품 관련 발생하는 모든 법률적 책임은 수행 기업에 있음(물적‧인적사고, 안전사고 등으로 인한 손배상 포함)

- 시공 및 납품 관련 기준은 발주처가 제시하는 가이드라인(규제기준)에 부합하여야 함

□ 수행기업은 과업을 수행함에 있어 발주처의 명예가 훼손 될 수 있는

일체의 행위를 하지 말아야 함

□ 수행기업은 과업내용 및 예산을 숙지한 후 진행하여야 하며, 진행의

각 단계별로 발주처 사업담당자와 협의 후 진행하여야 함

□ 과업진행과정에서 발주처가 과업의 범위 및 내용을 변경 요청할 경우

요청 시기와 상관없이 과업 추진일정 및 예산에 차질이 없는 한

성실히 반영하여야 함

□ 수행기업의 과제책임자는 충분한 전문지식과 경험 및 자격을 갖추어야

하며, 발주처 사업담당자가 과업의 적정한 수행을 위하여 부적격 하다고

판단할 경우에는 교체를 요구할 수 있으며, 수행기업은 이에 응하여야 함

□ 제3자의 저작권 도용, 초상권 침해 등 제작 시 타인의 지적재산권을

침해함에 따른 분쟁은 그 시기에 관계없이 수행기업이 책임져야 함

□ 수행기업은 본 과업수행 과정에서 알게 된 모든 사항에 대하여 제3자

에게 누설․전달하여서는 아니 됨

□ 성과물에 대한 지적재산권 등 모든 권리는 발주차가 소유함

□ 모든 과업은 본 과업지시서에 의하여 수행하며, 이에 규정되지 아니한

사항은 관계법령 및 정부가 정한 각종 기준과 연계 검토 후 발주처와

협의 하에 수행

Ⅳ	과업수행 절차

□ 착수보고 : 계약일로부터 3일 이내

- 제출서류 : 시공‧납품장비 목록, 착수신고서, 책임자선임계, 기타 발주처 착수관련 요청서류(별도안내)

□ 총 19종 시공 및 납품 장비에 대한 설치(수정 및 보완포함) 및 검수

□ 결과보고 : 준공일 3일 전

- 제출서류 : 결과보고서 1부(사진포함), 발주처 요청서류

Ⅴ	준공 및 준공금 청구

□ 결과물 납품

- 납품방법 : 발주처 지정장소에 준공일에 맞춰 과업지시서 내용을 모두 완료(설치)하여 납품

- 납품 전 반드시 발주처 담당자 입회하에 각종 현장 시험가동을 실시

하여 정상 작동여부 확인 후 결과에 문제가 없어야 하며, 시험가동 시

발견되는 오류나 문제점, 시스템 보완 요구 등에 대해서는 즉시 조치 후 납품

(최종 검수 결과, 장비운영이 불가하다고 판단되거나 기기의 하자 발생으로 계약조건을

이행하지 못하는 것으로 판단될 시 수행기업은 모든 장비를 철거 및 회수해야 하며

그 비용은 수행기업이 부담하고, 이 경우 계약을 해지 할 수 있음)

□ 준공 결과보고서 제출

- 제출기한 : 준공일

- 제출서류 : 진흥원 요청 서류(별도 안내), 결과보고서 1부(설치 사진 등),

설치 제품별 상세 사양서 1부 등

□ 준공금 청구

- 과업지시서 및 각종 관계법령에 따라 준공 검수를 진행하며 검수

완료 후 준공금 청구 및 지급을 원칙으로 함

Ⅵ	계약의 해지

□ 다음의 각 항목에 해당하는 경우, 본 계약의 전부 또는 일부를 해지 할 수 있다.

○ 정당한 사유 없이 약정한 착수 기일을 경과하고도 착수하지 아니할 경우

○ 과업지시서에 명시한 계약기간 내에 세부행사 집행계획에 의한 일정에 따라 완료되지 못하거나, 수행기업의 귀책사유로 과업완료할 가능성이 명백히 없다고 인정되는 경우

○ 계약내용과 실제 과업을 다르게 수행할 경우

○ 발주처의 사전 승인 없이 과업내용을 임의로 변경하는 경우

○ 과업수행과정에서 발주처의 정당한 요구를 이행하지 않을 경우

- 상기 사항에 해당할 경우 발주처는 수행기업에 과업중단 지시, 기 지급된 대금의 환수, 손해배상 등을 요구할 수 있으며, 수행기업은 발주처의 처리에 성실히 응하여야 함

Ⅶ	그 외 준수사항

□ 지방자치단체를 당사자로 하는 계약에 관한 법률 일체

□ 지방자치단체 입찰 및 계약 집행기준(행정자치부 예규 제27호)