충남콘텐츠기업 육성센터 장비 구축

과업지시서

2019. 2.

Ⅰ		일반시방

1. 일반 시방

가. 시방의 목적

본 시방은 충남콘텐츠기업 육성센터 장비 구축에 있어서, 구축 소기의 목적과 기능을 달성하기 위해 필요한 영역별 사업을 계약자가 원활히 수행하여 사업 전반에 걸쳐 효율적으로 시스템 구축 작업을 위해 필요한 일반적인 사항을 규정하고자 한다.

나. 계약당사자

“갑”  발주처

“을”  시스템 구축 계약 업체

다. 적용법령 및 기준

본 시방 및 규격서에 정한 사항이 관계 법령과 다른 부분이 있을 경우에는 관계법령을 우선으로 준수 시공한다.

라. 제출서류

1) 계약자는 계약 후 7일 이내에 현장조사를 실시하여 착수 신고서를 감독자에게 제출하고 승인을 받은 후 사업 수행을 할 수 있다.

○ 착수 시 제출 서류

(1)착수계

(2)사업 책임자 선임계(이력서, 기술자면허수첩사본 첨부)

(3)기타 감독관이 지정하는 필요한 서류

2) 계약자는 준공 검사시 다음 서류를 첨부하여야 한다.

○ 준공 검사시 제출 서류

(1)준공계

(2)시스템 구성 내역서

(3)실별 시스템 구성도

(4)시스템 사진 대지

(5)AS 유지보수 연락망

(6)기타 감독관이 지정하는 필요한 서류

마. 계약이행

1) 납품장비의 내역이 발주처의 의견과 상이 할 경우 제안내용과 관계없이 계약자는 발주처의 변경 지시를 따라야 한다.

2) 기술규격서상의 불합리한 점이나 문구, 용어해석에 대하여 발주기관과 의견을 달리할 경우에는 발주기관의 해석 및 지시에 따라야 한다.

3) 사업 수행 시 실제 구축내역과 시방서의 내용이 서로 상이하거나 작업 시 누락, 오기 되었다고 판단되는 경우 또는 작업 시 공정상에 의문이 있을 경우에는 감독자에게 질의하여 감독자의 지시에 따라 원활히 처리한다.

4) 계약자는 구성도 및 시방서에 명시되지 않은 사항일지라도 구축 및 구조상, 외관상, 시스템 구성상 필요한 사항은 감독자의 지시에 따라야 한다.

5) 사업 수행 시 구축에 수반되는 모든 부대비용은 계약자의 부담으로 한다.

바. 감독자

1) 본 시방서에서 감독자라 함은 발주처가 지명한 감독관 또는 그 대리인, 그가 쓰는 현장원을 말한다.

2) 시공자의 현장대리인에 대한 감독자의 지시 승인 또는 검사는 모두 감독자의 권한과 책임으로 간주한다. 이때 감독자의 지시 및 결정의 중요한 사항은 문서로 하여 감독자의 승인을 받는다.

사. 기술교육 실시

1) 본 공사 계약자는 설치한 시스템의 원활한 운영을 위하여 운용자들에 대하여 기술교육을 실시하여야 하고, 활용 메뉴얼을 제공하여야 함

- 교육 내용 : 시스템의 동작개요, 기능, 운영방법의 이해, 유지보수에 필요한 모든 운영 시스템, 시스템 소프트웨어와 하드웨어 구성, 시스템 백업, 기능복구 및 고장 복구과정, 구성 불일치, 사용자 에러에 대한 처리방법 및 사용자 관리 부분 등

2) 납품하는 장비의 원활한 운영과 보수 유지를 위하여 특별히 명시하지 않더라도 장비 설명서를 반드시 첨부하여 납품하여야 함.

3) 시스템 교육에 대한 책임은 계약자 주관 하에 실시함을 원칙으로 하며, 시스템 교육 계획과 절차는 해당 “을”이 준비하며 제반비용은 “을” 부담으로 한다.

아. 최종 검사 및 시험운전

1) 수급자는 설치 완료 후 최종 검사와 시험운영을 하여 발주처의 승인을 득해야  한다.

2) 수급자는 시험검사 항목을 작성, 제출하여 감독원의 승인을 받아야 한다.

각 설치 별 공동검사 및 시험 항목은 다음과 같다.

1. 외관 및 구조 검사

2. 배선 상태 검사

3. 성능 시험

4. 시운전 검사

5. 준공 검사

※ 검수 시 시방에 의한 측정 테스트 보고서와 장비의 설정값을 제출하여야 한다.

3) 검사 중 시방서 및 설계도서와 상이하게 설치한 사항이 발견된 경우 감리원의 지시에 따라 수급자 부담으로 재시공하여야 한다.

II		특별시방

1. 특별 시방

가. 시방의 목적

본 시방은 충남콘텐츠기업 육성센터의 장비를 구축함에 있어서 효율적 구축 및 향후 운영 효율성을 위한 제반 설비로써 기기의 구성 및 운영에 있어서의 전문성과 편의성을 최대한 보장하고 시스템의 안정성, 효율성, 연계성 등을 고려하여 시스템을 구축하는데 함에 있어서 계약자가 지켜야 할 특별한 사항을 규정하고자 한다.

나. 적용 범위

1) 본 특기 시방서는 충남콘텐츠기업 육성센터 장비 구축을 납품 설치함에 있어 일반시방서에 명시되지 않은 부분에 대하여 계약업체가 수행해야 할 제반 세부사항을 규정한다.

2) 본 특기 시방서는 시스템에 대한 최소요구사항이며, 본 시방서 상에 명시되지 않은 사항에 대해서도 장비 및 시스템 운영에 문제가 없도록 납품 설치되어야 한다.

다. 시스템 필수사항

1) 계약자는 반드시 본 사업의 목적과 취지를 파악하고 목적 달성을 위한 최적의 시스템을 구축하되 각 기기의 고유 성능을 최대한 발휘할 수 있도록 구성하여야 하며, 전체 시스템으로서의 호환, 연계 사용에 대한 고려를 하여야 한다.

2) 특별히 명기되지 않더라도 모든 장비는 설치 및 시험, 운영 교육을 포함하며 이를 위한 자재, 교보재를 포함한 비용은 계약자의 부담으로 한다.

3) 납품되는 운용 SW 는 유지관리의 용이를 위하여 반드시 저작권 문제가 없는 정식 인가된 제품으로 납품하여야 한다.

4) 납품되는 디스플레이의 경우 향후 유지보수 운영의 용이성을 위해 가급적 동일 제조사 제품으로 구성하도록 한다.

5) 영상스튜디오 및 PT, 상영관의 장비는 향후 운영 커리큘럼과 연관 있으므로 장비의 구성, 설치가 매우 중요하므로 기종, 구성의 변경에 신중하여야 하고 서면으로 승인 받아야 한다.

6) 모든 장비는 각 실별 구성이 중요하므로 납품시 실별 구성안을 제시하여 승인 받은 후 설치하도록 한다.

7) 계약자는 장비의 설치 납품을 위해 꼭 필요한 건축, 전기, 통신, 실내건축 영역의 작업을 위해서 관련 업체와의 협의 및 조언에 충실하여야 하고 필요시 관련 도면을 제공 하여야 한다.

8) 수입품일 경우 정식 국내 법인을 통해 정식 수입된 제품이어야 하며, 정품공급확약서 및 기술지원확약이 가능한 제품이어야 한다.(공식 A/S센터에서 기술지원 제품)

특히, 기술규격서에 별도로 명기된 장비의 경우 수입자 정품 공급증명원 및 A/S 지원확약서를 첨부하여야 한다.

9) 납품하는 장비 및 시스템에 대하여 하자담보책임기간은 사업 종료일로부터 1년으로 하되 이 기간 중 발생하는 하자에 대해 최단 기간 안에 조치가 완료되어야 하며 장비 개별적인 유지보수가 아닌 일괄적인 유지보수를 하여야 한다.

10) 단 제조사 또는 공급사가 보증하는 무상하자보수기간이 1년 이상일 경우, 제조사   또는 공급사가 보증하는 무상하자보수 기간을 하자담보 책임기간으로 한다.

2. 설치 시방

1) PT, 상영관

- PT, 상영관은 21 x 3m의 써클스크린에 3대의 레이져프로젝트를 사용하여 멀티영상을 투영하도록 하되, 화면 동기 솔루션을 활용하여 최소 6개의 입력 신호를 선택하여 1,2,3 또는 1,2 또는 전체를 하나의 화면으로 합쳐서 투사 할 수 있도록 구성한다.

- 써클스크린의 경우 철제프레임을 세운 후 지정 된 R 값 만큼 휘어서 설치하되 영상 투사면을 합판 또는 유공스크린으로 구성 할 경우 오디오 시스템의 구성에 대한 기술적인 해결방안을 제시하여야 한다.

- 각 스크린 중심부의 밝기는 14ftL~16ftL (2.39, 1.85/Side.Top Screen Type 동일) 색온도는 6300K캘빈(2.39, 1.85/Side.Top Screen Type 동일)이 객석 중심에서 나와야 한다.

- 스크린 밝기의 균일성은 스크린 주변부가 스크린 중심부 수치의 70~85%(2.39와 1.85 동일)가 객석 중심에서 나와야 한다.

- 영사각, 시야각, 경사도, 스크린에 위치와 관련되어 관객의 움직임이나 이동에 의한 영상의 간섭이 일어나지 않도록 최대한 주의하여 설치되어야 한다.

- 화면비율 1.78 : 1과 1.85 : 1 및 2.39 : 1을 모두 수용하여야 한다.

- 선명한 화질과 명료한 음질을 위하여 시스템 전원 인입은 반드시 조명, 발전, 동력전원과 분리되어 시설 운영해야 한다.

- 무빙 라이트 및 콘트롤러를 사용하여 발표자를 핀 스폿 할수 있도록 한다.

- ＨＵＭ(잡음) 노이즈 및 감전 예방을 위하여 장비는 접지하도록 한다.

2) 영상스튜디오

- 카메라, 스위쳐 등의 부대장비의 결선시에는 케이블 등을 최대한 숨기고 외관을 미려하게 한다.

- 장비 설치시에는 동선을 고려하여 설치한다.

- 카메라와 크로마키스크린을 활용한 영상 체험 스튜디오가 운영 될수 있도록 구성, 설치하고 필요시 기술 지원을 하여야 한다.

- 조정실과 스튜디오장비의 결선을 위한 월패널을 구성하여 다양한 활용이 가능하도록 구성한다.

- 스튜디오에는 영상 촬영용 특수 조명을 그리드 방식으로 설치하여 동영상 촬영시 활용 가능하도록 한다.

3) 미디어 월

- 관련 법령 및 규정에 적합하도록 설치한다.

- 승인도서를 제출하여야 한다.

- 설계 및 제작설치에 대한 모든 사항은 현장 상황을 면밀히 검토 후 발주처        및 감독관의 사전 승인을 득한 후 제작설치에 임하여야 한다.

- SYSTEM의 구성은 장애로 인한 경기 진행의 차질이 발생치 않도록 충분히 검토   되어야하며 구조적 안정성을 확보하여야 한다.

- 제작 설치에 사용되는 모든 자재는 KS 또는 CCC 규격품을 사용하여야 하며      규격품이 없을 경우에는 시중의 최상품을 사용하여야 한다. 단 자재의 사용은      사전에 발주처 및 감독관의 승인을 득하여야 하며 자재에 대한 시험성적서 등의 자료 요구에 대하여는 이에 응하여야 한다.

- 본 제작시방 항목 외 현장 시공 시 보완 요청되는 사항에 대해서는 특별한 사유가  없는 한 이에 응하며, 협의사항이 발생시는 발주처 및 감독관과 협의 하여야 한다.

- 미디어 월의 구조물 설치는 건축구조물의 안전성 확보를 위해 발주처와 사전 협의하여 철 구조물을 설치하여야 한다.

- 실시 설계에 의한 미디어 월 철 구조물 변경 시 건축 구조물의 안전성 및 지역 특성을 고려하여 구조안전진단을 받은 후 구조 계산에 의거하여 철 구조물을 설치하여야 한다.

- 미디어 월이 내부에 설치되는 특성을 감안하여 일정 온도유지를 위해 통풍구를 설비하고 먼지 등의 유입이 발생치 않도록 하여야 한다.

- 미디어 월 내부에 장착되는 각종 장치의 탈부착이 용이 하도록 하고 외부의 압력에 의해 장치가 탈락이 발생치 않도록 제작 하여야 한다.

- 천재지변이 아닌 어떠한 경우라도 무너지거나 넘어지는 일이 없어야 하며, 구조물  의 외형에 따른 부착장치의 탈락이 발생치 않도록 하여야 한다.

- 표출면의 좌,우에 A/S가 가능한 충분한 공간을 확보할 수 있도록 시설물을 배치   하여야 하며, 내부 작업이 가능하도록 조명기구를 설치하여야 한다.

- 철 구조물의 내 외부는 지정 색 으로 도장하여 부식이 발생치 않도록 하여야 한다.

- 기기 설치미디어 월 내부의 각종장치는 스프링 와셔를 삽입하여 진동에 의한 풀림이 없도록 하여야 한다.

- 철 구조물은 수평 및 수직을 정확하게 맞추어 설치하여 미디어 월에 외곡이 발생하지 않도록 설치하여야 한다.

- 계약자는 발주처와 협의에 의하여 미디어 월의 1분~1분 30초 분량의 인트로 영상을 제공할 수 있도록 한다.

4) 회의시스템

- 각 실의 회의시스템은 사용이 편라하도록 입력단자를 연장하는 월패널을 시공하여 PC 등의 소스기기 연결이 용이하도록한다.

- 무선 컨퍼런스 장비를 사용하되 필요시 각 실을 이동 사용하도록 구성한다.

- 프로젝터 및 디스플레이 장비는 사용자 시야각에 맞추어 설치한다.

5) 배관 배선

- 배선은 전기설비기술기준, 내선규정 등을 준수하여 설계도면 및 규격시방서에 의거하여 작업되어야 한다.

- 배선은 충분한 용량의 절연특성이 우수한 전선을 사용하여 기기간의 동작에 영향을 주지 않도록 규격에 맞는 우수품질을 가진 제품으로 제작되어야 한다.

- 전광판 내부의 배선은 접촉에 의한 사고를 예방할 수 있도록 덕트를 이용하여 최대한 은폐시켜 결선하여 외관상 미려하도록 하고 노출로부터의 사고를 방지하여야 한다.

- 케이블 분기 또는 접속은 분전반, 또는 접속함 안에서 하도록 설계 제작되어야 한다.

- 배선의 분기는 반드시 단자대에서 처리하고 단자접속 시 단선, 접촉 불량, 합선 등이 생기지 않도록 하여야 한다.

- 배선의 단말에는 적합한 터미널을 사용하여야 하며, 점검이 용이하도록 마크밴드 또는 튜브를 사용하여 점검이 용이하도록 조립되어야 한다.

- 단자대에는 투명한 합성수지판으로 된 탈착이 용이한 구조의 덮개를 덮도록 하여 안전에 대비할 수 있도록 하여야 한다.

- 각 단자대에는 번호 또는 기호를 기입하여 배선의 구분이 용이하도록 하여야 하며 A/S시 신속히 대처할 수 있도록 하여야 한다.

6) 기타

- 과업안내서의 내용 중 해석의 차이가 있을 시는 진흥원의 해석을 우선으로 한다.

- 본 과업 안내서에 포함되지 않은 사항에 대하여는 진흥원에게 별도의 사양서는 제출하여야 한다.

- 본 과업안내서의 내용을 수정할 필요가 있는 경우 별도의 합의서를 작성할 수 있다. 다만 진흥원의 추가비용이 없어야 하며 규격을 상향으로 하여야 한다.

- 사업자는 면허, 특허권, 의장권, 공업 소유권 및 지적 소유권의 침해로 인한 모든 문제와 소송에 대하여 사업자의 부담으로 하여야 하며 진흥원은 전적으로 면책권을 갖는다.

- 본 과업안내서 및 도입조건에 명시된 사항은 최소한의 사항, 내역만을 규정하였으므로 상세히 기술되지 않았거나 누락된 사항에 대하여 사업자는 시스템구축 운영상 하자가 발생되지 않도록 사전 조치하여야 하며, 본 과업안내서에 명시되지 않은 사항은 관계법령과 진흥원의 해석에 따른다.

- 본 과업안내서에서 정하는 것을 제외하고는 지방자치단체를 당사자로 하는 계약에 관한 법령, 조달관련규정에 의하여 당사자 협의하여 결정하며, 본 과업안내서에 관한 소송 관할 법원은 진흥원의 주소지를 관할하는 법원으로 한다.

III		구성 내역

No.	Description	Q'ty	Unit	Remark
	A. 지하층
	1). 서클 상영 시스템
1	레이져 DLP 프로젝터	3	set
2	씰링 브라켓	3	ea
3	Data Transmitter	3	ea
4	멀티비젼 서버 및 소프트웨어 시스템
4-1	Media Server	1	set
4-2	Live Input Card	1	ea
4-3	Video Matrix	1	ea
5	오디오 프로세서	1	ea
6	메인스피커(L, R)	2	ea
	- 메인스피커(C)	1	ea
7	서브우퍼스피커	1	ea
8	서라운드 스피커	6	ea
9	서라운드 스피커 브라켓	6	ea
10	스테이지 모니터 스피커	3	ea
11	파워앰프(Main Low)	4	ea
12	파워앰프(Main Low)	2	ea
13	무선 마이크	6	ea
14	Audio Mixer	1	ea
15	Power Distributor	2	ea
16	장비 랙	1	ea
17	설치 및 조정비	1	ea
18	카메라	2	ea
19	브라켓	2	ea
20	카메라 컨트롤러	1	ea
21	Moving Spot Light	3	ea
22	Controller	1	ea
	2). 스튜디오 영상 음향시스템
1	ENG HD Camcoder	1	ea
2	Camera Tripod	1	set
3	Dolly	1	ea
4	Studio Monitor Speaker	1	ea
5	Announcer Monitor	1	ea
6	이동용 TV 랙	1	ea
	Control Room Systems
1	Video Switcher	1	ea
2	PGM Display	1	ea
3	SSD Reader/Writer	1	ea
4	SD Card	2	ea
5	Audio Mixer	1	ea
6	P.D.U	1	ea
7	On-Air ON/OFF Display	2	ea
8	Control Desk	1	set
9	Wal Panel	1	ea
	이미지 촬영시스템
1	DSLR Camera	1	ea
2	Lens	1	ea
3	UV Filter	1	ea
4	SDHC Memory Card 128GB	2	ea
5	Battery	2	ea
6	샷건마이크	1	ea
7	Tripod	1	ea
8	카메라 가방	1	ea
9	스트로보	2	ea
10	소프트박스	2	ea
11	A Stand	2	ea
12	Boom Stand	1	ea
13	무선동조기	1	ea
14	전동 롤배경지	1	ea
	3). 스튜디오 특수조명
1	No. 1~4 Light Fly Duct	4	ea
2	LED Flux Light	9	set
3	LED Flux Light	2	set
4	Barndoor	2	set
5	Light Hanger	13	ea
6	Sagety Chain	13	ea
7	Roll Cromakey Screen	1	ea
8	RD Unit Panel	1	set
9	Light Control Board	1	set
10	Piping & Wiring	1	set
11	잡자재비	1	set
	B. 1층
1	안내 데스크 Display	1	ea
2	엘리베이터 사이니지	1	ea
3	멀티비젼	4	ea
4	북카페 Display	1	ea
5	무선 마이크	6	ea
6	스피커	8	ea
7	Power Amp	1	ea
8	Power Distributor	2	ea
9	장비 랙	1	ea
	C. 2층
	1). 경영기획실
1	LCD Display	1	set
2	벽걸이 브라켓	1	ea
3	설치비	1	lot
	2). 소회의실
1	LCD Display	1	ea
2	벽걸이 브라켓	1	ea
3	월패널	1	ea
	3). 중회의실-16인
1	LCD Display	1	set
2	벽걸이 브라켓	1	ea
3	월패널	1	ea
	D. 3층
	1). 회의실-8인
1	디스플레이	1	set
2	벽걸이 브라켓	1	ea
3	월패널	1	ea
	2). 출입구 - DID	1	set
	E. 4층
	1). 회의실-8인
1	디스플레이	1	set
2	벽걸이 브라켓	1	ea
3	월패널	1	ea
	2). 출입구 - DID	1	set
	F. 5층
	1). 회의실-28인
	A. 프로젝터
1	프로젝터	1	set
2	프로젝터 리프트	1	ea
3	전동스크린	1	ea
4	월패널	1	ea
5	앰프	1	ea
6	무선 마이크	2	ea
7	스피커	6	ea
8	Power Distributor	2	ea
9	장비 랙	1	ea
	B. LCD Display
1	LCD Display	1	set
2	벽걸이 브라켓	1	ea
3	월패널	1	ea
	C. Conference System
1	메인컨트롤러	1	ea
2	구즈넥마이크(의장용)	1	ea
3	구즈넥마이크	11	ea
4	배터리팩	12	ea
5	배터리 충전기	1	ea
6	안테나	1	ea
7	케이블	1	ea

IV		장비 규격서

※ 각 장비는 동등 규격 이상의 제품으로 제안, 납품해야 함

A. 지하층

1). 서클 상영 시스템

❍ 레이져 DLP 프로젝터

• Display System : 1-Chip 0.67" DLP

• Native Chip Resolution : 1920 x 1200 (WUXGA)

• Max Brightness : 10,000 Lumens

• Light Source : Laser diodes

• Aspect Ratio : 16:10

• Contrast Ratio : 20000:1

• Keystone Correction : Vertical: ± 40°, Horizontal: ± 15°

•  Inputs/Outputs :

- 1 x BNC(3G/HD/SDI) (Input)

- 1 x RGB(5xBNC) (Input)

- 1 x HDMI Audio/Video (Input)

- 1 x D-Sub HD 15-Pin (Input)

- 1 x DVI-D 24-pin

- 1 x D-Sub 9-pin (In/Out) Unspecified Signal (DE-9) Control (Output)

- 1 x M3 Control (Input)

- 1 x M3 Control (Output)

- 1 x Unspecified Signal (DE-9) Control (Input)

- 1 x Ethernet (RJ45) LAN (Input)

• AC Input Power : 240 VAC50 Hz

※. 옵션

• 줌렌즈 : 1 EA 포함

❍ 씰링 브라켓

가. 기능

천정에 프로젝터를 고정하기 위한 장치로 무거운 무게를 버티는 철판으로 절곡하여 제작한다.

나. 규격

• 색상 : 검정색

• 적합 프로젝터 : 대형프로젝터

• 각도조절 : 상하 5°, 좌우 5°

2x stereo [line]

• 최대 지지중량 : 80kg

• 강판 두께 : 5mm

• 형식 : 강판절곡

❍ Data Transmitter

가. 기능

HDBaseT Connectivity – extends an HDMI connection over a long distance via one Cat 5e/6/6a          cable.

나. 규격

• Video Input : Interface: 1 x HDMI Type A female (black), Impedance: 100 ohms, Maximum             Distance: 5.9' (1.8 m)

• Video Output : Interface: 1 x HDMI Type A female (black), Impedance: 100 ohms

• Video : Maximum Data Rate: 10.2 Gbps (3.4 Gbps per lane), Maximum Pixel Clock: 340 MHz,           Compliance: HDMI (3D, Deep Color, 4K) , HDCP compatible , Consumer Electronics Control             (CEC), Maximum Resolutions / Distance: Up to: 4K @ 115' (35 m) (Cat 5e/6) / 131' (40 m) (Cat         6a)

• 1080p @ 197' (60 m) (Cat 5e/6) / 230' (70m) (Cat 6a) 지원

• Audio : Input: 1 x HDMI Type A female (black), Output: 1 x HDMI Type A female (black)

• Power : Connector: 1 x DC jack / locking (black), Consumption: VE801T: DC5 V, 1.85 W,              VE801R: DC5 V, 4.23 W

• Housing : Metal

❍ 멀티비젼 서버 및 소프트웨어 시스템

가. 기능

프로젝터 멀티비젼의 프레임 락, 베젤메니지먼트, 타임코드 인덱싱 기능으로 디스플레이의 수량, 종류, 특성에 무관하게 동기화 된 스크린을 구현한다.

나. 규격

1. 프로덕션 서버

• 멀티 타임라인으로 멀티미디어 쇼 편성 및 재생 / 프로젝션 엣지블렌딩 및 왜곡보정 / 멀티             디스플레이 동기화 / SMPTE 타임코드 재생 / 다양한 프로토콜을 이용한 인터렉티브 연출              기능을 제공한다.

• 메인 프로세서 : 8-core 3.0Ghz 16-thread

• 메인 메모리 :DDR4 16GB

• 스토리지 : 1 * SATA3 250GB (read 550MB/s, write 480MB/s), 1 * PCIE3.0x4 250GB (read               3000MB/s, write 1500MB/s)

• 네트워크 : 1 * GBIC

• 지원 코덱 : MPEG2, WMV HD, H.264/AVC, HAP, HAPQ, ProRes

• 제어신호 출력 : TCP, UDP, Artnet, DMX-512, SMPTE, RS-232, Generic protocol

• 제어신호 입력 : TCP, UDP, MIDI, MSC, Artnet, DMX-512, SMPTE, RS-232, Generic protocol

2. 디스플레이 서버

• 미디어 파일을 디코딩하고 동기화된 비디오 및 오디오 신호를 출력한다.

• 메인 프로세서 : 8-core 3.0Ghz 16-thread

• 메인 메모리 :DDR4 16GB

• 스토리지 : 1 * SATA3 250GB (read 550MB/s, write 480MB/s), 1* PCIE3.0x4 500GB (read 3400MB/s, write 2300MB/s)

• 네트워크 : 1 * GBIC

• 비디오 출력 : 4 * DisplayPort 1.4 or DVI

• 비디오 동기 : External Framelock (option)

3. Gigabit Ethernet 스위치

• 기가비트 Full Duplex 속도로 ethernet 스위칭을 제공한다.

• 네트워크 프로토콜 : IEEE 802.3 10BASE-T Ethernet, IEEE 802.3u 100BASE-TX Fast Ethernet

IEEE 802.3ab 1000BASE-T Gigabit Ethernet, IEEE 802.3x full-duplex flow control

• 스위칭 용량 : 48Gbps

• 인터페이스 : 24 * RJ-45 connectors, 2 * SFP slots for fiber Gigabit Ethernet modules

4. Live Input Card

• The stand alone PCI Express x4 plug in capture card delivers extreme performance with   650MB/s transfer bus bandwidth providing a further  improvement to the 480MB/s of the   VisionRGB-E2.

• This video capture has two complete capture   channels supporting up to 1920×1200 HD-SDI Analog resolution.

5. Video Matrix 스위치

• 비디오 8채널 입력 및 8채널 출력에 대하여 매트릭스 스위칭을 제공한다.

• 제어 : EDID Management for each in and out channel, HDCP Emulation for each in channel

RS-232 channel control, TCP channel control

• 출력 단자 : 8 * HDMI type A female

• 입력 단자 : 8 * HDMI type A female

6. 프로덕션 SW

• 화면 영역에 관한 사용자 인터페이스 : 영상 연출 영역을 직관적으로 확인할 수 있도록 영상 및

음향 컨텐츠를 화면 영역에 배치하여 실시간으로 표현하는 WYSIWYG(What You See Is What

You Get)형식이어야 한다.

• 컨텐츠 확인에 관한 사용자 인터페이스 : 편성 가용한 비디오, 오디오, 스틸이미지, 플래쉬              무비등과 같은 미디어파일의 재생시간, 해상도, 경로, 썸네일을 일목요연하게 볼 수 있어야 한다.

• 컨텐츠 편성에 관한 사용자 인터페이스 : 다수의 관람객/체험객에 동시 대응하는 인터렉티브            연출을 구현하기 위해 50개 이상의 타임라인을 동시에 사용할 수 있어야 하며, 관람객에               대응하는 영상 오브젝트를 화려하게 연출하기 위하여 각각의 타임라인은 500개 이상의 레이어를         동시에 사용할 수 있어야 한다.

• 인터렉티브 연출 가능한 미디어 오브젝트 : 센서, 터치 패널 등 외부 입력장치를 통해 비디오           오브젝트를 실시간으로 제어할 수 있어야 하며, 제어의 범위는 포지션 이동, 확대/축소, x/y/z축         회전, 투명도 조절, 칼라값 조절이어야 한다.

• 무인 통합 제어와 미디어서버의 동작 연속성을 보장하기 위해 운전중, 타임라인 포지션, 보조           타임라인 재생중 여부에 대한 모니터링 값을 제공할 수 있어야 한다.

• 각종 장치와 인터렉티브 연동 구성을 하기 위하여 다음과 같은 프로토콜을 출력할 수 있어야           한다. TCP, UDP, Artnet, DMX-512, SMPTE LTC, RS-232, RS-485

• 고화질/고화소의 영상연출을 하기위해 다음과 같은 코덱의 비디오 파일을 디코딩 할 수 있어야         한다. MPEG2, WMV HD, H.264/AVC, HAP, HAPQ, ProRes

• 고품질/다채널의 음향연출을 하기위해 다음과 같은 디지털 오디오 출력 기법을 사용할 수              있어야 한다. WASAPI, ASIO

• 고성능을 요구하는 미디어서버에 안정적인 전원을 공급하기 위해 정격 850W 이상의                   파워서플라이를 갖추어야 한다.

• 전파법 제 58조의2 제3항에 따른 방송통신기자재등의 적합등록을 필한 제품이어야 한다.

• 제품 제조사의 공식 공급처 인증을 획득하여 품질보증기간 만료 후에도 지속적인 사후 지원을          받을 수 있는 제품이어야 한다.

6. Display SW

• 최대해상도 1920x1200@60hz의 DisplayPort 영상신호를 동시에 4채널, 혹은 최대해상도

3840x2160@60hz의 DisplayPort 영상신호를 동시에 2채널까지 출력이 가능하여야 한다.

• 동기화된 영상 연출을 구현하기 위하여 각각의 출력 영상 채널은 Framelock을 통해 1/60초의

정밀도로 동기화 하여야 한다.

• 옵션으로서 최대해상도 1080p60 의 DVI 영상신호를 동시에 4채널까지, 혹은 2160p60 의

DisplayPort 영상신호를 동시에 2채널까지 입력 받을 수 있어야 한다.

• 영상 입력 인터페이스에는 각각 EDID값을 매핑하여 영상 소스측의 EDID 설정을 강제할 수

있어야 한다.

• 무인 통합 제어와 미디어서버의 동작 연속성을 보장하기 위해 마스터 서버와 통신 연결에 대한

모니터링 값을 제공할 수 있어야 한다.

• 각종 장치와 인터렉티브 연동 구성을 하기 위하여 다음과 같은 프로토콜을 입력받을 수 있어야

한다. TCP, UDP, MIDI, MSC, Artnet, DMX-512, SMPTE LTC, RS-232, RS-485

• 각종 장치와 인터렉티브 연동 구성을 하기 위하여 다음과 같은 프로토콜을 출력할 수 있어야

한다. TCP, UDP, Artnet, DMX-512, SMPTE LTC, RS-232, RS-485

• 고화질/고화소의 영상연출을 하기위해 다음과 같은 코덱의 비디오 파일을 디코딩 할 수 있어야

한다.  MPEG2, WMV HD, H.264/AVC, HAP, HAPQ, ProRes

• 고품질/다채널의 음향연출을 하기위해 WASAPI, ASIO와 같은 디지털 오디오 출력 기법을 사용할

수 있어야 한다.

• 고성능을 요구하는 미디어서버에 안정적인 전원을 공급하기 위해 정격 850W 이상의

전원공급장치를 갖추어야 한다.

• 전파법 제 58조의2 제3항에 따른 방송통신기자재등의 적합등록을 필한 제품이어야 한다.

• 제품 제조사의 공식 공급처 인증을 획득하여 품질보증기간 만료 후에도 지속적인 사후 지원을

받을 수 있는 제품이어야 한다.

❍ 오디오 프로세서

가. 기능

7.2채널 AV 리시버로 HDMI(입력 7개/출력 2개), HDR(High Dynamic Range), 돌비 비전(Dolby Vision), HLG(Hybrid Log-Gamma) 및 BT.2020 등 4K 울트라 HD 완벽지원, 향상된 음질, 고출력, 뛰어난 기능을 제공한다.

나. 규격

• Output Power

- 100 W per channel @ 8 Ohms, 20 Hz to 20 kHz, 0.06% THD, 2 channels driven

- 110 W per channel @ 8 Ohms, 1 kHz, 0.9% THD, 2 channels driven

- 160 W per channel @ 8 Ohms, 1 kHz, 10% THD, 1 channel driven (JEITA)

• Dynamic Power per Channel

- 130 W @ 8 Ohms (front L/R)

- 170 W @ 6 Ohms (front L/R)

- 195 W @ 4 Ohms (front L/R)

- 240 W @ 2 Ohms (front L/R)

• Channels	7.2

• Object-Based Audio Support	Dolby Atmos, DTS:X

• Audio Decoding :	Dolby TrueHD, Dolby Digital Plus, Dolby Surround, DTS-HD Master Audio

• Video

- Pass-Through	4K/60p (4:4:4), HDR10, Dolby Vision, HLG, BT.2020

- HDCP Version	HDCP 2.2 on all ports

• Bluetooth	Yes (SBC / AAC)

• Wi-Fi : Yes, dual-band (2.4 / 5 GHz)

• AirPlay :	Yes

• Inputs

- 7 x HDMI

- 2 x optical TOSLINK

- 2 x digital coaxial

- 1 x RCA component video

- 1 x RCA composite video

- 3 x stereo RCA audio

- 1 x stereo RCA audio (phono, with ground screw)

- 1 x 1/8" / 3.5 mm analog audio (front)

• Outputs

- 2 x HDMI

- 2 x subwoofer pre-out

- 1 x Zone 2 RCA pre-out

- 1 x 7-channel RCA pre-out

- 1 x 1/4" / 6.35 mm headphone (front)

• Speaker Connectors : 9 x binding post pairs

❍ 메인스피커(L, R)

가. 기능

Three-Way Triamplified ScreenArray® Cinema Loudspeaker System

나. 규격

• Frequency Range : 30 Hz - 20 kHz

• Frequency Response : 40 Hz - 19 kHz

• System Sensitivity : 103 dB, 2.83V @ 1m (3.3 ft)

• Rated Maxium SPL : 125 dB @ 1m (3.3 ft), 131 dB peak

• System Input Power Rating	LF: 600 watts, M/HF: 150 watts [HF: 85 watts]

• Hor. Coverage Angle : (-6 dB)	90°

• Vert. Coverage :  Angle (-6 dB)	20° up, 30° down

• Directivity Factor (Q) : 10.0

• Directivity Index (DI) : 10 dB

• Crossover Frequencies : 350 Hz [1.2 kHz]

❍ 메인스피커(C)

가. 기능

Full range 2 way high sensitivity, dual woofer passive system, compact and versatile specially designed for under balcony applications.

나. 규격

• 주파수 응답특성(-10dB)     	: 55 ~ 20,000Hz

• 주파수 응답특성(-3dB)     	: 95 ~ 20,000Hz

• Coverage angle(HxV)       	: (-6dB) 90°x60°

• DIRECTIVITY FACTOR; Q	: 9.25

• System 감도               	: 93dB, 1W@1m

• Max. SPL @ 1m             	: 125dB, @1m

• System nominal impedance       	: 8Ω

• 허용입력/최대출력          	: RMS 400w / PEAK 1,600w

• 권장 앰프 출력              	: 800w

• 보호회로                   	: Dynamic

• Crossover 주파수           	: 2.1kHz

• Compression driver         	: 1" driver with 1.5” voice coil

• Woofer                    	: 2 x 8” woofer with 2” voice coil

❍ 서브우퍼스피커

가. 기능

High quality subwoofer system, featuring an advanced technology 460 mm (18 in), low frequency transducers mounted in a direct radiator, bass-reflex enclosure for smooth response to the lowest audible frequencies.

나. 규격

• Rated Impedance	4 ohms

• Minimum Impedance	3.2 ohms

• Power Handling Capability	-

• Continuous Pink Noise	1200 Watts

• Continuous Program	2400 Watts

• Peak Power	4800 Watts

• Output Capability	-

• Axial Sensitivity

- 50 Hz to 500 Hz; 101 dB, 1W @ 1m

- 40 Hz to 100 Hz; 100 dB, 1W @ 1m

❍ 서라운드 스피커

가. 기능

Cinema Surround Speaker offers high power handling, high sensitivity, and extended bass response in a very compact enclosure.

나. 규격

• Frequency Range : (-10 dB)	50 Hz - 20 kHz

• Frequency Response : (±3 dB)	65 Hz - 18 kHz

• Power Rating :

- 150 watts continuous

- pink noise

- 600 watts peak

• Sensitivity (1W/1m) :

- 94 dB-SPL half-space / wall-mounted

- 91 dB-SPL free-field

• Maximum Peak SPL : 122 dB/1m

• Nominal Impedance : 8 ohms

• Hor. Coverage Angle (-6 dB) : 100° averaged 400 Hz to 12 kHz

• Vert. Coverage Angle (-6 dB) : 90° averaged 400 Hz to 12 kHz

• Directivity Factor (Q) : 7 averaged 400 Hz to 12 kHz

• Directivity Index (DI) : 8.4 dB averaged 400 Hz to 12 kHz

• Crossover Frequency : 3 kHz

• High Frequency Contour :	ISO2969 Curve X surround contour

• Polarity : EIA (Positive voltage to RED terminal gives forward cone motion)

• Low Freq Transducer Nominal : 200 mm (8 in)

• Diameter : 38 mm (1.5 in) voice coil

• High Freq Transducer Nominal : 25 mm (1 in)

• Diameter : 25 mm (1 in) voice coil

• Downward Firing Angle	Nominal 20° when mounted flush on back panel

※. 옵션

• 서라운드 스피커 브라켓 -- 6EA 포함

❍ 스테이지 모니터 스피커

• FREQUENCY RESPONSE (-10DB): 60 Hz ÷ 20000 Hz

• MAX SPL @ 1M:123 dB

• HORIZONTAL COVERAGE ANGLE: 90°

• VERTICAL COVERAGE ANGLE: 60°

• DIRECTIVITY INDEX Q: 10

• SYSTEM SENSITIVITY: 94 dB

• NOMINAL IMPEDANCE (OHM): 8 ohm

• POWER HANDLING: 200 W RMS

• PEAK POWER HANDLING: 800 W PEAK

• RECOMMENDED AMPLIFIER: 400 W

• PROTECTIONS: Bulb lamp dynamic

• CROSSOVER FREQUENCIES: 1400 Hz

• COMPRESSION DRIVER: 1.0'', 1.75'' v.c

• NOMINAL IMPEDANCE (OHM): 8 ohm

• INPUT POWER RATING: 100 W AES, 200 W PEAK

• SENSITIVITY (DB, 1W @ 1M): 108 dB, 1W @ 1m

• WOOFER: 6.0'', 1.7'' v.c

• NOMINAL IMPEDANCE (OHM): 8 ohm

• INPUT POWER RATING: 150 W AES, 300 W PEAK

• SENSITIVITY (DB, 1W @ 1M): 94 dB, 1W @ 1m

• Input/Output section  :  INPUT CONNECTORS-Speakon® NL4

❍ 파워앰프(Main Low)

• Type :power amplifier

• Subcategory :audio components

• Functions :amplifier

• Sound Output Mode :stereo

• Digital Sound Processor (DSP) :Yes

• Additional Features :DC offset protection, overload protection, short circuit protection, thermal protection

• Output Power (per channel) 650 Watt

• Output Power / Channel :1200 Watt, 1450 Watt, 2400 Watt, 3000 Watt, 650 Watt

• Output Impedance / Channel :2 Ohm, 4 Ohm, 8 Ohm

• Frequency Response :at 1 kHz

• Total Harmonic Distortion (THD) :0.5 %, 1.0 %

• Channel Type :bridged, main

• Channel Qty :1, 2

• Frequency Response :20 - 20000 Hz

• Signal-To-Noise Ratio :100 dB

❍ 파워앰프(Main Low)

• Type : power amplifier

• Subcategory : audio components

• Functions : amplifier

• Sound Output Mode : tereo

• Digital Sound Processor (DSP) : Yes

• Additional Features : DC offset protection, overload protection, short circuit protection, thermal          protection

• Output Power / Channel : 1000 Watt, 1600 Watt, 2000 Watt, 474 Watt, 800 Watt

• Output Impedance / Channel : 2 Ohm, 4 Ohm, 8 Ohm

• Frequency Response : at 1 kHz

• Total Harmonic Distortion (THD) : 0.5 %, 1.0 %

• Channel Type : bridged, main

• Channel Qty : 1, 2

• Frequency Response : 20 - 20000 Hz

• Signal-To-Noise Ratio : 100 dB

❍ 무선 마이크

• Modulation : Wideband FM

• Frequency Range	A: 548 to 572 MHz

• Switching Bandwidth : Up to 24 MHz

• Signal to Noise Ratio : ≥ 103 dBA

• Total Harmonic Distortion : ≤ 0.9%

• Temperature Range : Operation: 32 to 104°F (0 to +40°C)

• Storage : -4 to 158°F (-20 to 70°C)

• Transmitter Synchronization : 2.4 GHz, Low Power OQPSK (only active during synchronization)

• Principle	Double superheterodyne

• Diversity	Antenna switching diversity via internal antennas

• Sensitivity	< 3 μV at 52 dBA RMS S/N (at peak deviation)

• Frequency Response : 50 Hz to 16 kHz (-3 dB)

• Max Output Voltage : At Peak Deviation, 1 kHz AF 1/4" (6.3 mm) Jack Socket (unbalanced): +6         dBu XLR Socket (balanced): +12 dBu

• Adjustment Range	Audio: 45 dB, adjustable in 5-dB steps

• Squelch	Adjustable from 3 dB μV to 28 dB μV (combined with pilot tone)

• Line/Mic Level	20 dB, switchable

• Microphone

- Output Power	10 mW

- Frequency Response	80 Hz to 14 kHz

- Power Supply	2 x AA batteries, 1.5 V

- Operating Time	Approximately 10 hrs.

- Microphone Type	Dynamic

- Polar Pattern	Cardioid

- Input Sensitivity	Capsule: 1.5 mV/Pa

- Adjustment Range : Transmitter Sensitivity: 0 to -30 dB, adjustable in 10 dB steps

❍ Audio Mixer

• Phantom Power : +48 V switchable, channels 1 - 12

• Digital I/O

- USB Audio Class 2.0 compliant

- Sampling Frequency: max 192 kHz

- Bit Depth: 24-bit

• Input Channels

- 8x mono [mic/line]

- 2x mono/stereo [mic/line]

- 2x stereo [line]

• Output Channels

- 2x stereo out

- 1x monitor out

- 1x headphone out

- 4x aux out

- 4x group out

• Bus

- Stereo: 1

- AUX: 4

- GROUP: 4

• HPF : 80 Hz, 12 dB/oct (mono/stereo: MIC only)

• Compressor

- Threshold: +22 dBu to -8 dBu

- Ratio: 1:1 to 4:1

- Output level: 0 dB to 7 dB

- Attack time: approx. 25 msec

- Release time: approx. 300 msec

• Equalizer	EQ high gain: +15 dB/-15 dB, frequency: 10 kHz shelving

- EQ mid gain: +15 dB/-15 dB, frequency: mono 250 Hz - 5 kHz peaking, stereo 2.5 kHz                peaking

- EQ low gain: +15 dB/-15 dB, frequency: 100 Hz shelving

• Frequency Response : +0.5 dB/-1.5 dB (20 Hz to 48 kHz), refer to the nominal output level@ 1         kHz, GAIN knob: Min

• Residual Output Noise : -102 dBu (STEREO OUT, STEREO master fader: min

❍ Power Distributor

가. 기능

순차적으로 전원이 공급되며 역순으로 8 번부터 2 번까지 전원이 차단되는 기기

나. 규격

• AC Voltage meter : line input /output AC Voltage meter 를 내장하여 전압표시

• 채널수 : 8 채널

• 채널당 로딩 수 : 220V/10A,2200W

• 채널당 소비전력 : 10~15W

• Output connector : 한국표준 three wire AC connector

• 연속작동 사이의 시간간격 : 1 초

• 링크 : 가능

• 링크시 사용하는 케이블 : 4P DIN CABLE

• 파워스위치 , 램프 스위치 , 채널 on / off switch, Bypass 버튼

• 리모트 콘트롤러 SPRC 을 사용하여 원거리에서 콘트롤 가능 (20m 이내 )

• 램프 전압 : AC12V/400mA

• FAN 전압 : DC24V/1.5A( 상시전원 )

• 전압 : 220V / 50Hz-60Hz, 표준 3-wire 어쓰된 wire

❍ 장비 랙

가. 기능

EQ Rack is a durable, fifteen-space rack unit that is designed with vented side panels in order to promote airflow throughout the rack.

나. 규격

• 전면부 : 강화유리

• 측면판넬 : 착탈식

• 후면부 : 스틸도어

• 유닛(Unit) : 15U

• 고정타입 : 케이즈너트 타입

• 선반 : 1개

• 냉각팬 : 2개

❍ 카메라

가. 기능

Equipped with a 4.3 to 129mm zoom lens (35mm equivalent is 31.6 to 962mm) with 30x optical zoom and 16x digital zoom, and a 1.4x digital extender, this PTZ camera enables you to zoom in on activity in the monitoring area for a closer look.

나. 규격

• Image Sensor	1/2.3" Type MOS

• Lens	Motorized 30x zoom, f/1.6 to 4.7 (F=4.3 to 129mm, 35mm equivalent: 31.6 to 962mm)

• Focus Distance	Entire zooming range: 3.9' / 120 cm Wide end: 4" / 10 cm

• Compression	JPEG (M-JPEG)/H.264

• Image Resolution	VGA (640 x 480) (16:9 Letterbox: 640 x 320), QVGA: (320 x 240) (16:9                    Letterbox: 320 x 180)

• Output Format

- 1080p: 29.97/25

- 1080i: 59.94/50

- 1080PsF: 29.97/25

- 720p: 59.94/50

• Synchronization System	Internal

• During Full Auto

- 59.94: 1/30 to 1/2000

- 50: 1/25 to 1/2000

• During Auto

- 59.94: 1/60 to 1/2000

- 50: 1/50 1/2000

• Manual

- 59.94: 1/100, 1/250, 1/500, 1/1000, 1/2000, 1/4000, 1/10000

- 50: 1/120, 1/250, 1/500, 1/1000, 1/2000, 1/4000, 1/10000

• Synchro Scan Shutter

- 59.94: 59.94 Hz to 660.09 Hz (255 steps)

- 50: 50.00 Hz to 570.12 Hz (255 steps)

• Pan/Tilt Speed	Maximum 90°/sec

• Pan Range	± 175°

• Tilt Range	-30 to 90°

• Input/Output Connectors

- LAN: 1 x RJ-45

- Hd-SDI: 1 x BNC 75 Ω Compliant with the SMPTE292M standards RS232C: 1 x Mini DIN               8-pin (in)/1 x Mini DIN 8-pin (out)

- RS422: 1 x RJ-45 (control in RS422A)

- USB: 1 x Mini B-port (for maintenance)

- SD Card: ` x microSD card slot (for maintenance)

※. 옵션

• 전용 브라켓 2EA 포함

❍ 카메라 컨트롤러

가. 기능

원격 카메라(pan-tilt 헤드로 통합된 카메라)와 pan-tilt 헤드 시스템(pan-tilt 헤드와 pan-tilt 헤드가 장착된 카메라)을 콘트롤하도록 설계된 기기이다.

나. 규격

•  Remote Control

- Protocol - IPv4, RS-422 (Panasonic AW series protocol)

- Connection - Serial: Up to 5 cameras / IP: Up to 100 cameras (Up to 100 when Serial and IP           are used together)

- Adjustment functions - Pan/Tilt, Zoom, Focus, Iris, Gain, Pedestal, Shutter, Detail,White                Balance (Auto, R/B Gain), Black Balance (Auto, R/B Pedestal), Switch scene files

- Preset memory - Up to 100

• Switcher Control

- Connection - IP: 1

- Switcher Supported - AW-HS50N

- Linkage - Camera information display, TALLY information imported, BUS material selection            (AUX/PVW/PinP/KEY-F), Parameter changes (Pan/Tilt lever, Zoom button)

• Interface

- TALLY/GPI - TALLY input x 5 channels, GPI INPUT x 4 channels, GPI OUTPUT x 4                   channels, D-sub 15 pin (female x 1)

- LAN - 10BASE-T/100BASE-TX (for IP control), RJ45 x 1

- Pan/Tilt head - RS422 (for Serial control), RJ45 x 5

❍ Moving Spot Light

가. 기능

빛의 움직임, 크기, 밝기, 포커스 및 다양한 색, 고보(gobo) 등을 컴퓨터에 의해 조절할 수 있는 조명기이다.

나. 규격

•  50000Hr life span and low power consumption

•  Gobo Wheel : 1 rotation gobo wheel 6 rotatable/1Static gobo wheel with 8 gobos plus open

•  Color Wheel : 1 Color wheel with 7 colors plus open

•  DMX Channel : 14/16/18/ DMX Channel USITT DMX-512(vector mode 18ch)

•  PAN/Tilt : 540/630/360/Pan and 270/180/90 Tilt movement, 8/16 bit mmoth and precise                  resolution for PAN/Tilt movement

•  Zoom : Smooth linear motorized zoom ranging from 11-23 degree

❍ Controller

가. 기능

Moving light controller, with microcomputer as core, in adoption of new technology,

has more powerful and humanized functions.

나. 규격

•  DMX512 Total Channels 512

•  MAX Intelligent Fixtures 60

•  MAX Playback Programs 240

•  MAX Preset Focus 20

•  MAX Groups 20

•  Scene-snapshots 40

•  Shape-Generator YES

•  LCD Display Screen YES (Chinese/English)

•  Synchronous Trigger Mode Auto1, Auto2, Music

•  Library Format R20 Format

•  USB Port YES

•  Music Control Signal Input Line level input / MIC input

2). 스튜디오 영상 음향시스템

❍ ENG HD Hand-Held Camera System

가. 기능

The camcorder features a single Exmor RS sensor with a UHD 4K (3840 x 2160) resolution, Sony G lens with 12x optical zoom range, and 18/24x Clear Image Zoom in 4K/HD. It can record 4K in XAVC Long at 4:2:0 8-bit, and HD in XAVC Long at 4:2:2 10-bit, as well as MPEG2HD at 4:2:2 or 4:2:0 in 8-bit only. The integrated zoom lens features individual lens control rings for focus, iris, and zoom, and produces smooth-rounded-out-of-focus highlights.

나. 규격

• Image Sensor : 1-Chip 1" CMOS Sensor

• ISensor Resolution	: 20.00 MP

• IEffective Sensor Resolution : 14.2 MP

• IGain : -3 to 33 dB

• IMinimum Illumination : 1.7 lux

• IWhite Balance Range : 2300 to 15,000K

• Focal Length : 9.3 to 111.6mm

• 35mm Equivalent Focal Length : 29 to 348mm

• Optical Zoom Ratio : 12x

• Max Digital Zoom : 48x

• Maximum Aperture : f/2.8 to 4.5

• Filter Size : 62 mm

• Image Stabilization	Optical

• Focus Control : Autofocus, Manual Focus

• Shutter Speed : 1/6 to 1/10,000 sec

• Built-In ND Filter	Mechanical Filter Wheel with 2 Stop (1/4), 4 Stop (1/16), 6 Stop (1/64) ND

Filters

• Built-In Microphone Type	Stereo

• Recording Media

- 1 x SDXC/Memory Stick PRO Duo Hybrid Card Slot

- 1 x SDXC Card Slot

• Variable Frame Rates : 1080i: 120 fps, 1080i: 100 fps, 1080i: 1 to 60 fps, 1080i: 1 to 50 fps,

• Audio Recording	2-Channel 24-Bit 48 kHz

• Video Connectors	1 x RCA (Composite) Output, 1 x HDMI Output, 1 x BNC (3G-SDI) Output

• Audio Connectors	1 x Stereo 2RCA Output, 1 x 1/8" (3.5 mm) Stereo Headphone Output, 2 x 3-Pin XLR Mic/Line Level (+48 V Phantom Power) Input

• Wireless Interfaces : 2.4 GHz Wi-Fi

• Screen Size ; 3.5"

• Screen Resolution	: 1,560,000 Dots

• EVF

- Screen Size	.39"

- EVF Resolution	1,440,000 Dots

나. 옵션

• Battery Pack :  1EA 포함

• AC Adapter : 1EA 포함

• Remote :	1EA 포함

• SD Card 128G : 1EA 포함

• Wireless Mic. : 1EA 포함

• Soft Case	: 1EA 포함

❍ Camera Tripod

가. 기능

This patented Bridging Technology allows for a wider top plate and longer sliding plate that add stability and balance to a set of state-of-the-art professional features. A newly designed counterbalance system includes four presets--from 0 to 16.5 lbs--enabling proper balance for camera loads up to 19.8 lbs, while 3/8" threads in the top plate allow attachment of monitors, arms, and other accessories directly to the head.

나. 규격

• Load Capacity : 16.5 lbs (7.5kg)

• Maximum Height : 66.7" (169.4cm)

• Minimum Height :	17.9" (45.5cm)

• Folded Length : 33.3" (84.6cm)

• Head

- Counter Balance System	4-Step

- Quick Release/Wedge Plate	Yes

- Balance Plate	Sliding, 1/4" and 3/8" Screws

- Tilt Drag : Continuous

- Tilt Range : -60° / +90°

- Tilt Lock : Independent

- Spring Loaded Counter Balance : Continuous

- Pan Range : 360°

- Pan Lock : Independent

• Legs

- Material : Aluminum

- Head Attachment Fitting : 75mm Bowl

- Leg Stages/Sections : 2/3

- Leg Lock Type : Flip Levers

- Independent Leg Spread : Yes

- Spiked/Retractable Feet : Yes, w/rubber covers

- Center Brace : Mid-level Spreader

❍ Dolly

가. 기능

This Cine/Video Dolly is designed for use with tripods with spiked feet. The 5" wheels with independent brakes, cable guards, and unique leg locking system make this dolly very stable. It's also foldable for transport. Doorway clearance needed for the fully assembled dolly is only 44.1".

나. 규격

• Construction : Aluminum

• Doorway Width : 44.1" / 112 cm

• Load Capacity : 132 lb / 60 kg

• Folded Length : 25.5" / 64.7 cm

• Wheel Diameter : 5.0" / 12.7 cm

• Wheel Lock : Yes

• Cable Guards : Yes

❍ Studio Monitor Speaker

가. 기능

This is a two-way powered monitor designed for use in personal music production systems. Each unit features a built-in 20 watt amplifier that drives both the 4" woofer and the 7/8" tweeter.

나. 규격

• Low Frequency Driver : 4"

• Mid Frequency Driver : No

• High Frequency Driver : 7/8"

• Crossover	: 4kHz

• LF Amplifier : 20 watts for both drivers

• HF Amplifier : See above

• Frequency Range : 65Hz to 22kHz

• Impedance : Not applicable

• Maximum Sound Pressure Level (SPL) : 98dB @ 1 meter

• Maximum Power Handling	Not applicable (already powered)

• Controls and Indicators

- 2 x Front panel volume controls

- Front panel high and low tone controls

- Power On LED

- Rear mounted Power ON/OFF switch

• Connectors : 1 x XLR, 1 x 1/4" TRS balanced, 1 x RCA coaxial unbalanced

• Shielded : Yes

• Specialties : Seperate volume controls for both Line 1 and Line 2 inputs

❍ Studio Announcer Monitor

가. 기능

This TV has a 49.5" LED-backlit LCD display, and incorporates Motion Rate 60 technology to digitally enhance fast-moving images to reduce blur.

나. 규격

• Screen Size (Diagonal) : 50“

• SAspect Ratio : 16:9

• SPixel Resolution : 1920 x 1080

• Primary Connectivity Location : Display

• Input Ports

- 2 x HDMI – Audio, Video

- 1 x RCA Component/Composite Combo – Video

- 1 x RCA Stereo (L/R) – Video

• USB Ports	1 x USB (Version Unspecified) – Audio, Photo, Video

• Wi-Fi : Built-In

• Remote Control : Yes

• Wall Mounting : 200 x 200mm

❍ 이동형 랙

가. 기능

Able to hold TVs in sizes 32 to 70" in size and up to 125 pounds in weight, the Height-Adjustable Rolling TV Stand is useful in offices, trade shows, presentation areas, schools, and other locations that require moveable A/V equipment.

나. 규격

• 구분 : TV 브라켓

• 설치형태 : 이동식

• VESA : 100x100 ~ 600x400 mm

• 특징 : 10단계 높낮이 조절 (1280 ~ 1780 mm)

• 재질 : 냉간 압연 강판 (SPCC)

• 적용모델 : (LCD,LED) 32~60 인치, (PDP) 42~58 인치  / 45.5kg 이하

Control Room Systems

❍ Video Switcher

• Video Processing : 4:4:4 (YPbPr), 10-bit

- Connectors : Input  2 x HDMI type A

• Output

- Program: 1 x HDMI type A

- Preview: 1 x HDMI type A

• Input Formats	Video

- 1920 x 1080p: 59.94/50

- 1920 x 1080i: 59.94/50

- 1280 x 720p: 59.94/50

- 576i/p: 50

- 480i/p: 59.94

• Computer (60 Hz)

- WUXGA (1920 x 1200)

- UXGA (1600 x 1200)

- SXGA+ (1400 x 1050)

- SXGA (1280 x 1024)

- FWXGA (1366 x 768)

- WXGA (1280 x 800)

- XGA (1024 x 768)

- SVGA (800 x 600)

- VGA (640 x 480)

• Output Formats	Video

- 1920 x 1080p: 59.94/50

- 1920 x 1080i: 59.94/50

- 1280 x 720p: 59.94/50

- 576p: 50

- 480p: 59.94

• Audio Processing	Sampling Rate: 24-bit, 48 kHz

• Audio Formats	Linear PCM, 24-bit, 48 kHz, 2-ch

• Input

- 2 x HDMI type A (shared with video)

- 1 x 3.5 mm stereo mini

• Output

- Program: 1 x HDMI type A (shared with video)

- Preview: 1 x HDMI type A (shared with video)

- 1 x 3.5 mm stereo mini

• Input Level - -10 dBu (+8 dBu max)

• Output Level - Phones: 92 mW + 92 mW (32 Ohms)

• Input Impedance - 45 kOhms

• Output Impedance - Phones: 10 Ohms

• Interface	USB Memory: USB Type-B (for backup from PC)

- CTL/EXP: 1/4" TRS phone type

❍ LED Display

• 면종류 : LED TV

• 화면크기 : 32형

• 해상도 : 풀HD 1920 x 1080

• 응답속도 : 1ms

• 스캔방식 : 60Hz

• MHL연결 : 화면공유 Only

• USB재생 : ○

• 유선랜 : ○

• DLNA : ○

• HDMI : HDMI(2개)

• USB : USB(1개)

❍ SSD Reader/Writer

• Video Input : 6G-SDI: 1 x BNC

• Video Output : 6G-SDI: 2 x BNC, HDMI: 1 x HDMI (type A)

• Audio Input : None (embedded audio only 16 channel)

• Audio Output : None (embedded audio only 16 channels SDI, 8 channels HDMI)

• Device Control : 1 x RS-422 deck control port on DB9 female

• Ethernet : 1 x RJ-45 for remote operation

• Computer Interface : 1 x USB-C connector for software updates and HyperDeck Utility                        software control

• Media Interface :  x SD slots for SD, HD and UHD recording

- Media Type: UHS II and able to support ProRes 4444 playback and 422 recording

• Supported Resolutions

- 4K 3840 x 2160p: 30/29.97/25/24/23.98

• HD

- 1920 x 1080p: 60/59.94/50/30/29.97/25/24/23.98

- 1920 x 1080i: 60/59.94/50

- 1280 x 720p: 60/59.94/50

• SDI Compliance : SMPTE 259M/292M/296M/425M

• SDI Metadata Support : HD RP188 and closed captioning

• Video Sampling : 4:4:4:4

• Color Depth : 10-bit

• Color Space : REC 601, REC 709

• Audio Sampling : Television standard 48 kHz, 24-bit

• Supported Codecs

- Apple ProRes 422 HQ QuickTime

- ProRes 422 QuickTime

- ProRes 422 LT QuickTime

- ProRes 422 Proxy QuickTime

다. 옵션

• SDXC 128G 2EA 포함

❍ Audio Mixer

가. 기능

Acompact 6-input mixer and USB interface with built-in DSP for sound-reinforcement and recording of small performances, podcasts, lectures and similar applications. Capable of recording and playback of high-resolution 24-bit/192 kHz sound, this mixer features two XLR/1/4" combo mic/line inputs, as well as stereo 1/4" and RCA line inputs with level control, and a Hi-Z switch for direct recording of guitar and bass.

나. 규격

• Phantom Power : +48 V

• Input Channels : Mono [MIC/LINE]: 2 including HEADSET MIC (Plug-in Power) Stereo [LINE]: 2, Aux: 1

• Output Channels	Stereo Out: 1, Monitor Out: 1, Phones: 2 including headset phones

• Bus : Stereo: 1

• Pad : 26 dB

• Meter Peak Indication : LED turns on when the signal reaches 3 dB below clipping level

• DSP : CH1: COMP / EQ, EFFECT (SPX Reverb), CH2: AMP SIM, EFFECT (SPX Reverb)

• Level Metering : USB Output Level; 2 x 2 point LED meter [PEAK, SIG]

• USB Audio : 2 in / 2 out, USB Audio Class 2.0 compliant Sampling Frequency: Max 192 kHz, Bit Depth: 24-bit

• Power Requirements : DC 5 V, 500 mA

• Power Consumption : Max. 2.5 W

❍ Power Distributor

가. 기능

순차적으로 전원이 공급되며 역순으로 8 번부터 2 번까지 전원이 차단되는 기기

나. 규격

• AC Voltage meter : line input /output AC Voltage meter 를 내장하여 전압표시

• 채널수 : 8 채널

• 채널당 로딩 수 : 220V/10A,2200W

• 채널당 소비전력 : 10~15W

• Output connector : 한국표준 three wire AC connector

• 연속작동 사이의 시간간격 : 1 초

• 링크 : 가능

• 링크시 사용하는 케이블 : 4P DIN CABLE

• 파워스위치 , 램프 스위치 , 채널 on / off switch, Bypass 버튼

• 리모트 콘트롤러 SPRC 을 사용하여 원거리에서 콘트롤 가능 (20m 이내 )

• 램프 전압 : AC12V/400mA

• FAN 전압 : DC24V/1.5A( 상시전원 )

• 전압 : 220V / 50Hz-60Hz, 표준 3-wire 어쓰된 wire

❍ On-Air ON/OFF Display

가. 기능

A warning light that can be used in the studio and outdoors.

나. 규격

• 색상 : 고휘도 적색 LED type

• 제어 전류 :  10mA이내

• 전원 : 220 Volts, AC 60Hz, 2W

• 크기 : 270(W) × 78(H) × 60(D)mm

❍ Console Desk

가. 기능

The modular, configurable design enables you to customize the Monitoring & Command Desk to fit your needs

나. 규격

• Side Plate : Steel, Wood / Standard : 블랙,  아이보리 – 현장에 상황을 고려해 제작

이미지 촬영시스템

❍ DSLR Camera

• Camera Format : Full-Frame (1.0x Crop Factor)

• Pixels : Actual: 27.1 Megapixel

• Effective: 26.2 Megapixel

• Max Resolution : 26 MP6240 x 4160

• Aspect Ratio : 1:1, 3:2, 4:3, 16:9

• Sensor Type / Size : CMOS, 35.9 x 24 mm

• File Formats : Still Images: JPEG, RAW

• Movies: MJPEG, MOV, MP4,

• Audio: AAC

• Bit Depth	14-Bit

• Dust Reduction System : Yes

• Memory Card Type : SDXC, SDHC, SD

• Image Stabilization	Digital, 5-Way

• Focus Type :  Auto & Manual Focus

• Focus Mode : Automatic (A), Continuous-Servo AF (C), Manual Focus (M), Single-servo AF (S)

• Autofocus Points : Phase Detection: 45 (45 Cross-Type)

• Viewfinder Type : Optical

• Viewfinder Eye Point : 21.00 mm

• Viewfinder Coverage : 98%

• Viewfinder Magnification : Approx. 0.71x

• Diopter Adjustment : -3 to +1 m

• Display Screen : 3"  Swivel Touchscreen LCD (1,040,000)

• Diagonal Angle of View : 170.0°

• ISO Sensitivity : Auto, 100 to 40000 (Extended Mode:50 to 102400)

• Shutter : Type: Mechanical, Speed: 30 to 1/4000 Second , Bulb Mode

• Video Recording : Yes, NTSC/PAL

• Video Format

- 1920 x 1080p at 23.98/25/29.97/50/59.94 fps

- 1280 x 720p at 23.98/25/29.97/50/59.94 fps

• Aspect Ratio : 16:9

• Focus : Auto, Manual, Continuous Auto

• Max Video Clip Length : 1920 x 1080: 29 Minutes, 59 Seconds

• Audio Recording

- Built-In Mic: With Video (Stereo)

- Optional External Mic: With Video (Stereo)

다. 옵션

• Lens : 16-35mm — 1EA 포함

• UV Filter : 82mm — 1EA 포함

• SDHC Memory Card : SDXC 128G — 2EA 포함

• Battery : LP-E6N — 2EA 포함

• 카메라 가방 : 3355 — 1EA 포함

❍ 샷건마이크

가. 기능

It is used on video camcorders, DSLR cameras, or field recorders to capture audio.

나. 규격

• Transducer : Electret Condenser

• Polar Pattern : Cardioid, Supercardioid

• Frequency Range : 150 Hz to 18 kHz

• Signal to Noise Ratio : 40 dB

• Maximum SPL : 100 dB SPL

• Impedance : Cardioid: 760 Ohms

• Supercardioid : 1.7 kOhms

• Sensitivity	Cardioid : -43 dB

• Supercardioid : -33 dB

❍ Tripod

가. 기능

The Fluid Drag Video Head with Tripod and Carry Bag features a fluid head with a wide platform to support the HDSLR form factor, and a 60mm half ball for quick leveling without adjusting the legs.

나. 규격

• Fluid Head

- Load Capacity	11 lb (5 kg)

- Material	Aluminum alloy

- Head Attachment Fitting	60 mm half ball

- Counter Balance System	Spring-loaded

- Counter Balance Range	Pre-set to 5.3 lb (2.4 kg)

- Quick Release/Wedge Plate	Yes – 500PLONG

- Tilt Drag	Fluid cartridge with fixed drag

- Pan Drag	Fixed

- Pan Range	360°

- Tilt Range	-70°/+90°

• Tripod Legs

- Head Attachment Fitting	75 mm bowl

- Note: The included 60 to 75 mm adapter is required to use the head on the tripod

- Material of Construction	Aluminum

- Stages	2

- Leg Lock Type	Flip

- Independent Leg Spread	No

- Feet	Rubber

- Spiked / Retractable Feet	No

- Load Capacity	33 lb (15 kg)

- Minimum Height	22.4" (56.9 cm)

- Maximum Height	56.5" (143.5 cm)

- Closed Length	24.2" (61.5 cm)

• Fluid Head & Tripod

- Load Capacity	11 lb (5 kg)

- Minimum Height	26.6" (67.6 cm)

- Maximum Height	60.6" (153.9 cm)

- Closed Length	28.4" (72.1 cm)

❍ 스트로보

가. 기능

본 기기는 세밀한 광량 조절을 지원하고 테이터를 눈으로 바로 확인할 수 있도록 아날로그와 디지털을 조합시킨 스트로브 라이트 이다.

나. 규격

• Intervals in f-shop	1/10 f-stops

• Recycle time : 0.1 ~ 1.0sec

• Color temp	5,500k(±150k)

• Ready Charge	LED Light / Buzzer(Sound ON)

• Power display	Digital

• Model lamp	Halogen 250W (E11 base, screw typed)

• Model lamp control	Volume controller (VR), MODEL (ON/OFF)

• Flash trigger	Infrared photo cell, synchro cord, manual ready button

• Synchro, voltage	DC 8V

• Over temperature warning	Display(E0) on the FND

• Over Charge warning	Red LED

• Model	ON / OFF

• Slave (Infrared Sensor )	ON / OFF

• Sound	ON / OFF

• Ready	ON / OFF

• Cooling system	DC Cooling Fan

❍ 소프트박스

가. 기능

인상/정물/패션사진 등 어떠한 촬영시에도 뛰어난 조명 효과를 나타내며, 휴대가 간편할 뿐만 아니라 기존 제품의 어려운 조립방식을 개선하여 매우 쉽고 편리하게 조립할 수 있도록 제작되었다.

나. 규격

• 소프트박스 : 1개 (80x100)

• 디퓨져 : 2개 (겉천,속천)

• 프레임(폴대) : 4개

• 소프트박스 가방 : 1개

❍ A Stand

가. 기능

3단 구성의 압축 다이케스트 알루미늄 중형스탠드로 삼각대 부분이 견고하여 안정적으로 지탱시켜 주며 스프링 방식으로 되어있어 조명이 설치된 상태에서도 스탠드 조절이 안정적이다.

나. 규격

• 직경 : 아래부터 32/ 28/ 25mm

• 다리직경 : 22mm

• 접었을 때 : 970mm

• 최소높이 : 1000mm

• 최대높이 : 2520mm

❍ Boom Stand

가. 기능

조명 위치를 안정적으로 원하는 위치에 세팅할 수 있는 스탠드로 주로 탑라이트 촬영시 사용됩니다.

나. 규격

• 붐대 길이 : 228cm

• 스탠드 최대높이 : 170cm

• 추 무게 : 4.5kg

❍ 무선동조기

가. 기능

2.4GHz의 안정된 신호를 사용하는 16채널의 모선 동조기이다.

나. 규격

• 송신기 / 수신기 전원 :  AAA 배터리 X 2 - 1.5V (3A)

• 송신 주파수 : 2.4GHz

• 동조 거리 : 100m

• 동조 속도 : 최대 1/250s

• 채널수 : 16개 설정 가능

• 인증 : KC 인증

• 송신기 크기 : 85 x 36 x 34mm / 40g

• 수신기 크기 : 85 x 37 x 37mm / 40g

❍ 전동 롤배경지

가. 기능

강력한 벽면 고정형 3롤 훅을 이용하여 설치하며 인물, 상업, 제품, 비디오 등에서 매끄럽고 균일한 배경을 만들기 위한 전동 컨트롤 배경지이다.

나. 규격

• 벽면 3롤 후크 (2개 1조)

• 전동 익스판 3set

• 3M 연장 케이블 3ea

• 매직 수퍼 클램프 3set

• 6채널 무선 리모트 컨트롤러 RMS6 1set

• 알루코어 2.8M : 3set

• 카운터 웨이트 2.8M : 3set

3). 스튜디오 특수조명

❍ No. 1~4 Light Power Rail

가. 기능

조명기구의 전원공급 장치로서 조명기구 PLUG의 사양에 맞게 내부배선 및 CONSENT가

전기적, 기계적으로 견고 하고 안전하게 부착되어야 하며, 수리 및 점검이 용이하게 부착하여

Light에 연결이 쉽게 되도록 한다.

나. 규격

• BODY : ALUMINIUM or STEEL

• CONSENT : A TYPE 매입형

• 내부배선: HIV 4.0SQ 이상 회로용량에 맞게 배선하며 회로는 COLOR로 구분

• DIMENSION : 제작사양

❍ LED Flux Light

가. 기능

This approximately 35% more light output than its predecessor while maintaining its same form factor, appearance, low power draw, and compatibility with all existing Caster Series power and mounting accessories.

나. 규격

• Color Temp : 3200K~5600K

• Power Consumption : 150W

• Brightness @1m : *w/ 2T Acryl Diffuser : 3,935 Lux @ 5600K

• 3,775 Lux @ 3200K

• Beam Angle : 120˚

• Input Power : 100~240VAC, 50/60Hz

• Dimming :100%~0%

• Hi Output Soft LED Panel

• Ra 98~95 High CRI Color Property

• 3200K~5600K Variable Color Temperature

• 100%~0% Dimmable Brightness

• LED Numeric Display for Easy Operation

• Integrated DMX Interface

• 2 Way Slide-In Accessory Slots

• Soft Dimming and Kelvin Change by Software Tuning

❍ LED Spot Light

가. 기능

This approximately 35% more light output than its predecessor while maintaining its same form factor, appearance, low power draw, and compatibility with all existing Caster Series power and mounting accessories.

나. 규격

• Power : AC 100 ~ 240V 50~60Hz 0r DC 54V , 5A

• Power Consumption : 100 W cnds

• Light Source : COB 1PCS　PHLIPS LED

• CRI : >95

• Lumen Out put : >27,500Lumen

• Color Temperature : 5600K

• Lens Degree : 15o  ~ 45o

• Control Protocol : DMX512 /Master/slave / Wireless Remote Control APP Wifi 2.4G

• Refresh Frequency : 40,000 Hz

• Cooling Method : Efficient heat pipe technology, natural cooling, No Fan , No Noise

• Size : 565 x 390 x 450 이하

• Weight : 18.01Kg 이하(contains adapter)

• Material  : Aluminum & Steel

• Built-In 2.4G remote control receiver,Working with Wifi-2.4G control box, Can both control by the APP of mobile phone and 2.4G remote controller.

다. 옵션

• Barndoor --- 2EA 포함

❍ Light Hanger

가. 기능

LIGHT를 BATTEN에 설치할 수 있도록 하는 부속

나. 규격

• 장착 및 취급이 간편하고 기계적, 물리적으로 견고하도록 재료를 선정

• 특히, 기구의 흔들림에 의하여 BATTEN으로부터 이탈되지 않는 구조이어야 한다.

• BODY : 프레스 및 압출가공  TYPE

• 재질 : AL 및 스틸(제작사양에 따라 상이)

• 도장 : 흑색 및 기타 색상

❍ Safety Chain

가. 기능

LIGHT를 BATTEN에 설치한 후 라이트의 추락을 방지하기 위하여 라이트와 바텐을 연결하여주는 안전고리

나. 규격

• 재질 : STEEL WIRE ∅ 2  L=700

❍ Roll Cromakey Screen

가. 기능

상,하로 이동되는 크로마키용 영사막으로 불필요시 상부의 박스로 감아 두어 공간활용을 극대화 시키고 작동시 소음이나 잡음을 최소화 하여야 한다.

나. 규격

• 크로마키 작업을 위해 사용한다.

• 색상 : 그린

• 크기 : 3000 x 5000mm

• 동력 : DC 270W ~ 370W

• 속도 : 제작사양

• 케이스 : 알루미늄

❍ RD Unit Panel

• 주간선 M.C.C.B MAGNET S/W 및 기타 전기장치 등으로 구성된다.

• 제작사양에 따라 전기적으로 안전하게 제작되어야 하며 시설 관리자가 동작 상태를 쉽게 볼 수

있는 곳에 설치한 CONTROL 부분과 연결하여 사용한다.

• 외함은 옥내 자립형으로 제작되며, 각부의 주요 취부틀에 대해서는 STEEL PLATE 1.2T이상을

사용하고 측면 및 문은 1.2T이상의 강판을 사용한다.

• PANEL 전면에 DOOR를 설치하여, 설치 후 점검 및 보수가 용이 하도록 개폐할 수 있도록

제작한다.

• PANEL의 모든 입, 출입 배선은 현장여건에 따라 상부 및 하부로 통하여 결선 되도록 제작한다.

• 외 함  : 지정색상이 없을 경우 베이지 혹은 회색

• DIMENSION : 제작사양

❍ Light Control Board

가. 기능

DMX-512 시그날로 조명기구를 콘트롤하는 제어용 저장 장치

나. 규격

• 메모리 방식을 채택하여 초보자도 쉽고 편하게 운용할 수 있다.

• DMX OUT 포트가 4개 구성되어있다.

• Voltage：AC110V~240V 50/60Hz±10％

• Voltage: AC 100-240V,50/60Hz.

• Performance characterisitic: 2048 dmx channels,4 optical isolative DMX output ports.

B. 1층

❍ Info 데스크 Display

• 화면크기 : 178cm(70인치)

• 해상도 : 3840x2160 울트라HD

• 밝기 : 350cd

• 스캔방식 : 60Hz

• 응답속도 : 8ms

• 명암비 : 2000:1

• HDR10 : ○

• 시스템 출력 : 2.0ch스피커(20W)

• 미라캐스트 : ○

• HDMI : HDMI (3개)

• USB : USB

❍ 엘리베이터 사이니지

가. 기능

음성서비스, 동영상 구현 등 이용자에게 효율적인 정보를 제공하는 무인 종합정보안내시스템 KIOSK 세로형으로 멀티미디어 기술을 이용하는 키오스크는 개방된 장소에서 무인으로 운영되면서 이용자들이 정보 획득, 물품구매, 발권, 등록 등의 처리를 쉽게 할 수 있도록 설계됩니다.

나. 구성

1. 벽걸이형 DID

2. STB(사이니지 SW 포함)

다. 규격

1. 벽걸이형 DID

• 실내용 사이니지

• LED / 139cm(55인치)

• 풀HD

• IPS패널

• 밝기: 300cd /

• 화면비 : 16:9

• 비디오 입력 : HDMI / D-SUB

2. STB

• CPU : QUad core 3.2 GHZ

• Ram : 32Gb

• OS : Android 7.0

❍ 북카페용 Display

• 화면크기 : 178cm(70인치)

• 해상도 : 3840x2160 울트라HD

• 밝기 : 350cd

• 스캔방식 : 60Hz

• 응답속도 : 8ms

• 명암비 : 2000:1

• HDR10 : ○

• 시스템 출력 : 2.0ch스피커(20W)

• 미라캐스트 : ○

• HDMI : HDMI (3개)

• USB : USB

❍ 무선 마이크

1. 수신기

• Modulation : Wideband FM

• Frequency Range	A: 548 to 572 MHz

• Switching Bandwidth : Up to 24 MHz

• Signal to Noise Ratio : ≥ 103 dBA

• Total Harmonic Distortion : ≤ 0.9%

• Temperature Range : Operation: 32 to 104°F (0 to +40°C)

• Storage : -4 to 158°F (-20 to 70°C)

• Transmitter Synchronization : 2.4 GHz, Low Power OQPSK (only active during synchronization)

• Principle	Double superheterodyne

• Diversity	Antenna switching diversity via internal antennas

• Sensitivity	< 3 μV at 52 dBA RMS S/N (at peak deviation)

• Frequency Response ; 50 Hz to 16 kHz (-3 dB)

• Max Output Voltage : At Peak Deviation, 1 kHz AF 1/4" (6.3 mm)

• Jack Socket (unbalanced): +6 dBu XLR Socket (balanced): +12 dBu

• Adjustment Range	Audio: 45 dB, adjustable in 5-dB steps

• Power Supply

- Nominal Input Voltage: 100 to 240 VAC

- Nominal Output Voltage: 12 VDC/300 mA

• Line/Mic Level	20 dB, switchable

2. Microphone

• Output Power : 10 mW

• Frequency Response : 80 Hz to 14 kHz

• Power Supply: 2 x AA batteries, 1.5 V

• Operating Time	Approximately 10 hrs.

• Microphone Type : Dynamic

• Polar Pattern : Cardioid

• Input Sensitivity	Capsule: 1.5 mV/Pa

• Adjustment Range; Transmitter Sensitivity: 0 to -30 dB, adjustable in 10 dB steps

❍ Audio Mixer

• Phantom Power	+48 V switchable, channels 1 - 12

• Digital I/O

- USB Audio Class 2.0 compliant

- Sampling Frequency: max 192 kHz

- Bit Depth: 24-bit

• Input Channels

- 8x mono [mic/line]

- 2x mono/stereo [mic/line]

- 2x stereo [line]

• Output Channels

- 2x stereo out

- 1x monitor out

- 1x headphone out

- 4x aux out

- 4x group out

• Bus

- Stereo: 1

- AUX: 4

- GROUP: 4

• HPF	80 Hz, 12 dB/oct (mono/stereo: MIC only)

• Compressor

- Threshold: +22 dBu to -8 dBu

- Ratio: 1:1 to 4:1

- Output level: 0 dB to 7 dB

- Attack time: approx. 25 msec

- Release time: approx. 300 msec

• Equalizer	EQ high gain: +15 dB/-15 dB, frequency: 10 kHz shelving

- EQ mid gain: +15 dB/-15 dB, frequency: mono 250 Hz - 5 kHz peaking, stereo 2.5 kHz                peaking

- EQ low gain: +15 dB/-15 dB, frequency: 100 Hz shelving

• Frequency Response	+0.5 dB/-1.5 dB (20 Hz to 48 kHz), refer to the nominal output level@ 1 kHz, GAIN knob: Min

• Residual Output Noise	-102 dBu (STEREO OUT, STEREO master fader: min

❍ 스피커

• Active or Passive : Passive

• Frequency Response : 80Hz - 20kHz (-10dB), 100Hz - 18kHz (±3dB)

• Power Capacity : 150W

• Maximum Sound Pressure Level (SPL) : 110dB (40W @ 0.5 m)

• Nominal Sensitivity : 108dB, Continuous

• Impedance : 4 Ohms

• Crossover : 4.2kHz

• Low Frequency Driver : 5.25" (135mm) Low Frequency Loudspeaker

• High Frequency Driver : 0.75" (19mm) Polycarbonate Dome Tweeter

• Enclosure Material : Polypropylene Structural Foam

• Input Connections : Spring Speaker Terminals

• Environmental : Indoor

❍ Power Amp

• AC Line Voltage and Frequency Configurations Available	(+/- 10%) 100VAC 50/60 Hz, 110VAC 60 Hz, 220 and 230~240VAC 50 Hz

• Voltage Gain	35

• Sensitivity	1.4V (for full rated power at 4 ohms)

• Signal to Noise Ratio	(ref. rated power, 8 ohms, 1 kHz) > 103 dB

• THD : <0.5%

• Damping Factor :	(8 ohms, 10 Hz to 400 Hz) >200

• Intermodulation Distortion	(from full rated output to -30 dB) <0.3%

• Frequency Response (at 1W, 20 Hz - 20 kHz)	0 dB

• Crosstalk	>85 dB (below rated 8 ohms power, at 1 kHz); >55 dB (below rated 8 ohms power, at 20 kHz)

• Input Impedance (nominal)	20 kilohms balanced, 10 kilohms unbalanced

• Load Impedance	2~8 ohms per channel in Stereo; 4~8 ohms in Bridge

❍ Power Distributor

• AC Voltage meter : line input /output AC Voltage meter 를 내장하여 전압표시

• 채널수 : 8 채널

• 채널당 로딩 수 : 220V/10A,2200W

• 채널당 소비전력 : 10~15W

• Output connector : 한국표준 three wire AC connector

• 연속작동 사이의 시간간격 : 1 초

• 링크 : 가능

• 링크시 사용하는 케이블 : 4P DIN CABLE

• 파워스위치 , 램프 스위치 , 채널 on / off switch, Bypass 버튼

• 리모트 콘트롤러 SPRC 을 사용하여 원거리에서 콘트롤 가능 (20m 이내 )

• 램프 전압 : AC12V/400mA

• FAN 전압 : DC24V/1.5A( 상시전원 )

• 전압 : 220V / 50Hz-60Hz, 표준 3-wire 어쓰된 wire

❍ 장비 랙

• 전면부 : 강화유리

• 측면판넬 : 착탈식

• 후면부 : 스틸도어

• 유닛(Unit) : 15U

• 고정타입 : 케이즈너트 타입

• 선반 : 1개

• 냉각팬 : 2개

• 크기 : 750 x 1000 x 600 (HxDxW)

❍ Media Wall

가. 규격

1. LED 미디어 월

1.1 정보 표출부 특성

• LED 미디어 월은 여타 소자에 비해 수명이 매우 길며, 장시간 사용하여도 밝기 및 색상의              변화가 적고, 소모전력이 적어 유지에 매우 경제적인 LED 소자를 사용하여야 한다.

• LED 미디어 월의 표출부는 현장여건에 가장 적합한 가시각도를 보유한 LED 소자를 적용하여          관람자가 미디어 월 표출내용을 충분히 인식할 수 있도록 제작하여야 한다.

• LED 미디어 월의 표출화면 색상은 부드럽고 깨끗하여야 한다.

• 본 LED 미디어 월은 문자, 그래픽, 동영상이 미디어 월에 표출 되어야 한다.

1.2 정보 표출부 세부사양

• 구조물 전체크기 : (W)13,540mm x (H)2,980mm x (D)150mm

• 영상 표시면 크기 : (W)13,440 x (H)2,880mm

• 화면비(가로 : 세로) : 약 14 : 3

• LED MAKER: NATIONSTAR 社 (광각 실내용)

• 표출 색상 :FULL COLOR

• 모듈수량(영상표시부) : (W)70 x (H)15 = 1,050 MODULES

• 영상부 해상도 : (W)4,480 x (H)960 = 4,300,800 Pixels

• 휘도(WHITE 시) : 1,200nit (cd/㎡) 미만

• 색온도 : 6,500°K or 사용자 지정

• 영상부 화소간격(PIXEL PITCH) : 3mm

• 가시각도 : Hor. 120(±60°), Ver. 120(±60°) 이상

• R.G.B LED 배열 : PIXELRED(1), PURE GREEN(1), BLUE(1) 균등배열

• RED : 625㎚ Typ.

• PURE GREEN : 525㎚ Typ.

• BLUE : 470㎚ Typ.

• MODULE 구성 : (W)64 x (H)64 Pixel Matrix Panel / (Hood분리형) Type

• MODULE SIZE : (W)192 x (H)192 mm

• 소비전력(MODULE)/1MODULE 당 : Max. 28W

• LED 수명 :50,000시간 이상

2. 컨트롤 시스템

2.1 운영 컴퓨터

운영체제는 Microsoft Windows 8 version 이상 이어야 하며, 미디어 월 운영 software를 실행하는        데 문제가 없는 성능 이상이어야 한다.

2.2. 운영 Software

• 미디어 월 운영자가 손쉽게 사용이 가능하도록 대화형 메뉴선정 방식으로 설계된 운영                 Program으로 미디어 월 System 운영에 가장 적절하도록 설계하여야 한다.

• 그래픽 환경 : Mouse 및 Keyboard를 이용하여 간편히 운영할 수 있도록 디자인 된 화면으로            하여야 한다.

• 메뉴선택 방식 : 상위메뉴에서 하위메뉴를 선택하여 운영이 가능하여야 하며, 쉽고 신속하게            정보입력 및 변경이 가능하도록 하여야 한다.

• 편집기능 : 미디어 월에 표출하고자 하는 문자나 숫자, 동영상를 Program을 사용하여 입력한 후         변환 Program을 사용하여 미디어 월에 표출하기 알맞는 형태로 저장

• 전송기능 : 문자 표출장비를 사용하여 편집된 화면을 미디어 월 제어용 Computer로 전송하여           미디어 월에 표출하는 기능

• 보관기능 : 문자 작업이 완료된 Data를 미디어 월 제어용 Computer에 저장하는 기능.

• 확인기능 : 저장된 문자를 운영자가 간단한 조작으로 호출하여 Computer의 Monitor를 통하여           확인하는 기능.

3. 비디오 프로세서

3.1 용도

페이드 인/아웃 기능을 가지는 16개의 스위칭 효과를 제공하는  Full Color LED  비디오 프로세서

3.2 세부 사양

• Support high resolution

• Seamless mosaic/switching

• Fade/hot backup, text overlay/input resolution lock

• Advanced interlaces the moving pictures adaptive processing technology, to eliminate the video         image motion trailing and serrated phenomenon, for ordinary PAL/NTSC video, output image           clearer is exquisite, the 1080 I signals for high definition, the output of the image detail is            rich, full color, the image quality is in a leading level

• Advanced image zoom technology, support kinds of output resolution, and single supports              horizontal 2560 points, vertical 1536 points, and according to the size of the LED screen to            display input image point by point scale

• Intelligent large size seamless splicing technology, the unique frame synchronization with               dynamic technology, guaranteed that the moving picture is fluent, no displacement and delay           phenomenon

• Complete Video input interface, including 2 x VGA, 1 x DVI, 1 x HDMI, 2 x Video ,1*DP,              support the HD signal input, and a variety of audio and Video equipment can be                      interconnected

• Support external expansion input module, optional  DVI, HDMI, SDI module

• Hot backup

• Support  seamless switching between the  different signal source

• Support double picture function (PIP/POP)

• DVI input signal loop out , 2 DVI output, 1  VGA monitor output, VGA anti-shaking  function

DVI enhance function

• The graphic overlying function

• Fade in fade out/cut/ slide picture

• Multi-machine connecting function

• 2 sending cards can be built-in

• Template function

• Lock input resolution(for point to point output solution)

• Dual channel image crop

• With more convenient operation interface

• Test pattern(include 72 test patterns)

• With two button (Take/Effect) make signal switching more easy

4. 프레임 및 배관 배선

4.1. 마감

• 패널의 조립시공에 사용되는 모든 자재는 취급에 주의하여 파손 또는 표면 흠집이 생기지              않도록 주의해야 한다.

• 패널 조립시공에 사용되는 조립자재가 외부에 노출되어 사용하는 경우 부식에 강한 재질을             선택하여 시공한다.

• 사용자재는 방청을 위하여 아연 도금한 것을 사용하거나 또는 방청페인트를 칠한다.

• 칼라쉬트 철판으로 제작된 조립자제의 끝 부분은 반드시 절곡  가공하여 사용한다.

• 풍하중에 따른 적정 허용 SPAN을 결정하여 보조 프레임을 설치한다.

4.2. 외관

• 철판의 산화막을 완전히 제거하고 정전분체도장을 하여야 하며 표면이 미려하게 도장하여야            한다.

• 눈, 비 등으로부터 보호하기 위한 방수구조로 하여야 한다.

• 모든 사용자재에 부식방지 및 방수 처리를 하여야 한다.

• 내부의 열을 방출할 수 있도록 통풍구 및 FAN을 설치하여야 하며, 가동 및 정지 시 환기구를           통해 비, 물기, 먼지, 벌레, 이물질 등이 유입되지 않는 구조로 제작되어야 한다.

• 전광판의 외함에는 추후 유지보수 및 안전점검을 위하여 출입문(개구부)을 설치하여야 하며,            출입문에는 시건장치를 하여 외부인의 접근으로부터 보호하여야 한다.

4.3. 배관 배선 및 표시

• 배선은 전기설비기술기준, 내선규정 등을 준수하여 설계도면 및 규격시방서에 의거하여 작업           되어야 한다.

• 배선은 충분한 용량의 절연특성이 우수한 전선을 사용하여 기기간의 동작에 영향을 주지 않도록         규격에 맞는 우수품질을 가진 제품으로 제작되어야 한다.

• 전광판 내부의 배선은 접촉에 의한 사고를 예방할 수 있도록 덕트를 이용하여 최대한 은폐시켜         결선하여 외관상 미려하도록 하고 노출로부터의 사고를 방지하여야 한다.

• 케이블 분기 또는 접속은 분전반, 또는 접속함 안에서 하도록 설계 제작되어야 한다.

• 배선의 분기는 반드시 단자대에서 처리하고 단자접속 시 단선, 접촉 불량, 합선 등이 생기지            않도록 하여야 한다.

• 배선의 단말에는 적합한 터미널을 사용하여야 하며, 점검이 용이하도록 마크밴드 또는 튜브를          사용하여 점검이 용이하도록 조립되어야 한다.

• 단자대에는 투명한 합성수지판으로 된 탈착이 용이한 구조의 덮개를 덮도록 하여 안전에 대비할         수 있도록 하여야 한다.

• 각 단자대에는 번호 또는 기호를 기입하여 배선의 구분이 용이하도록 하여야 하며 A/S시 신속히         대처할 수 있도록 하여야 한다.

C. 2층

1). 경영기획실

❍ LCD Display

• 화면크기 : 163cm(65인치)

• 해상도 : 3840x2160 울트라HD

• 밝기 : 320cd

• 스캔방식 : 60Hz

• 응답속도 : 8ms

• HDR10 : ○

• 시스템 출력 : 2.0ch스피커(20W)

• 미라캐스트 : ○

• HDMI : HDMI (3개)

• USB : USB

• 디지털음성 : ○

• 헤드폰출력 : ○

• 컴포넌트 : ○

• HDMI 2.0 지원 : ○

❍ 벽걸이 브라켓

가. 기능

대형TV를 벽에 고정하여 다양한 디스플레이가 가능한 제품

나. 규격

•   Vesa : 200x100 / 200x200 / 400x200 / 400x400

•   적용인치 : 32~65“

•   최대 적용 하중 : 45kg

•   벽과의 거리 : 30mm

2). 소회의실

❍ LCD Display

• 화면크기 : 163cm(65인치)

• 해상도 : 3840x2160 울트라HD

• 밝기 : 320cd

• 스캔방식 : 60Hz

• 응답속도 : 8ms

• HDR10 : ○

• 시스템 출력 : 2.0ch스피커(20W)

• 미라캐스트 : ○

• HDMI : HDMI (3개)

• USB : USB

• 디지털음성 : ○

• 헤드폰출력 : ○

• 컴포넌트 : ○

• HDMI 2.0 지원 : ○

❍ 벽걸이 브라켓

가. 기능

대형TV를 벽에 고정하여 다양한 디스플레이가 가능한 제품

나. 규격

•   Vesa : 200x100 / 200x200 / 400x200 / 400x400

•   적용인치 : 32~65“

•   최대 적용 하중 : 45kg

•   벽과의 거리 : 30mm

❍ 월 패널

가. 기능

디스플레이와 소스장비의 연결을 쉽게 하기 위한 단자 연장 패널

나. 규격

•   재질 : 알루미늄

•   모듈 : HDMI

3). 중회의실-16인

❍ LCD Display

• 화면크기 : 178cm(70인치)

• 해상도 : 3840x2160 울트라HD

• 밝기 : 350cd

• 스캔방식 : 60Hz

• 응답속도 : 8ms

• 명암비 : 2000:1

• HDR10 : ○

• 시스템 출력 : 2.0ch스피커(20W)

• 미라캐스트 : ○

• HDMI : HDMI (3개)

• USB : USB

• 디지털음성 : ○

• 헤드폰출력 : ○

• 컴포넌트 : ○

• HDMI 2.0 지원 : ○

❍ 벽걸이 브라켓

가. 기능

대형TV를 벽에 고정하여 다양한 디스플레이가 가능한 제품

나. 규격

•   Vesa : 600x400mm

•   적용인치 : 32~70“

•   최대 적용 하중 : 50kg

•   벽과의 거리 : 50mm

❍ 월 패널

가. 기능

디스플레이와 소스장비의 연결을 쉽게 하기 위한 단자 연장 패널

나. 규격

•   재질 : 알루미늄

•   모듈 : HDMI

D. 3층

1). 회의실-8인

❍ LCD Display

• 화면크기 : 178cm(70인치)

• 해상도 : 3840x2160 울트라HD

• 밝기 : 350cd

• 스캔방식 : 60Hz

• 응답속도 : 8ms

• 명암비 : 2000:1

• HDR10 : ○

• 시스템 출력 : 2.0ch스피커(20W)

• 미라캐스트 : ○

• HDMI : HDMI (3개)

• USB : USB

• 디지털음성 : ○

• 헤드폰출력 : ○

• 컴포넌트 : ○

• HDMI 2.0 지원 : ○

❍ 벽걸이 브라켓

가. 기능

대형TV를 벽에 고정하여 다양한 디스플레이가 가능한 제품

나. 규격

•   Vesa : 600x400mm

•   적용인치 : 32~70“

•   최대 적용 하중 : 50kg

•   벽과의 거리 : 50mm

❍ 월 패널

가. 기능

디스플레이와 소스장비의 연결을 쉽게 하기 위한 단자 연장 패널

나. 규격

•   재질 : 알루미늄

•   모듈 : HDMI

2). 출입구

❍ LCD Display

• 화면크기 : 55인치

• 해상도 : 3840x2160 울트라HD

• 밝기 : 300cd

• 스캔방식 : 60Hz

• 응답속도 : 6.5ms

• 명암비 : 1000만:1

• HDR10 : ○

• 시스템 출력 : 2.0ch스피커(20W)

• 미라캐스트 : ○

• HDMI : HDMI (3개)

• USB : USB

• 디지털음성 : ○

• 헤드폰출력 : ○

• 컴포넌트 : ○

• HDMI 2.0 지원 : ○

E. 4층

1). 회의실-8인

❍ LCD Display

• 화면크기 : 178cm(70인치)

• 해상도 : 3840x2160 울트라HD

• 밝기 : 350cd

• 스캔방식 : 60Hz

• 응답속도 : 8ms

• 명암비 : 2000:1

• HDR10 : ○

• 시스템 출력 : 2.0ch스피커(20W)

• 미라캐스트 : ○

• HDMI : HDMI (3개)

• USB : USB

• 디지털음성 : ○

• 헤드폰출력 : ○

• 컴포넌트 : ○

• HDMI 2.0 지원 : ○

❍ 벽걸이 브라켓

가. 기능

대형TV를 벽에 고정하여 다양한 디스플레이가 가능한 제품

나. 규격

•   Vesa : 600x400mm

•   적용인치 : 32~70“

•   최대 적용 하중 : 50kg

•   벽과의 거리 : 50mm

❍ 월 패널

가. 기능

디스플레이와 소스장비의 연결을 쉽게 하기 위한 단자 연장 패널

나. 규격

•   재질 : 알루미늄

•   모듈 : HDMI

2). 출입구

❍ LCD Display

• 화면크기 : 55인치

• 해상도 : 3840x2160 울트라HD

• 밝기 : 300cd

• 스캔방식 : 60Hz

• 응답속도 : 6.5ms

• 명암비 : 1000만:1

• HDR10 : ○

• 시스템 출력 : 2.0ch스피커(20W)

• 미라캐스트 : ○

• HDMI : HDMI (3개)

• USB : USB

• 디지털음성 : ○

• 헤드폰출력 : ○

• 컴포넌트 : ○

• HDMI 2.0 지원 : ○

F. 5층

1). 회의실-28인

❍ Projector

• Image Display

- Display System : 3-Chip 0.76" LCD

- Native Chip Resolution : 1920 x 1200 (WUXGA)

- Max Brightness	: 5500 Lumens

- Aspect Ratio : Native: 16:10

- Dynamic Contrast Ratio : 3,000,000:1

• Inputs/Outputs

- 2 x HDMI (HDMI Type-A) Audio, Video Input

- 1 x HDBaseT (RJ45) Audio, Control, Video Input/Output

- 1 x 5BNC Video Input

- 1 x VGA (DE-15) Video Input

- 1 x VGA (DE-15) Video Output

- 1 x RCA Video Input

- 1 x 2RCA Audio Input

- 2 x 1/8" (3.5 mm) Mini Audio Input

- 1 x 1/8" (3.5 mm) Mini Audio Output

- 1 x USB 2.0 (USB Type-A) Power Output

- 1 x USB 2.0 (USB Type-A) LAN Input

- 1 x Ethernet (RJ45) LAN

- 1 x DE-9 Remote Input

- 1 x DE-9 Control Input

- 1 x 1/8" (3.5 mm) Mini Remote Input

• Wireless LAN / Wi-Fi :  No, Optional Adapter Available

❍ 프로젝터 리프트

가. 기능

가변 브라켓을 부착하여 프로젝터 장착후 각도 조정이 용이하며 모터와 케이스가 일체형으로 제작되어 시공이 용이하고 매립형으로 비사용시 프로젝터 오염과 훼손을 방지한다.

나. 규격

•   타공 : 730 x 700 x 400

•   모터 : 60Hz 220V IP44 19r/min

•   밑판 : 765 x740

•   하강 : 300mm

•   크기 : 720 x 670 x 350

❍ 전동스크린

가. 기능

천장에 설치하여 유선, 무선 리모트로 제어하는 전동 스크린이다.

나. 규격

•  White Matte(PU)

•  시야각 : 160

•  Gain : 1.0

•  Case : Aluminium

•  Type : 매립형

•  사이즈 : 120“

•  비율 : 4:3

•  친환경 소재 사용

다. 옵션 - Wall Panel -- 1EA 포함

•  사이즈 : 120 x 70 x 10mm

•  Material : Aluminium or Plastic

•  기능 : Up/Down

❍ 앰프

가. 기능

다양한 입출력 단자와 팬텀파워, 패드스위치, 멀티이펙터, 고급리버브, 그래픽EQ 시스템이 기본장착되어 있으며, 소규모 공간에서 별도의 모니터 앰프없이 모니터 환경을 구축할 수 있도록 Main Amp Assign 회로가 장착된 오디오 믹서 앰프이다.

나. 규격

•  8옴 스테레오 출력 : 2 x 250W

•  입력 : 마이크 x8ch, 라인 x8ch, 라인전체 x10ch

•  E/N : -110db

•  잔류노이즈(스피커출력잭) : -70db

•  잔류노이즈(메인출력잭) : -97db

•  신호대 잡음비 : >90db

•  4옴 스테레오출력 : 1kHz,>0.05%

•  메인출력 : 0dBm, 1kHz,>0.05%

•  혼변조 왜율 : 0.05%

•  채널 분리도(1kHz) : -60db

•  마이크 임피던스 : 4KΩ

•  Main, Mon, Aux 출력 : 10KΩ

•  Tape 출력 : 10KΩ

•  그래픽 이퀄라이져 : +/-12db, 5밴드 스테레오, 125Hz, 250Hz, 500Hz, 1kHz, 4kHz

❍ 스피커

가. 기능

This Speaker are a pair of compact professional loudspeakers offering high quality at an affordable price for professional or residential applications.

나. 규격

• Active or Passive : Passive

• Frequency Response : 80Hz - 20kHz (-10dB), 100Hz - 18kHz (±3dB)

• Power Capacity : 150W

• Maximum Sound Pressure Level (SPL) : 110dB (40W @ 0.5 m)

• Nominal Sensitivity : 108dB, Continuous

• Impedance : 4 Ohms

• Crossover : 4.2kHz

• Low Frequency Driver : 5.25" (135mm) Low Frequency Loudspeaker

• High Frequency Driver : 0.75" (19mm) Polycarbonate Dome Tweeter

• Enclosure Material : Polypropylene Structural Foam

• Input Connections : Spring Speaker Terminals

• Environmental : Indoor

❍ Power Distributor

가. 기능

순차적으로 전원이 공급되며 역순으로 8 번부터 2 번까지 전원이 차단되는 기기

나. 규격

• AC Voltage meter : line input /output AC Voltage meter 를 내장하여 전압표시

• 채널수 : 8 채널

• 채널당 로딩 수 : 220V/10A,2200W

• 채널당 소비전력 : 10~15W

• Output connector : 한국표준 three wire AC connector

• 연속작동 사이의 시간간격 : 1 초

• 링크 : 가능

• 링크시 사용하는 케이블 : 4P DIN CABLE

• 파워스위치 , 램프 스위치 , 채널 on / off switch, Bypass 버튼

• 리모트 콘트롤러 SPRC 을 사용하여 원거리에서 콘트롤 가능 (20m 이내 )

• 램프 전압 : AC12V/400mA

• FAN 전압 : DC24V/1.5A( 상시전원 )

• 전압 : 220V / 50Hz-60Hz, 표준 3-wire 어쓰된 wire

❍ 장비 랙

가. 기능

EQ Rack is a durable, fifteen-space rack unit that is designed with vented side panels in order to promote airflow throughout the rack.

나. 규격

• 전면부 : 강화유리

• 측면판넬 : 착탈식

• 후면부 : 스틸도어

• 유닛(Unit) : 15U

• 고정타입 : 케이즈너트 타입

• 선반 : 1개

• 냉각팬 : 2개

• 크기 : 750 x 1000 x 600 (HxDxW)

❍ LCD Display

• 화면크기 : 189cm(75인치)

• 해상도 : 3840x2160 울트라HD

• 크로마샘플링 4:4:4

• 디밍 기술 : UHD Dimming

• 응답속도 : 8ms

• HDR10 : ○

• 시스템 출력 : 2.0ch스피커(20W)

• 미라캐스트 : ○

• HDMI : HDMI (3개)

• USB : USB (2개)

• 디지털음성 : ○

• 헤드폰출력 : ○

• 컴포넌트 : ○

• HDMI 2.0 지원 : ○

❍ 벽걸이 브라켓

가. 기능

대형TV를 벽에 고정하여 다양한 디스플레이가 가능한 제품

나. 규격

•   Vesa : 200x200, 300x300, 400x200, 400x400, 600x400mm

•   적용인치 : 32~75“

•   최대 적용 하중 : 50kg

•   벽과의 거리 : 64mm~510mm

•   홀패턴 Universal

다. 옵션

•   HDMI Wall Panel 1EA 포함

C. Conference System

❍ 메인컨트롤러

가. 기능

본 기기는 회의용 마이크 시스템 컨트롤러로써 소,중,대규모의 회의 진행시 참석자들의 마이크

사용을 통제하여 발언자의 의사를 효율적으로 참석자에게 전달함으로써 보다 현장감있고

원활한 회의 진행을 위한 시스템이다.

나. 규격

• Frequency Band : 2.4 GHz ISM Band

• Frequency Stability : ± 20 ppm

• Modulation : GFSK

• RF Data Rate : 1 Mbps

• RF Impedance : 50 Ω

• Rx Sensitivity : - 87 dB (BER＜ 0.1%)

• SNR : 79 dB (A–Weighted)

• THD : 0.1 %

• Sampling Rate : 24 KHz Mono

• Audio Output Impedance : 600 Ω, Balanced

• Output Audio Range : –15 ∼ –5dB

• Audio Input Impedance : 600 Ω, Balanced

• Input Audio Range : –20 ∼ –5dB

• Color : Black

• Power Requirements : DC 5V, 1A (SMPS)

• Operating Temp : - 10 ∼ +50℃

❍ 구즈넥마이크(의장용)

가. 기능

본 마이크는 회의용 마이크 시스템의 의장용 마이크로써 메인 컨트롤러에 연결하여 사용 하며 발언시 유니트 부분의 램프가 점등되어 발언자를 쉽게 확인 할 수 있으며 진행을 원활히 하는데 편리하게 사용 할 수 있다.

나. 규격

• Frequency Band:  2.4 GHz ISM Band

• Frequency Stability : ± 20 ppm

• Modulation : GFSK

• RF Data Rate : 1 Mbps

• RF Impedance : 50 Ω

• Rx Sensitivity : - 87 dB (0.1% BER)

• SNR : 73 dB (A–Weighted)

• THD : 0.1 %

• Sampling Rate : 24 KHz Mono

• SPK Power : 0.5 W

• Color : Dark gray, Silver

• Power Requirements : DC 3.7 V (Polymer Lithium-Ion Battery Pack)

• Time :

- up to 20 hours (Talk Mode)

- Up to 12 hours (Stand – alone Mode)

• Operating Temp : - 10 ∼ +50℃

❍ 구즈넥마이크

가. 기능

본 마이크는 회의용 마이크 시스템의 의장용 마이크로써 메인 컨트롤러에 연결하여 사용 하며 발언시 유니트 부분의 램프가 점등되어 발언자를 쉽게 확인 할 수 있으며 진행을 원활히 하는데 편리하게 사용 할 수 있다.

나. 규격

• Frequency Band:  2.4 GHz ISM Band

• Frequency Stability : ± 20 ppm

• Modulation : GFSK

• RF Data Rate : 1 Mbps

• RF Impedance : 50 Ω

• Rx Sensitivity : - 87 dB (0.1% BER)

• SNR : 73 dB (A–Weighted)

• THD : 0.1 %

• Sampling Rate : 24 KHz Mono

• SPK Power : 0.5 W

• Color : Dark gray, Silver

• Power Requirements : DC 3.7 V (Polymer Lithium-Ion Battery Pack)

• Time :

- up to 20 hours (Talk Mode)

- Up to 12 hours (Stand – alone Mode)

• Operating Temp : - 10 ∼ +50℃

다. 옵션

• 배터리팩 : 12개

• 충전기 : 1개

• 안테나 : 1개

• 연결 케이블 : 20M